A B C D E F G H I J K L M N O P Q R S T U V W X Z

## L

L - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
last_sx - Variable in class com.rscja.team.qcom.utility.GyroAngle
last_sy - Variable in class com.rscja.team.qcom.utility.GyroAngle
last_sz - Variable in class com.rscja.team.qcom.utility.GyroAngle
last_time - Variable in class com.rscja.team.qcom.utility.GyroAngle
led() - Method in interface com.rscja.deviceapi.interfaces.IURAxOfAndroidUart
  成功的通知提示(指示灯闪烁)
  Success Notification Sound (flashing light)
led() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  成功的通知提示(指示灯闪烁)
  Success Notification Sound (flashing light)
led() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
  成功的通知提示(指示灯闪烁)
  Success Notification Sound (flashing light)
led() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
  成功的通知提示(指示灯闪烁)
  Success Notification Sound (flashing light)
led() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  成功的通知提示(指示灯闪烁)
  Success Notification Sound (flashing light)
led() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
  成功的通知提示(指示灯闪烁)
  Success Notification Sound (flashing light)
led() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
  成功的通知提示(指示灯闪烁)
  Success Notification Sound (flashing light)
LedLight - Class in com.rscja.deviceapi
  手柄LED灯控制类
  Handdeld LED control type
LedLight() - Constructor for class com.rscja.deviceapi.LedLight
LedLight_mtk - Class in com.rscja.team.mtk.deviceapi
  手柄LED灯控制类
  Handdeld LED control type
LedLight_mtk() - Constructor for class com.rscja.team.mtk.deviceapi.LedLight_mtk
LedLight_qcom - Class in com.rscja.team.qcom.deviceapi
  手柄LED灯控制类
  Handdeld LED control type
LedLight_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.LedLight_qcom
LedOff(String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
LedOff(String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
LedOn(String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
LedOn(String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
loadChar(Fingerprint.BufferEnum, int) - Method in class com.rscja.deviceapi.Fingerprint
  加载指定ID页到特征值缓存区
  Load specified ID page to feature value buffer zone
loadChar(int, FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  读取模块中的指纹并暂存在RamBuffer中
loadChar(Fingerprint.BufferEnum, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  加载指定ID页到特征值缓存区
  Load specified ID page to feature value buffer zone
loadChar(int, FingerprintWithZAZ.BufferEnum, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  读取模块中的指纹并暂存在RamBuffer中
loadChar(Fingerprint.BufferEnum, int) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  加载指定ID页到特征值缓存区
  Load specified ID page to feature value buffer zone
loadChar(int, FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  读取模块中的指纹并暂存在RamBuffer中
lockAFI() - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  锁定AFI(lock AFI)
lockAFI() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  锁定AFI
  lock AFI
lockAFI() - Method in class com.rscja.deviceapi.RFIDWithISO15693
  锁定AFI
  lock AFI
lockAFI() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
  锁定AFI
  lock AFI
lockAFI() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
  锁定AFI
  lock AFI
lockAFI() - Method in class com.rscja.team.qcom.r1.hf.HF15693
  锁定AFI(lock AFI)
LockBank_ACCESS - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定的区域ACCESS (ACCESS LOCK area)
LockBank_EPC - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定的区域EPC (EPC LOCK area)
LockBank_KILL - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定的区域KILL (KILL LOCK area)
LockBank_TID - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定的区域TID (TID LOCK area)
LockBank_USER - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定的区域USER (USER LOCK area)
lockDsfid() - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  锁定Dsfid(lock Dsfid)
lockDSFID() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  锁定DSFID
  lock DSFID
lockDSFID() - Method in class com.rscja.deviceapi.RFIDWithISO15693
  锁定DSFID
  lock DSFID
lockDSFID() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
  锁定DSFID
  lock DSFID
lockDSFID() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
  锁定DSFID
  lock DSFID
lockDsfid() - Method in class com.rscja.team.qcom.r1.hf.HF15693
  锁定Dsfid(lock Dsfid)
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.BleDevice
  锁定指定标签
  Lock specific tag
lockMem(String, String) - Method in class com.rscja.deviceapi.BleDevice
  锁定标签
  Lock tag
lockMem(String, int, int, int, String, String) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
lockMem(String, String) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
lockMem(String, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
lockMem(String, String, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
lockMem(String, int, int, int, String, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  锁定指定标签
  Lock specific tag
lockMem(String, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  锁定标签
  Lock tag
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  锁指定标签(Lock specified label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,bank,ptr,cnt,filterData,hexLockCode);
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  锁标签(lock label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,hexLockCode);
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  锁指定标签(Lock specified label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,bank,ptr,cnt,filterData,hexLockCode);
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  锁标签(lock label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,hexLockCode);
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  锁指定标签(Lock specified label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,bank,ptr,cnt,filterData,hexLockCode);
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  锁标签(lock label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,hexLockCode);
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  锁指定标签(Lock specified label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,bank,ptr,cnt,filterData,hexLockCode);
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  锁标签(lock label) 示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode); lockMem(accessPwd,hexLockCode);
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
lockMem(String, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  锁定指定标签
  Lock specific tag
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  锁定标签
  Lock tag
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
lockMem(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
lockMem(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
lockMem(String, String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
lockMem(String, String) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
lockMem(String, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  锁定指定标签
  Lock specific tag
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  锁定标签
  Lock tag
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
lockMem(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
lockMem(String, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
LockMode_LOCK - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定模式:锁定(LOCK mode: lock)
LockMode_OPEN - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定模式:开放(LOCK mode: Release)
LockMode_PLOCK - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定模式:永久锁定(LOCK mode: Permanent LOCK)
LockMode_POPEN - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  锁定模式:永久开放(LOCK mode: Permanent release)
logD(String) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
LogUtility_mtk - Class in com.rscja.team.mtk.utility
LogUtility_mtk() - Constructor for class com.rscja.team.mtk.utility.LogUtility_mtk
LogUtility_qcom - Class in com.rscja.team.qcom.utility
LogUtility_qcom() - Constructor for class com.rscja.team.qcom.utility.LogUtility_qcom
long2Bytes(long) - Static method in class com.rscja.utility.StringUtility
  long转byte数组
LowBatteryEntity - Class in com.rscja.deviceapi.entity
LowBatteryEntity() - Constructor for class com.rscja.deviceapi.entity.LowBatteryEntity
LowBatteryException - Exception in com.rscja.deviceapi.exception
LowBatteryException(String) - Constructor for exception com.rscja.deviceapi.exception.LowBatteryException

A B C D E F G H I J K L M N O P Q R S T U V W X Z