A B C D E F G H I J K L M N O P Q R S T U V W X Z

## M

M - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
M1_ReadData(int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Read data in specified block of specified sector, used for S50 and S70 tag.
M1_ReadData(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Read data in specified block of specified sector, used for S50 and S70 tag.
M1_ReadData(int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Read data in specified block of specified sector, used for S50 and S70 tag.
M1_ReadData(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Read data in specified block of specified sector, used for S50 and S70 tag.
M1_WriteData(int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  向指定的扇区的Block 写入数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Write data in specified sector of block, used for S50 and S70 tag.
M1_WriteData(int, int, String) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  向指定的扇区的Block 写入数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Write data in specified sector of block, used for S50 and S70 tag.
M1_WriteData(int, int, String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  向指定的扇区的Block 写入数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Write data in specified sector of block, used for S50 and S70 tag.
M1_WriteData(int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  向指定的扇区的Block 写入数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。
  Write data in specified sector of block, used for S50 and S70 tag.
M775Authenticate - Class in com.rscja.custom
  英频杰特殊标签定制
  Special label customization
  第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 盘点标签之前先要设置回调函数`M775Authenticate.setInventoryCallback(IUHFInventoryCallback)`,然后调用盘点函数`RFIDWithUHFUART.startInventoryTag()`开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。
  For parameter setting, after the connection is successful, call the corresponding function to set parameters and read/write operations.
M775Authenticate.AuthenticateInfo - Class in com.rscja.custom
  AuthenticateInfo对象实体(AuthenticateInfo object entity)
M775Authenticate.IUHFInventoryCallback - Interface in com.rscja.custom
  盘点回调函数（Inventory callback function）
M775Authenticate_mtk - Class in com.rscja.team.mtk.custom
M775Authenticate_qcom - Class in com.rscja.team.qcom.custom
makeSendData(int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
MANUFACTOR_CW - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
MANUFACTOR_HONYWELL - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
MANUFACTOR_IA - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
MANUFACTOR_IDATA - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
MANUFACTOR_MOBYDATA - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
MANUFACTOR_NEWLAND - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
MANUFACTOR_ZEBRA - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
match() - Method in class com.rscja.deviceapi.Fingerprint
  对比模板缓冲区1与模板缓冲区2的指纹模板文件
  fingerprint template file of comparison template buffer zone 1 and template buffer zone 2.
match(FingerprintWithZAZ.BufferEnum, FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  指定的两个 Ram Buffer 中的 Template 之间进行比对
match() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  对比模板缓冲区1与模板缓冲区2的指纹模板文件
  fingerprint template file of comparison template buffer zone 1 and template buffer zone 2.
match(FingerprintWithZAZ.BufferEnum, FingerprintWithZAZ.BufferEnum, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  指定的两个 Ram Buffer 中的 Template 之间进行比对
match() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  对比模板缓冲区1与模板缓冲区2的指纹模板文件
  fingerprint template file of comparison template buffer zone 1 and template buffer zone 2.
match(FingerprintWithZAZ.BufferEnum, FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  指定的两个 Ram Buffer 中的 Template 之间进行比对
MC50_4350_120 - Static variable in class com.rscja.CWDeviceInfo
MC50_4350_120 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
MC50_4350_12_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
MC51_4350_120 - Static variable in class com.rscja.CWDeviceInfo
merge(FingerprintWithZAZ.BufferEnum, int, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  合并模版
merge(FingerprintWithZAZ.BufferEnum, int, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  合并模版
merge(FingerprintWithZAZ.BufferEnum, int, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  合并模版
mesage(String) - Method in interface com.rscja.deviceapi.interfaces.IUpgradeProgress
message(Printer.PrinterStatus) - Method in interface com.rscja.deviceapi.Printer.PrinterStatusCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.EnrollCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.GRABCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.IdentificationCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.PtCaptureCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.TemplateVerifyCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.EnrollCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.GrabCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.IdentificationCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.PtCaptureCallBack
messageInfo(String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.TemplateVerifyCallBack
messageInfo(String) - Method in interface com.rscja.deviceapi.FingerprintWithTLK1NC.IUPImageCallback
messages - Variable in class com.rscja.team.qcom.http.NetResult_qcom
mFd - Variable in class com.rscja.team.mtk.deviceapi.DeviceAPI
mFd - Variable in class com.rscja.team.qcom.deviceapi.DeviceAPI
MobyDataBarcodeSymbol_qcom - Class in com.rscja.team.qcom.barcode.symbol
MODE_EPC - Static variable in class com.rscja.deviceapi.entity.InventoryModeEntity
MODE_EPC_RESERVED - Static variable in class com.rscja.deviceapi.entity.InventoryModeEntity
MODE_EPC_TID - Static variable in class com.rscja.deviceapi.entity.InventoryModeEntity
MODE_EPC_TID_USER - Static variable in class com.rscja.deviceapi.entity.InventoryModeEntity
MODE_LED_TAG - Static variable in class com.rscja.deviceapi.entity.InventoryModeEntity
MODE_TEMPERATURE_TAG - Static variable in class com.rscja.deviceapi.entity.InventoryModeEntity
MODEL_CW_CW9281 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_HONYWELL_3601 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_HONYWELL_3603 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_HONYWELL_6603 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_HONYWELL_EX30 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_HONYWELL_N5703 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_HONYWELL_N6703 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IA_100S - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IA_101S - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IA_166S - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IA_171S - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IA_181S - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IA_400S - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IA_417S - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_IDATA_DS7000 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_MOBYDATA_E3200 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_MOTO_5500 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_NEWLAND_CM30 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_NEWLAND_CM47 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_NEWLAND_CM60 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_ZEBRA_2100 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_ZEBRA_4100 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_ZEBRA_4710 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_ZEBRA_4720 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_ZEBRA_4750 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_ZEBRA_4770 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Model_ZEBRA_4850 - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
Module - Class in com.rscja.deviceapi
Module_mtk - Class in com.rscja.team.mtk.deviceapi
Module_qcom - Class in com.rscja.team.qcom.deviceapi
ModuleFree(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModuleFree(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModuleInit(String, String, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModuleInit(String, String, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModuleInitEX(String, String, int, int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModuleInitEX(String, String, int, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModulePowerOff(String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModulePowerOff(String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModulePowerOn(String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModulePowerOn(String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModuleReceive() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModuleReceive() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModuleReceiveEx(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModuleReceiveEx() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModuleSend(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModuleSend(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ModuleSendAndReceive(byte[], int, byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ModuleSendAndReceive(byte[], int, byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoCancel() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoCancel() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoCapture(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoCapture(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoCapturePKComp(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoCapturePKComp(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoDescriptor() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoDescriptor() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoEnroll(char, char[], char[], String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoEnroll(char, char[], char[], String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
morphoEraseAllBase() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  删除所有指纹信息
  delete all fingerprint infor
morphoEraseAllBase() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  删除所有指纹信息
  delete all fingerprint infor
MorphoEraseAllBase() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
morphoEraseAllBase() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  删除所有指纹信息
  delete all fingerprint infor
MorphoEraseAllBase() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
morphoEraseAllBase() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  删除所有指纹信息
  delete all fingerprint infor
MorphoFingerFree(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoFingerFree(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoFingerInit(String, String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoFingerInit(String, String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoFingerMessage() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoFingerMessage() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoGetSecurityLevel() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoGetSecurityLevel() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoGrab(char, String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoGrab(char, String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoIdentify(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoIdentify(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoLoadKs(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoLoadKs(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoPIDSN() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoPIDSN() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoSetSecurityLevel(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoSetSecurityLevel(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoStop() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoStop() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
MorphoVerifyPKComp(char, byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
MorphoVerifyPKComp(char, byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
mRFID - Variable in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
MTK - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk.Platform
MTK - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
MultipleTemperatureInfo() - Constructor for class com.rscja.custom.UHFTemperatureTagsAPI.MultipleTemperatureInfo
myLogDebug(String, String) - Static method in class com.rscja.team.mtk.utility.LogUtility_mtk
myLogDebug(String, String) - Static method in class com.rscja.team.qcom.utility.LogUtility_qcom
myLogErr(String, String) - Static method in class com.rscja.team.mtk.utility.LogUtility_mtk
myLogErr(String, String) - Static method in class com.rscja.team.qcom.utility.LogUtility_qcom
myLogInfo(String, String) - Static method in class com.rscja.team.mtk.utility.LogUtility_mtk
myLogInfo(String, String) - Static method in class com.rscja.team.qcom.utility.LogUtility_qcom
myLogV(String, String) - Static method in class com.rscja.team.mtk.utility.LogUtility_mtk
myLogV(String, String) - Static method in class com.rscja.team.qcom.utility.LogUtility_qcom

A B C D E F G H I J K L M N O P Q R S T U V W X Z