com.rscja.deviceapi.interfaces

## Interface ISingleAntenna

- All Known Subinterfaces:
    IRFIDWithUHFUSB, IUhfBle
  All Known Implementing Classes:
    EmptyUhfBle, M775Authenticate, M775Authenticate_mtk, M775Authenticate_qcom, RFIDWithUHFA4, RFIDWithUHFA4_qcom, RFIDWithUHFA8, RFIDWithUHFA8_qcom, RFIDWithUHFAxBase, RFIDWithUHFAxBase_qcom, RFIDWithUHFBLE, RFIDWithUHFBLE_qcom, RFIDWithUHFBLEN51_qcom, RFIDWithUHFBLEN52_qcom, RFIDWithUHFJieCe, RFIDWithUHFJieCe_qcom, RFIDWithUHFRLM, RFIDWithUHFRLM_qcom, RFIDWithUHFShuangYingDianZi_qcom, RFIDWithUHFUART, RFIDWithUHFUART_mtk, RFIDWithUHFUART_qcom, RFIDWithUHFUARTUAE_qcom, RFIDWithUHFUSB, RFIDWithUHFUSB_qcom, UHFCSYX, UHFCSYX_qcom, UHFTamperAPI, UHFTamperAPI_qcom, UHFTemperatureSensors, UHFTemperatureTag, UHFTemperatureTag.RFIDWithUHFBLEN51, UHFTemperatureTag.RFIDWithUHFBLEN52, UHFTemperatureTagsAPI, UHFTemperatureTagsAPI_mtk, UHFTemperatureTagsAPI_qcom, UHFTemperatureTagsBLEAPI, UHFUartFoxconn, UHFUartFoxconn_mtk, UHFUartFoxconn_qcom, UHFUartTemperatureTag, UHFXSAPI

      public interface ISingleAntenna

- - ### Method Summary

    All Methods Instance Methods Abstract Methods
    Modifier and Type | Method and Description
    --- | ---
    `int` | `getPower()` 读取模块的功率 Read module output power
    `boolean` | `setPower(int power)` 设置模块的功率 Setup output power

- - ### Method Detail

    - #### getPower

          int getPower()

      读取模块的功率
      Read module output power
      Returns:
        返回功率，返回-1为失败(Return output power, return -1 means failure.)

    - #### setPower

          boolean setPower(int power)

      设置模块的功率
      Setup output power
      Parameters:
        `power` - 功率值(Power values)
      Returns:
        true:成功(success) false:失败(failure)