## Uses of Interface
com.rscja.deviceapi.interfaces.IUHFInventoryCallback

- Packages that use IUHFInventoryCallback
  Package | Description
  --- | ---
  com.rscja.custom |
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.mtk.deviceapi |
  com.rscja.team.qcom.ble |
  com.rscja.team.qcom.deviceapi |
  com.rscja.team.qcom.socket |
  com.rscja.team.qcom.uhfparse |

- - ### Uses of IUHFInventoryCallback in com.rscja.custom

    Classes in com.rscja.custom that implement IUHFInventoryCallback
    Modifier and Type | Class and Description
    --- | ---
    `class` | `UHFXSAPI`

    Methods in com.rscja.custom with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | UHFXSAPI.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | UHFTemperatureSensors.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | UHFCSYX_A4NetWork.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`

  - ### Uses of IUHFInventoryCallback in com.rscja.deviceapi

    Methods in com.rscja.deviceapi with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | RFIDWithUHFA8NetWork.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 设置盘点回调接口，接收循环盘点到的标签数据 Set the inventory callback interface to receive the label data from the cyclic inventory 备注：需要在开始循环盘点`RFIDWithUHFA8NetWork.startInventoryTag()`之前调用此方法。 Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA8NetWork.startInventoryTag()`.
    `void` | RFIDWithUHFA8.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUSB.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUrxUart.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUrxUsbToUart.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | BleDevice.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 设置盘点回调接口，接收循环盘点到的标签数据 Set the inventory callback interface to receive the label data from the cyclic inventory 备注：需要在开始循环盘点`BleDevice.startInventoryTag()`之前调用此方法。 Note: This method needs to be called before starting the loop inventory `BleDevice.startInventoryTag()`.
    `void` | RFIDWithUHFUrxNetwork.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFA4.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFA4NetWork.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 设置盘点回调接口，接收循环盘点到的标签数据 Set the inventory callback interface to receive the label data from the cyclic inventory 备注：需要在开始循环盘点`RFIDWithUHFA4NetWork.startInventoryTag()`之前调用此方法。 Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA4NetWork.startInventoryTag()`.
    `void` | RFIDWithUHFBLE.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUART.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 设置盘点回调接口，接收循环盘点到的标签数据 Set the inventory callback interface to receive the label data from the cyclic inventory 备注：需要在开始循环盘点`RFIDWithUHFUART.startInventoryTag()`之前调用此方法。 Note: This method needs to be called before starting the loop inventory `RFIDWithUHFUART.startInventoryTag()`.
    `void` | RFIDWithUHFA4RS232.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 设置盘点回调接口，接收循环盘点到的标签数据 Set the inventory callback interface to receive the label data from the cyclic inventory 备注：需要在开始循环盘点`RFIDWithUHFA4RS232.startInventoryTag()`之前调用此方法。 Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA4RS232.startInventoryTag()`.
    `void` | RFIDWithUHFA8RS232.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 设置盘点回调接口，接收循环盘点到的标签数据 Set the inventory callback interface to receive the label data from the cyclic inventory 备注：需要在开始循环盘点`RFIDWithUHFA8RS232.startInventoryTag()`之前调用此方法。 Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA8RS232.startInventoryTag()`.

  - ### Uses of IUHFInventoryCallback in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | IUHFURAxExtend.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | IUHF.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 设置盘点回调接口，接收循环盘点到的标签数据 Set the inventory callback interface to receive the label data from the cyclic inventory 备注：需要在开始循环盘点`IUHF.startInventoryTag()`之前调用此方法。 Note: This method needs to be called before starting the loop inventory `IUHF.startInventoryTag()`.
    `void` | IBleDevice.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | IUHFUrxAutoInventoryTag.`start(IUHFInventoryCallback iuhfInventoryCallback)`

  - ### Uses of IUHFInventoryCallback in com.rscja.team.mtk.deviceapi

    Methods in com.rscja.team.mtk.deviceapi with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | RFIDWithUHFUART_mtk.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`

  - ### Uses of IUHFInventoryCallback in com.rscja.team.qcom.ble

    Methods in com.rscja.team.qcom.ble with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | RFIDWithUHFBLEN52_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFBLEN51_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | EmptyUhfBle.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`

  - ### Uses of IUHFInventoryCallback in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | RFIDWithUHFUSB_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUrxUsbToUart_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUrxUart_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUrxUart2_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUrxNetwork_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFUART_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | RFIDWithUHFBLE_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | BleDevice_qcom.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`
    `void` | UHFUrxNetWorkAutoInventoryTag_qcom.`start(IUHFInventoryCallback iuhfInventoryCallback)`

  - ### Uses of IUHFInventoryCallback in com.rscja.team.qcom.socket

    Methods in com.rscja.team.qcom.socket with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | SocketUdpClientUR4.`startReceiveUhfTagInfo(IUHFInventoryCallback iuhfInventoryCallback)`

  - ### Uses of IUHFInventoryCallback in com.rscja.team.qcom.uhfparse

    Methods in com.rscja.team.qcom.uhfparse with parameters of type IUHFInventoryCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | UHFProtocolProtocolParseBase.`setInventoryCallback(IUHFInventoryCallback inventoryCallback)`