com.rscja.deviceapi.interfaces

## Interface IRFIDWithISO14443B

- All Superinterfaces:
    IRFIDBase
  All Known Implementing Classes:
    RFIDWithISO14443B, RFIDWithISO14443B_mtk, RFIDWithISO14443B_qcom

      public interface IRFIDWithISO14443B
      extends IRFIDBase

- - ### Method Summary

    All Methods Instance Methods Abstract Methods
    Modifier and Type | Method and Description
    --- | ---
    `java.lang.String` | `getUID()` 获取卡片ID Acquire card ID
    `byte[]` | `getUIDBytes()` 获取卡片ID Acquire card ID
    `java.lang.String` | `reset()` CPU卡复位操作指令 CPU card reset operation commande
    `java.lang.String` | `sendCommand(java.lang.String cmd)` CPU卡 T=CL发送COS指令 CPU card T=CL send COS command

    - ### Methods inherited from interface com.rscja.deviceapi.interfaces.IRFIDBase

      `free, getVersion, init, init, isPowerOn, rfidUpgrade`

- - ### Method Detail

    - #### getUID

          java.lang.String getUID()

      获取卡片ID
      Acquire card ID
      Returns:
        失败返回null
        failure return null

    - #### getUIDBytes

          byte[] getUIDBytes()

      获取卡片ID
      Acquire card ID
      Returns:
        失败返回null
        failure return null

    - #### sendCommand

          java.lang.String sendCommand(java.lang.String cmd)

      CPU卡 T=CL发送COS指令
      CPU card T=CL send COS command
      Parameters:
        `cmd` - COS指令内容
        COS command content
      Returns:
        CPU卡返回的COS指令内容
        CPU card return COS command

    - #### reset

          java.lang.String reset()

      CPU卡复位操作指令
      CPU card reset operation commande
      Returns:
        CPU卡返回的reset操作数据
        CPU card return reset operation data