## Uses of Class
com.rscja.team.qcom.uhfhandler.UHFDataHandleBase.CMDInfo

- Packages that use UHFDataHandleBase.CMDInfo
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.qcom.deviceapi |
  com.rscja.team.qcom.socket |
  com.rscja.team.qcom.uhfhandler |
  com.rscja.team.qcom.usb |

- - ### Uses of UHFDataHandleBase.CMDInfo in com.rscja.deviceapi

    Methods in com.rscja.deviceapi with parameters of type UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `static java.util.ArrayList<UHFTAGInfo>` | UHFProtocolParseBase.`parseReadTagDataEPC_TID_USER(UHFDataHandleBase.CMDInfo data, TagInfoRule tagInfoRule)`

  - ### Uses of UHFDataHandleBase.CMDInfo in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces that return UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `UHFDataHandleBase.CMDInfo` | IBluetoothData.`getTagCmd()`
    `UHFDataHandleBase.CMDInfo` | IBluetoothData.`sendAndReceive(byte[] sendData, int timeOut)`

  - ### Uses of UHFDataHandleBase.CMDInfo in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi with parameters of type UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `UHFTAGInfo` | UHFProtocolParseByJava.`parseContinuousInventoryTagData(UHFDataHandleBase.CMDInfo inData, TagInfoRule tagInfoRule)`
    `java.util.ArrayList<UHFTAGInfo>` | UHFProtocolParseUSBByJava_qcom.`parseReadTagDataEPC_TID_USER(UHFDataHandleBase.CMDInfo inData)`
    `java.util.List<UHFTAGInfo>` | UHFProtocolParseByJava.`parseReadTagDataEPC_TID_USER(UHFDataHandleBase.CMDInfo inData, TagInfoRule tagInfoRule)`

  - ### Uses of UHFDataHandleBase.CMDInfo in com.rscja.team.qcom.socket

    Methods in com.rscja.team.qcom.socket that return UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `UHFDataHandleBase.CMDInfo` | SocketManageUR4.`getTagInfo()`
    `UHFDataHandleBase.CMDInfo` | SocketManageA4.`receiveGPIOData()`
    `UHFDataHandleBase.CMDInfo` | SocketManageA4.`receiveTagData()`
    `UHFDataHandleBase.CMDInfo` | SocketManageUR4.`sendAndReceive(byte[] senddata)`
    `UHFDataHandleBase.CMDInfo` | SocketManageA4.`sendAndReceive(byte[] sendData)`
    `UHFDataHandleBase.CMDInfo` | SocketManageUR4.`sendAndReceive(byte[] senddata, int timeOut)`
    `UHFDataHandleBase.CMDInfo` | SocketManageA4.`sendAndReceive(byte[] sendData, int controlWord)`
    `UHFDataHandleBase.CMDInfo` | SocketManageA4.`sendAndReceive(byte[] sendData, int controlWord, int timeOut)`

  - ### Uses of UHFDataHandleBase.CMDInfo in com.rscja.team.qcom.uhfhandler

    Methods in com.rscja.team.qcom.uhfhandler that return UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `UHFDataHandleBase.CMDInfo` | UHFUrAxDataHandle.`getGPIOCmd()`
    `UHFDataHandleBase.CMDInfo` | UHFDataHandleBase.`getLastBarcodeCmd(int cmd, int controlWord, int timeOut)`
    `UHFDataHandleBase.CMDInfo` | UHFDataHandleBase.`getLastCmd(int cmd, int timeOut)`
    `UHFDataHandleBase.CMDInfo` | UHFDataHandleBase.`getLastCmd(int cmd, int controlWord, int timeOut)`
    `UHFDataHandleBase.CMDInfo` | UHFDataHandleBase.`getTagCmd()`

    Methods in com.rscja.team.qcom.uhfhandler that return types with arguments of type UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `java.util.List<UHFDataHandleBase.CMDInfo>` | UHFDataHandleBase.`getCmdList(int cmd)`
    `java.util.List<UHFDataHandleBase.CMDInfo>` | UHFDataHandleBase.`getCmdList(int cmd, int controlWord)`

    Methods in com.rscja.team.qcom.uhfhandler with parameters of type UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `void` | UHFUrAxDataHandle.`addCmdList(UHFDataHandleBase.CMDInfo info)`
    `void` | UHFUR4DataHandle.`addCmdList(UHFDataHandleBase.CMDInfo info)`
    `void` | UHFRxUsbDataHandle.`addCmdList(UHFDataHandleBase.CMDInfo info)`
    `void` | UHFRxBLEDataHandle.`addCmdList(UHFDataHandleBase.CMDInfo info)`
    `abstract void` | UHFDataHandleBase.`addCmdList(UHFDataHandleBase.CMDInfo info)`
    `void` | HFR1UsbDataHandle.`addCmdList(UHFDataHandleBase.CMDInfo info)`
    `boolean` | UHFUrAxDataHandle.`isBuildFullData(UHFDataHandleBase.CMDInfo cmdInfo)`
    `boolean` | UHFUR4DataHandle.`isBuildFullData(UHFDataHandleBase.CMDInfo cmdInfo)`
    `boolean` | UHFRxUsbDataHandle.`isBuildFullData(UHFDataHandleBase.CMDInfo cmdinfo)`
    `boolean` | UHFRxBLEDataHandle.`isBuildFullData(UHFDataHandleBase.CMDInfo cmdinfo)`
    `abstract boolean` | UHFDataHandleBase.`isBuildFullData(UHFDataHandleBase.CMDInfo cmdinfo)`
    `boolean` | HFR1UsbDataHandle.`isBuildFullData(UHFDataHandleBase.CMDInfo cmdinfo)`

  - ### Uses of UHFDataHandleBase.CMDInfo in com.rscja.team.qcom.usb

    Methods in com.rscja.team.qcom.usb that return UHFDataHandleBase.CMDInfo
    Modifier and Type | Method and Description
    --- | ---
    `UHFDataHandleBase.CMDInfo` | UrxUsb_qcom.`getUHFTAGInfo()`
    `UHFDataHandleBase.CMDInfo` | UrxUsb_qcom.`sendAndReceive(byte[] bytes)`
    `UHFDataHandleBase.CMDInfo` | RxUsb_qcom.`sendAndReceive(byte[] bytes, boolean clean)`
    `UHFDataHandleBase.CMDInfo` | RxUsb_qcom.`sendAndReceive(byte[] bytes, boolean clean, int timeOut)`
    `UHFDataHandleBase.CMDInfo` | UrxUsb_qcom.`sendAndReceive(byte[] bytes, int timeOut)`