com.rscja.deviceapi.interfaces

## Interface ConnectionStatusCallback<T>

- All Known Implementing Classes:
    RFIDWithUHFBLEN51_qcom, RFIDWithUHFBLEN52_qcom, UHFTemperatureTag.RFIDWithUHFBLEN51, UHFTemperatureTag.RFIDWithUHFBLEN52

      public interface ConnectionStatusCallback<T>

- - ### Method Summary

    All Methods Instance Methods Abstract Methods
    Modifier and Type | Method and Description
    --- | ---
    `void` | `getStatus(ConnectionStatus status, T device)`

- - ### Method Detail

    - #### getStatus

          void getStatus(ConnectionStatus status,
                         T device)

      Parameters:
        `status` - 状态(status)
        `device` - 目标设备(device)