A B C D E F G H I J K L M N O P Q R S T U V W X Z

## P

P00 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P01 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P02 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P03 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P04 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P05 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P06 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P08 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P09 - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P0A - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P0B - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P0H - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P0X - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
P80_8786_130 - Static variable in class com.rscja.CWDeviceInfo
P80_8786_130 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
P80_8786_130_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
P80_8953 - Static variable in class com.rscja.CWDeviceInfo
P80_8953 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
P80_8953_90 - Static variable in class com.rscja.CWDeviceInfo
P80_8953_90 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
P80_8953_90_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
PARITY_EVEN - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Even parity.
PARITY_MARK - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Mark parity.
PARITY_NONE - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  No parity.
PARITY_ODD - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Odd parity.
PARITY_SPACE - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Space parity.
parseA4GPIOInputStatusData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseAndroidDeviceHardwareVersionData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseAndroidDeviceRebootData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseBarcodeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析扫描条码返回的数据
parseBarcodeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBatteryData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析获取电量返回的数据
parseBatteryData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBeepData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析设置蜂鸣器返回的数据
parseBeepData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
  解析设置蜂鸣器返回的数据
parseBeepData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBeepData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseBeepData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseBlinkOfLedData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBlinkOfLedData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBlockEraseDataData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBlockEraseDataData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBlockWriteData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBlockWriteData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBtDeleteAllTagToFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtDeleteAllTagToFlashData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBtGetAllTagNumFromFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtGetAllTagNumFromFlashData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBtGetNewTagNumFromFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtGetNewTagNumFromFlashData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseBtGetTagDataFromFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtGetTagDataFromFlashData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseCloseLedData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseCloseLedData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseCloseUhf(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseContinuousInventoryTagData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  循环盘点标签返回的数据
parseContinuousInventoryTagData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseContinuousInventoryTagData(UHFDataHandleBase.CMDInfo, TagInfoRule) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom
parseData(byte[]) - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
parseData(byte[]) - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
ParseEPCAndTamperAlarm(char[]) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFUARTUAE
ParseEPCAndTamperAlarm(char[]) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
parseErrorCodeData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseEthernetConfigInfoData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseFastIdData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseFastIdData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGBTagLockData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGBTagLockData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetAntData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetAntData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetAntData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetAntennaConnectStateReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetAntennaConnectStateReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetAntWorkTimeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetAntWorkTimeReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetAntWorkTimeReceiveData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetCWData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetCWData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetEPCTIDModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetEPCTIDModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetEthernetIpConfigData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetEthernetIpv6ConfigResultData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetFastIdData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetFastIdData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetFrequencyModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetFrequencyModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetGen2Data(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetGen2Data(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetIOControlReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetIOControlReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetParameterData(byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetPowerAllData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetPowerData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析获取功率返回的数据
parseGetPowerData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetProtocolData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析获取协议返回的数据
parseGetProtocolData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetReaderAwaitSleepTimeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetReaderAwaitSleepTimeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetReaderBeepStatusData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetReaderBeepStatusData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetReaderBeepStatusData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetReaderDestIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetReaderDestIpData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetReaderIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetReaderIpData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetRFLinkData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetRFLinkData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetTagfocusData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetTagfocusData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetTriggerWorkModeParaReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetTriggerWorkModeParaReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseGetUpgradeTcpServiceVersionData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetUserSettingData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseGetWifiIpConfigData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetWifiIpv6ConfigResultData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseGetWorkModeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetWorkModeReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseInventorySingleTagData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析单次盘点标签返回的数据
parseInventorySingleTagData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseInventorySingleTagData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUSBByJava_qcom
parseisBarcodeDataContainSSIIDData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseisBarcodeDataContainTypeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseisBarcodeScanTimeOutData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseKillData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析销毁标签返回的数据
parseKillData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseLockData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析锁标签返回的数据
parseLockData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseOpenLedData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseOpenLedData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseOpenUhf(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseOpenWifiData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseOutputOnAndOffData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parsePortData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseReadData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析读标签返回的数据
parseReadData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseReadMacData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseReadTagData_EPC(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析循环盘点标签返回的标签数据
parseReadTagData_EPC(byte[]) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parseReadTagData_EPC(byte[]) - Static method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
parseReadTagData_EPC(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseReadTagDataEPC_TID_USER(byte[]) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parseReadTagDataEPC_TID_USER(UHFDataHandleBase.CMDInfo, TagInfoRule) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parseReadTagDataEPC_TID_USER(byte[]) - Static method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
parseReadTagDataEPC_TID_USER(UHFDataHandleBase.CMDInfo, TagInfoRule) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseReadTagDataEPC_TID_USER(UHFDataHandleBase.CMDInfo) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUSBByJava_qcom
parserUhfTagBuff_EPC_TID_USER(byte[], TagInfoRule) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parserUhfTagBuff_EPC_TID_USER(byte[], boolean) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parserUhfTagBuff_EPC_TID_USER(byte[], boolean) - Static method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
parserUhfTagBuff_EPC_TID_USER(byte[], boolean) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parserUhfTagBuff_EPC_TID_USER(byte[], TagInfoRule) - Static method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseScanBarcodeInBlinkModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseScanBarcodeInTriggleModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetA4GPIO01Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
parseSetA4GPIO02Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
parseSetA4GPIO03Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
parseSetA4GPIO04Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
parseSetA4GPIOWgData0Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
parseSetA4GPIOWgData1Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
parseSetAntBlinkData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseSetAntData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetAntData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseSetAntData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseSetAntWorkTimeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetAntWorkTimeReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseSetAntWorkTimeReceiveData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseSetBarcodeSSIDData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetBarcodeTypeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetBeepTimeOfDuration(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetBeepTimeOfDuration(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetBuzzeroffOfAndroidData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseSetBuzzerOnOfAndroidData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseSetCWData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetCWData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetEPCAndTIDModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetEPCAndTIDModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetEPCAndTIDUserModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetEPCAndTIDUserModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetEPCModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetEPCModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetEthernetDynamicResultData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseSetFilterData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetFilterData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetFrequencyModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetFrequencyModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetGen2Data(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetGen2Data(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetGPIO03Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA8_qcom
parseSetGPIO04Data(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA8_qcom
parseSetIOControlReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetIOControlReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseSetJumpFrequencyData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetJumpFrequencyData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetParameterData(byte[], byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetPowerData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析设置功率返回的数据
parseSetPowerData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetPowerOnDynamicData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetPowerOnDynamicData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetProtocolData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析设置协议返回的数据
parseSetProtocolData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetR6WorkModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetR6WorkModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetReaderAwaitSleepTimeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetReaderAwaitSleepTimeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetReaderDestIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetReaderDestIpData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseSetReaderIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetReaderIpData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseSetRFLinkData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetRFLinkData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetSoftResetData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetSoftResetData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetSoftResetData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseSetTagfocusData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetTagfocusData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetTriggerWorkModeParaReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetTriggerWorkModeParaReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseSetUserSettingData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseSetWorkModeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetWorkModeReceiveData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
parseStartInventoryTagData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析开始盘点标签返回的数据
parseStartInventoryTagData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseStartUpgradeTcpServiceData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseStartUpgradeUhfData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseSTM32VersionData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSTM32VersionData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseStopInventoryData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析停止盘点标签返回的数据
parseStopInventoryData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseStopScanBarcodeInBlinkModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseStopScanBarcodeInTriggleModeData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseTemperatureData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析模块温度返回的数据
parseTemperatureData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseUHFCurrentIpConfigResultData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseUHFJump2BootData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseUHFJump2BootData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseUHFStartUpdateData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseUHFStartUpdateData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseUHFStopUpdateData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseUHFStopUpdateData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseUHFUpdatingData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseUHFUpdatingData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseVersionData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseVersionData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
parseWifiConfigInfoData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseWifiInfoData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
parseWriteData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析写标签返回的数据
parseWriteData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
Platform() - Constructor for class com.rscja.team.mtk.DeviceConfiguration_mtk.Platform
Platform() - Constructor for class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
PLATFORM_MTK - Static variable in class com.rscja.CWDeviceInfo
PLATFORM_QCOM - Static variable in class com.rscja.CWDeviceInfo
POWER_LED_OFF(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
POWER_LED_OFF(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
POWER_LED_ON(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
POWER_LED_ON(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
powerOff(int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(int) - Method in class com.rscja.deviceapi.Module
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(Context, int) - Method in class com.rscja.deviceapi.Module
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(int) - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(Context, int) - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(int) - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(Context, int) - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  模块下电，仅下电不关串口
  module power off, power off only
powerOn(int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块上电，仅上电不开串口,通过DeviceAPI代码上电,配合`IModule.powerOff(int module)` 使用
  Module power on, power on only
powerOn(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块上电，仅上电不开串口,通过系统app上电,不经过DeviceAPI, 配合`IModule.powerOff(Context context,int module)` 使用
  Module power on, power on only
powerOn(int) - Method in class com.rscja.deviceapi.Module
  模块上电，仅上电不开串口,通过DeviceAPI代码上电,配合`Module.powerOff(int module)` 使用
  Module power on, power on only
powerOn(Context, int) - Method in class com.rscja.deviceapi.Module
  模块上电，仅上电不开串口,通过系统app上电,不经过DeviceAPI, 配合`Module.powerOff(Context context,int module)` 使用
  Module power on, power on only
powerOn(int) - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  模块上电，仅上电不开串口,通过DeviceAPI代码上电,配合`Module_mtk.powerOff(int module)` 使用
  Module power on, power on only
powerOn(Context, int) - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  模块上电，仅上电不开串口,通过系统app上电,不经过DeviceAPI, 配合`Module_mtk.powerOff(Context context,int module)` 使用
  Module power on, power on only
powerOn(int) - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  模块上电，仅上电不开串口,通过DeviceAPI代码上电,配合`Module_qcom.powerOff(int module)` 使用
  Module power on, power on only
powerOn(Context, int) - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  模块上电，仅上电不开串口,通过系统app上电,不经过DeviceAPI, 配合`Module_qcom.powerOff(Context context,int module)` 使用
  Module power on, power on only
print(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印字符
  print character
print(String) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印字符
  printe character
print(String, String) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印字符
  print character
print(Bitmap, int, int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印图片
  print pciture
print(Bitmap, int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印图片
  print picture
print(Bitmap) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印图片
  print picture
print(String, Printer.BarcodeType) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印条码
  print barcode
print(byte[]) - Method in class com.rscja.deviceapi.Printer
  打印字符
  print character
print(String) - Method in class com.rscja.deviceapi.Printer
  打印字符
  printe character
print(String, String) - Method in class com.rscja.deviceapi.Printer
  打印字符
  print character
print(Bitmap, int, int) - Method in class com.rscja.deviceapi.Printer
  打印图片
  print pciture
print(Bitmap, int) - Method in class com.rscja.deviceapi.Printer
  打印图片
  print picture
print(Bitmap) - Method in class com.rscja.deviceapi.Printer
  打印图片
  print picture
print(String, Printer.BarcodeType) - Method in class com.rscja.deviceapi.Printer
  打印条码
  print barcode
print(byte[]) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印字符
  print character
print(String) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印字符
  printe character
print(String, String) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印字符
  print character
print(Bitmap, int, int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印图片
  print pciture
print(Bitmap, int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印图片
  print picture
print(Bitmap) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印图片
  print picture
print(String, Printer.BarcodeType) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印条码
  *print barcode
Printer - Class in com.rscja.deviceapi
  打印机操作类
  Printer operation type
Printer.BarcodeType - Enum in com.rscja.deviceapi
  1D条码类型
Printer.PrinterStatus - Enum in com.rscja.deviceapi
Printer.PrinterStatusCallBack - Interface in com.rscja.deviceapi
Printer_mtk - Class in com.rscja.team.mtk.deviceapi
  打印机操作类
  Printer operation type
PrinterBarcodeInvalidException - Exception in com.rscja.deviceapi.exception
PrinterBarcodeInvalidException(String) - Constructor for exception com.rscja.deviceapi.exception.PrinterBarcodeInvalidException
PrinterFree(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PrinterFree(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PrinterInit(String, String, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PrinterInit(String, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PrinterLowPager - Exception in com.rscja.deviceapi.exception
  打印机缺纸异常类
  printer lack paper exceotion type
PrinterLowPager() - Constructor for exception com.rscja.deviceapi.exception.PrinterLowPager
PrinterReceive(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PrinterReceive(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PrinterSend(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PrinterSend(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PrinterSendAndReceive(byte[], int, byte[], int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PrinterSendAndReceive(byte[], int, byte[], int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PrinterSerialPortOpen(String, String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PrinterSerialPortOpen(String, String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
progress(int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.GRABCallBack
  当前获取指纹图像的进度值
  current progress value of acquired fingerprint
progress(int) - Method in interface com.rscja.deviceapi.FingerprintWithTLK1NC.IUPImageCallback
  当前获取指纹图像的进度值
  current progress value of acquired fingerprint
progress(int) - Method in interface com.rscja.deviceapi.interfaces.IUpgradeProgress
PSAM - Class in com.rscja.deviceapi
  PSAM操作类
  PSAM operation type
PSAM - Class in com.rscja.team.qcom.r1.psam
PSAM(R1HFUSB) - Constructor for class com.rscja.team.qcom.r1.psam.PSAM
Psam_Cmd(String, char, char[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Psam_Cmd(String, char, char[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Psam_Free(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Psam_Free(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Psam_Init(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Psam_Init(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Psam_InitXy(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Psam_InitXy(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PSAM_mtk - Class in com.rscja.team.mtk.deviceapi
  PSAM操作类
  PSAM operation type
PSAM_qcom - Class in com.rscja.team.qcom.deviceapi
  PSAM操作类
  PSAM operation type
PSAM_UPDATE(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PSAM_UPDATE(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PSAMException - Exception in com.rscja.deviceapi.exception
  PSAM异常
  PSAM exceprion
PSAMException(String) - Constructor for exception com.rscja.deviceapi.exception.PSAMException
ptCapture() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹模版
  Acquire fingerprint template
ptCapture() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取指纹模版
  Acquire fingerprint template
PTCapture(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ptCapture() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  获取指纹模版
  Acquire fingerprint template
PTCapture(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ptCapture() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  获取指纹模版
  Acquire fingerprint template
ptConvertTemplateEx(FingerprintWithFIPS.DataFormat, byte[], int) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
ptConvertTemplateEx(FingerprintWithFIPS.DataFormat, byte[], int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
PTConvertTemplateEx(byte, byte, byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ptConvertTemplateEx(FingerprintWithFIPS.DataFormat, byte[], int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
PTConvertTemplateEx(byte, byte, byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ptConvertTemplateEx(FingerprintWithFIPS.DataFormat, byte[], int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
PTDeleteAllFingers(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTDeleteAllFingers(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTEnroll(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTEnroll(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTExit(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTExit(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTGetAppData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTGetAppData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTGrab(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTGrab(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTGUICancel(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTGUICancel(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTInfo(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTInfo(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTInit(String, String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTInit(String, String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTListAllFingers(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTListAllFingers(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTResponseContinue(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTResponseContinue(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTSetAppData(char, char[], char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTSetAppData(char, char[], char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTStoreFinger(byte, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTStoreFinger(byte, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTTLSFContinue(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTTLSFContinue(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTVerify(char, char[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTVerify(char, char[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
PTVerifyALL(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
PTVerifyALL(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
purgeHwBuffers(boolean, boolean) - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Flush non-transmitted output data and / or non-read input data
purgeHwBuffers(boolean, boolean) - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom

A B C D E F G H I J K L M N O P Q R S T U V W X Z