# Constant Field Values

## Contents

- com.rscja.*

## com.rscja.*

- com.rscja.CWDeviceInfo
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `C60_MTK_6765_110` | `"C60_6765_110"`
  `public static final java.lang.String` | `C60_QCM2150_100` | `"C60_QCM2150_100"`
  `public static final java.lang.String` | `C60_SMD450_100` | `"C60_SMD450_100"`
  `public static final java.lang.String` | `C6000_6762` | `"C6000_6762"`
  `public static final java.lang.String` | `C61_SMD450_90` | `"C61_SMD450_90"`
  `public static final java.lang.String` | `C61P_SM6115_110` | `"C61P_SM6115_110"`
  `public static final java.lang.String` | `C66_8953` | `"C66_8953"`
  `public static final java.lang.String` | `C66_SMD450_90` | `"C66_SMD450_90"`
  `public static final java.lang.String` | `C66P_SM6115_110` | `"C66P_SM6115_110"`
  `public static final java.lang.String` | `C90_6762_10` | `"C90"`
  `public static final java.lang.String` | `CW102_6761` | `"CW102_6761"`
  `public static final java.lang.String` | `CW107_6762` | `"CW107_6762"`
  `public static final java.lang.String` | `CW108_8781` | `"CW108_8781"`
  `public static final java.lang.String` | `CW108_8791` | `"CW108_8791"`
  `public static final java.lang.String` | `CW95_6762` | `"CW95_6762"`
  `public static final java.lang.String` | `H100_8953` | `"H100_8953"`
  `public static final java.lang.String` | `MC50_4350_120` | `"MC50_4350_120"`
  `public static final java.lang.String` | `MC51_4350_120` | `"MC51_4350_140"`
  `public static final java.lang.String` | `P80_8786_130` | `"P80_8786_130"`
  `public static final java.lang.String` | `P80_8953` | `"P80_8953"`
  `public static final java.lang.String` | `P80_8953_90` | `"P80_8953_90"`
  `public static final java.lang.String` | `PLATFORM_MTK` | `"mtk"`
  `public static final java.lang.String` | `PLATFORM_QCOM` | `"qualcomm"`
  `public static final int` | `TEAM_MTK` | `1`
  `public static final int` | `TEAM_QCOM` | `2`

- com.rscja.barcode.Barcode2DSHardwareInfo
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `MANUFACTOR_CW` | `"CW"`
  `public static final java.lang.String` | `MANUFACTOR_HONYWELL` | `"HONYWELL"`
  `public static final java.lang.String` | `MANUFACTOR_IA` | `"COASIA"`
  `public static final java.lang.String` | `MANUFACTOR_IDATA` | `"IDATA"`
  `public static final java.lang.String` | `MANUFACTOR_MOBYDATA` | `"MOBYDATA"`
  `public static final java.lang.String` | `MANUFACTOR_NEWLAND` | `"NEWLAND"`
  `public static final java.lang.String` | `MANUFACTOR_ZEBRA` | `"Zebra"`
  `public static final java.lang.String` | `MODEL_CW_CW9281` | `"cw9281"`
  `public static final java.lang.String` | `Model_HONYWELL_3601` | `"HONYWELL_3601"`
  `public static final java.lang.String` | `Model_HONYWELL_3603` | `"HONYWELL_3603"`
  `public static final java.lang.String` | `Model_HONYWELL_6603` | `"N6603"`
  `public static final java.lang.String` | `Model_HONYWELL_EX30` | `"EX30"`
  `public static final java.lang.String` | `Model_HONYWELL_N5703` | `"N5703"`
  `public static final java.lang.String` | `Model_HONYWELL_N6703` | `"N6703"`
  `public static final java.lang.String` | `Model_IA_100S` | `"ia100s"`
  `public static final java.lang.String` | `Model_IA_101S` | `"IA_101S"`
  `public static final java.lang.String` | `Model_IA_166S` | `"IA_166S"`
  `public static final java.lang.String` | `Model_IA_171S` | `"IA_171S"`
  `public static final java.lang.String` | `Model_IA_181S` | `"IA_181S"`
  `public static final java.lang.String` | `Model_IA_400S` | `"IA_400S"`
  `public static final java.lang.String` | `Model_IA_417S` | `"ia417s"`
  `public static final java.lang.String` | `Model_IDATA_DS7000` | `"ds7000p"`
  `public static final java.lang.String` | `Model_MOBYDATA_E3200` | `"e3200"`
  `public static final java.lang.String` | `Model_MOTO_5500` | `"SE5500"`
  `public static final java.lang.String` | `Model_NEWLAND_CM30` | `"cm30_newland"`
  `public static final java.lang.String` | `Model_NEWLAND_CM47` | `"cm47_newland"`
  `public static final java.lang.String` | `Model_NEWLAND_CM60` | `"cm60_newland"`
  `public static final java.lang.String` | `Model_ZEBRA_2100` | `"SE2100"`
  `public static final java.lang.String` | `Model_ZEBRA_4100` | `"SE4100"`
  `public static final java.lang.String` | `Model_ZEBRA_4710` | `"SE4710"`
  `public static final java.lang.String` | `Model_ZEBRA_4720` | `"SE4720"`
  `public static final java.lang.String` | `Model_ZEBRA_4750` | `"SE4750"`
  `public static final java.lang.String` | `Model_ZEBRA_4770` | `"SE4770"`
  `public static final java.lang.String` | `Model_ZEBRA_4850` | `"SE4850"`
  `public static final java.lang.String` | `ZEBRA_ENGINE_SUFFIX_DP` | `"DP"`
  `public static final java.lang.String` | `ZEBRA_ENGINE_SUFFIX_MR` | `"MR"`
  `public static final java.lang.String` | `ZEBRA_ENGINE_SUFFIX_SR` | `"SR"`

- com.rscja.barcode.BarcodeDecoder
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DECODE_CANCEL` | `-1`
  `public static final int` | `DECODE_ENGINE_ERROR` | `-3`
  `public static final int` | `DECODE_FAILURE` | `-2`
  `public static final int` | `DECODE_SUCCESS` | `1`
  `public static final int` | `DECODE_TIMEOUT` | `0`

- com.rscja.barcode.BarcodeSymbolUtility
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `INT_AIM_128` | `52`
  `public static final int` | `INT_AUSPOST` | `16`
  `public static final int` | `INT_AZTEC` | `0`
  `public static final int` | `INT_BOOKLAND` | `53`
  `public static final int` | `INT_BPO` | `14`
  `public static final int` | `INT_CANPOST` | `15`
  `public static final int` | `INT_CHINAPOST` | `42`
  `public static final int` | `INT_CODABAR` | `1`
  `public static final int` | `INT_CODABLOCK` | `18`
  `public static final int` | `INT_CODABLOCK_A` | `35`
  `public static final int` | `INT_CODE_16K` | `48`
  `public static final int` | `INT_CODE11` | `2`
  `public static final int` | `INT_CODE128` | `3`
  `public static final int` | `INT_CODE32` | `28`
  `public static final int` | `INT_CODE39` | `4`
  `public static final int` | `INT_CODE39_FULL_ASCII` | `59`
  `public static final int` | `INT_CODE49` | `36`
  `public static final int` | `INT_CODE93` | `5`
  `public static final int` | `INT_COUPON_CODE` | `55`
  `public static final int` | `INT_CUSTOM_GS1_DATAMATRIX` | `10001`
  `public static final int` | `INT_DATAMATRIX` | `43`
  `public static final int` | `INT_DISCRETE_2_OF_5` | `44`
  `public static final int` | `INT_DUTCHPOST` | `21`
  `public static final int` | `INT_EAN_128` | `46`
  `public static final int` | `INT_EAN13` | `7`
  `public static final int` | `INT_EAN8` | `6`
  `public static final int` | `INT_GRIDMATRIX` | `29`
  `public static final int` | `INT_GS1_128` | `31`
  `public static final int` | `INT_GS1_DATA_MATRIX` | `60`
  `public static final int` | `INT_GS1_DataBar` | `38`
  `public static final int` | `INT_GS1_DataBar_Expanded` | `40`
  `public static final int` | `INT_GS1_DataBar_Limited` | `39`
  `public static final int` | `INT_GS1_QR_CODE` | `61`
  `public static final int` | `INT_HANXIN` | `30`
  `public static final int` | `INT_IATA` | `17`
  `public static final int` | `INT_INFOMAIL` | `37`
  `public static final int` | `INT_INTERLEAVED_2_OF_5` | `45`
  `public static final int` | `INT_ISBT_128` | `54`
  `public static final int` | `INT_ISSN` | `58`
  `public static final int` | `INT_JAPOST` | `19`
  `public static final int` | `INT_KOREAPOST` | `26`
  `public static final int` | `INT_MACRO_PDF` | `56`
  `public static final int` | `INT_MACRO_QR` | `57`
  `public static final int` | `INT_MATRIX25` | `27`
  `public static final int` | `INT_MAXICODE` | `9`
  `public static final int` | `INT_MICRO_QR` | `51`
  `public static final int` | `INT_MICROPDF` | `10`
  `public static final int` | `INT_MSI` | `23`
  `public static final int` | `INT_NEC_2_OF_5` | `41`
  `public static final int` | `INT_PDF417` | `11`
  `public static final int` | `INT_PLANET` | `20`
  `public static final int` | `INT_POSTAL_4I` | `34`
  `public static final int` | `INT_QR` | `25`
  `public static final int` | `INT_TELEPEN` | `22`
  `public static final int` | `INT_TLCODE39` | `24`
  `public static final int` | `INT_TRIOPTIC` | `50`
  `public static final int` | `INT_UPC_D` | `49`
  `public static final int` | `INT_UPC_E1` | `47`
  `public static final int` | `INT_UPCA` | `12`
  `public static final int` | `INT_UPCE0` | `13`
  `public static final int` | `INT_US_POSTALS1` | `33`
  `public static final int` | `INT_USPS4CB` | `32`
  `public static final java.lang.String` | `STR_AIM_128` | `"AIM_128"`
  `public static final java.lang.String` | `STR_AUSPOST` | `"AUSPOST"`
  `public static final java.lang.String` | `STR_AZTEC` | `"AZTEC"`
  `public static final java.lang.String` | `STR_BOOKLAND` | `"BOOKLAND"`
  `public static final java.lang.String` | `STR_BPO` | `"BPO"`
  `public static final java.lang.String` | `STR_CANPOST` | `"CANPOST"`
  `public static final java.lang.String` | `STR_CHINAPOST` | `"CHINAPOST"`
  `public static final java.lang.String` | `STR_CODABAR` | `"CODABAR"`
  `public static final java.lang.String` | `STR_CODABLOCK` | `"CODABLOCK"`
  `public static final java.lang.String` | `STR_CODABLOCK_A` | `"CODABLOCK_A"`
  `public static final java.lang.String` | `STR_CODE_16K` | `"CODE_16K"`
  `public static final java.lang.String` | `STR_CODE11` | `"CODE11"`
  `public static final java.lang.String` | `STR_CODE128` | `"CODE128"`
  `public static final java.lang.String` | `STR_CODE32` | `"CODE32"`
  `public static final java.lang.String` | `STR_CODE39` | `"CODE39"`
  `public static final java.lang.String` | `STR_CODE39_FULL_ASCII` | `"CODE39_FULL_ASCII1"`
  `public static final java.lang.String` | `STR_CODE49` | `"CODE49"`
  `public static final java.lang.String` | `STR_CODE93` | `"CODE93"`
  `public static final java.lang.String` | `STR_COUPON_CODE` | `"COUPON_CODE"`
  `public static final java.lang.String` | `STR_CUSTOM_GS1_DATAMATRIX` | `"GS1_DATAMATRIX"`
  `public static final java.lang.String` | `STR_DATAMATRIX` | `"DATAMATRIX"`
  `public static final java.lang.String` | `STR_DISCRETE_2_OF_5` | `"DISCRETE_2_OF_5"`
  `public static final java.lang.String` | `STR_DUTCHPOST` | `"DUTCHPOST"`
  `public static final java.lang.String` | `STR_EAN_128` | `"EAN128"`
  `public static final java.lang.String` | `STR_EAN13` | `"EAN13"`
  `public static final java.lang.String` | `STR_EAN8` | `"EAN8"`
  `public static final java.lang.String` | `STR_GRIDMATRIX` | `"GRIDMATRIX"`
  `public static final java.lang.String` | `STR_GS1_128` | `"GS1_128"`
  `public static final java.lang.String` | `STR_GS1_DATA_MATRIX` | `"GS1_DATA_MATRIX"`
  `public static final java.lang.String` | `STR_GS1_DataBar` | `"GS1_DataBar"`
  `public static final java.lang.String` | `STR_GS1_DataBar_Expanded` | `"GS1_DataBar_Expanded"`
  `public static final java.lang.String` | `STR_GS1_DataBar_Limited` | `"GS1_DataBar_Limited"`
  `public static final java.lang.String` | `STR_GS1_QR` | `"GS1_QR"`
  `public static final java.lang.String` | `STR_HANXIN` | `"HANXIN"`
  `public static final java.lang.String` | `STR_IATA` | `"IATA"`
  `public static final java.lang.String` | `STR_INFOMAIL` | `"INFOMAIL"`
  `public static final java.lang.String` | `STR_INTERLEAVED_2_OF_5` | `"INTERLEAVED_2_OF_5"`
  `public static final java.lang.String` | `STR_ISBT_128` | `"ISBT_128"`
  `public static final java.lang.String` | `STR_ISSN` | `"ISSN"`
  `public static final java.lang.String` | `STR_JAPOST` | `"JAPOST"`
  `public static final java.lang.String` | `STR_KOREAPOST` | `"KOREAPOST"`
  `public static final java.lang.String` | `STR_MACRO_PDF` | `"MACRO_PDF"`
  `public static final java.lang.String` | `STR_MACRO_QR` | `"MACRO_QR"`
  `public static final java.lang.String` | `STR_MATRIX25` | `"MATRIX25"`
  `public static final java.lang.String` | `STR_MAXICODE` | `"MAXICODE"`
  `public static final java.lang.String` | `STR_MICRO_QR` | `"MICRO_QR"`
  `public static final java.lang.String` | `STR_MICROPDF` | `"MICROPDF"`
  `public static final java.lang.String` | `STR_MSI` | `"MSI"`
  `public static final java.lang.String` | `STR_NEC_2_OF_5` | `"NEC_2_OF_5"`
  `public static final java.lang.String` | `STR_PDF417` | `"PDF417"`
  `public static final java.lang.String` | `STR_PLANET` | `"PLANET"`
  `public static final java.lang.String` | `STR_POSTAL_4I` | `"POSTAL_4I"`
  `public static final java.lang.String` | `STR_QR` | `"QR"`
  `public static final java.lang.String` | `STR_TELEPEN` | `"TELEPEN"`
  `public static final java.lang.String` | `STR_TLCODE39` | `"TLCODE39"`
  `public static final java.lang.String` | `STR_TRIOPTIC` | `"TRIOPTIC"`
  `public static final java.lang.String` | `STR_UPC_D` | `"UPC_D"`
  `public static final java.lang.String` | `STR_UPC_E1` | `"UPC_E1"`
  `public static final java.lang.String` | `STR_UPCA` | `"UPCA"`
  `public static final java.lang.String` | `STR_UPCE0` | `"UPCE0"`
  `public static final java.lang.String` | `STR_US_POSTALS1` | `"US_POSTALS1"`
  `public static final java.lang.String` | `STR_USPS4CB` | `"USPS4CB"`

- com.rscja.barcode.BarcodeUtility
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `ACTION_SCAN_KEYBOARD_HELPER_PARAM_RESPONSE` | `"android.intent.action.SCAN_KEYBOARD_HELPER_PARAM_RESPONSE"`
  `public static final java.lang.String` | `SCANNER_BARCODE_1D` | `"scanner_cbBarcode1D"`
  `public static final java.lang.String` | `SCANNER_BARCODE_2D` | `"scanner_cbBarcode2D_s"`
  `public static final java.lang.String` | `SCANNER_BARCODENOTREPEAT` | `"scanner_BarcodeNotRepeat"`
  `public static final java.lang.String` | `SCANNER_BROADCAST_ACTION` | `"scanner_etBroadcast"`
  `public static final java.lang.String` | `SCANNER_BROADCAST_EXTRA` | `"scanner_etBroadcastKey"`
  `public static final java.lang.String` | `SCANNER_CONTINUOUS` | `"scanner_Continuous"`
  `public static final java.lang.String` | `SCANNER_CONTINUOUS_INTREVALTIME` | `"scanner_ContinuousIntervalTime"`
  `public static final java.lang.String` | `SCANNER_CONTINUOUSMODE` | `"ContinuousMode"`
  `public static final java.lang.String` | `SCANNER_CONTINUOUSTIMEOUT` | `"scanner_ContinuousTimeOut"`
  `public static final java.lang.String` | `SCANNER_ENDINDEX` | `"scanner_etEndIndex"`
  `public static final java.lang.String` | `SCANNER_ENTER` | `"scanner_cbEnter"`
  `public static final java.lang.String` | `SCANNER_FAILUREBROADCAST` | `"scanner_failureBroadcast"`
  `public static final java.lang.String` | `SCANNER_FAILURESOUND` | `"scanner_failureSound"`
  `public static final java.lang.String` | `SCANNER_FILTERCHARS` | `"scanner_FilterChars"`
  `public static final java.lang.String` | `SCANNER_FORMAT_BARCODE` | `"scanner_format_barcode"`
  `public static final java.lang.String` | `SCANNER_ILLUMINATIONPOWERLEVEL` | `"scanner_IlluminationPowerLevel"`
  `public static final java.lang.String` | `SCANNER_KEYBORADHELPER_OPEN` | `"scanner_cbOpen"`
  `public static final java.lang.String` | `SCANNER_OUTPUTMODE` | `"scanner_target"`
  `public static final java.lang.String` | `SCANNER_PREFIX` | `"scanner_etPrefix"`
  `public static final java.lang.String` | `SCANNER_RELEASESCAN` | `"scanner_cbERKOS"`
  `public static final java.lang.String` | `SCANNER_SCANKEYCODE_1` | `"scanner_scanKeyCode_1"`
  `public static final java.lang.String` | `SCANNER_SCANKEYCODE_3` | `"scanner_scanKeyCode_3"`
  `public static final java.lang.String` | `SCANNER_SOUND` | `"scanner_Sound"`
  `public static final java.lang.String` | `SCANNER_STARTINDEX` | `"scanner_etStartIndex"`
  `public static final java.lang.String` | `SCANNER_SUFFIX` | `"scanner_etSuffix"`
  `public static final java.lang.String` | `SCANNER_TAB` | `"scanner_cbTab"`
  `public static final java.lang.String` | `SCANNER_TIMEOUT` | `"scanner_TimeOut"`
  `public static final java.lang.String` | `SCANNER_VIBRATE` | `"scanner_Vibrate"`

- com.rscja.barcode.ConstantUtil
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `BARCODE_BYTE_DATA` | `"barcodeByteData"`
  `public static final java.lang.String` | `BARCODE_CODE` | `"barcodeCode"`
  `public static final java.lang.String` | `BARCODE_DECODE_TIME` | `"barcodeDecodeTime"`
  `public static final java.lang.String` | `BARCODE_HEX_DATA` | `"barcodeHexData"`
  `public static final java.lang.String` | `BARCODE_NAME` | `"barcodeNAME"`
  `public static final java.lang.String` | `BARCODE_RESULT_CODE` | `"barcodeResultCode"`
  `public static final java.lang.String` | `BARCODE_STRING_DATA` | `"barcodeStringData"`
  `public static final java.lang.String` | `RESULT_STATUS` | `"resultStatus"`

- com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `ACTION_USB_PERMISSION` | `"com.rscja.USB_PERMISSION"`

- com.rscja.deviceapi.RFIDWithUHFUSB
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `ACTION_USB_PERMISSION` | `"com.rscja.USB_PERMISSION"`

- com.rscja.deviceapi.UhfBase.ErrorCode
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `ERRCODE_FAILURE` | `-1`
  `public static final int` | `ERRCODE_SUCCESS` | `0`
  `public static final int` | `ERROR_INSUFFICIENT_PRIVILEGES` | `2`
  `public static final int` | `ERROR_MEMORY_LOCK` | `4`
  `public static final int` | `ERROR_MEMORY_OVERRUN` | `3`
  `public static final int` | `ERROR_NO_ENOUGH_POWER_ON_TAG` | `11`
  `public static final int` | `ERROR_NO_TAG` | `1`
  `public static final int` | `ERROR_OPERATION_FAILED` | `255`
  `public static final int` | `ERROR_PASSWORD_IS_INCORRECT` | `6`
  `public static final int` | `ERROR_RECV_FAIL` | `253`
  `public static final int` | `ERROR_RESPONSE_BUFFER_OVERFLOW` | `7`
  `public static final int` | `ERROR_SEND_FAIL` | `252`
  `public static final int` | `ERROR_TAG_NO_REPLY` | `5`

- com.rscja.deviceapi.entity.BarcodeResult
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `A` | `"UPC-A, UPC-E, UPC-E1, EAN-8, EAN-13"`
  `public static final java.lang.String` | `B` | `"Code 39, Code 32"`
  `public static final java.lang.String` | `C` | `"Codabar"`
  `public static final java.lang.String` | `D` | `"Code 128, ISBT 128, ISBT 128 Concatenated"`
  `public static final java.lang.String` | `E` | `"Code 93"`
  `public static final java.lang.String` | `F` | `"Interleaved 2 of 5"`
  `public static final java.lang.String` | `G` | `"Discrete 2 of 5, or Discrete 2 of 5 IATA"`
  `public static final java.lang.String` | `H` | `"Code 11"`
  `public static final java.lang.String` | `J` | `"MSI"`
  `public static final java.lang.String` | `K` | `"GS1-128"`
  `public static final java.lang.String` | `L` | `"Bookland EAN"`
  `public static final java.lang.String` | `M` | `"Trioptic Code 39"`
  `public static final java.lang.String` | `N` | `"Coupon Code"`
  `public static final java.lang.String` | `P00` | `"Data Matrix"`
  `public static final java.lang.String` | `P01` | `"QR Code, MicroQR"`
  `public static final java.lang.String` | `P02` | `"Maxicode"`
  `public static final java.lang.String` | `P03` | `"US Postnet"`
  `public static final java.lang.String` | `P04` | `"US Planet"`
  `public static final java.lang.String` | `P05` | `"Japan Postal"`
  `public static final java.lang.String` | `P06` | `"UK Postal"`
  `public static final java.lang.String` | `P08` | `"Netherlands KIX Code"`
  `public static final java.lang.String` | `P09` | `"Australia Post"`
  `public static final java.lang.String` | `P0A` | `"USPS 4CB/One Code/Intelligent Mail"`
  `public static final java.lang.String` | `P0B` | `"UPU FICS Postal"`
  `public static final java.lang.String` | `P0H` | `"Han Xin"`
  `public static final java.lang.String` | `P0X` | `"Signature Capture"`
  `public static final java.lang.String` | `R` | `"GS1 DataBar Family"`
  `public static final java.lang.String` | `S` | `"Matrix 2 of 5"`
  `public static final java.lang.String` | `T` | `"UCC Composite, TLC 39"`
  `public static final java.lang.String` | `U` | `"Chinese 2 of 5"`
  `public static final java.lang.String` | `V` | `"Korean 3 of 5"`
  `public static final java.lang.String` | `X` | `"ISSN EAN, PDF417, Macro PDF417, Micro PDF417"`
  `public static final java.lang.String` | `Z` | `"Aztec, Aztec Rune"`

- com.rscja.deviceapi.entity.GPIStateEntity
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `GPI1` | `"GPI1"`
  `public static final java.lang.String` | `GPI2` | `"GPI2"`
  `public static final java.lang.String` | `GPI3` | `"GPI3"`
  `public static final java.lang.String` | `GPI4` | `"GPI4"`

- com.rscja.deviceapi.entity.GPOEntity
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `GPO1` | `"GPO1"`
  `public static final java.lang.String` | `GPO2` | `"GPO2"`
  `public static final java.lang.String` | `GPO3` | `"GPO3"`
  `public static final java.lang.String` | `GPO4` | `"GPO4"`
  `public static final java.lang.String` | `WiegandData0` | `"WiegandData0"`
  `public static final java.lang.String` | `WiegandData1` | `"WiegandData1"`

- com.rscja.deviceapi.entity.UHFTAGInfo
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public final java.lang.String` | `EXTRADATA_EPCAREA` | `"epcArea"`

- com.rscja.deviceapi.interfaces.IBarcodePictureCallback
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final byte` | `IMG_FORMAT_BMP` | `3`
  `public static final byte` | `IMG_FORMAT_JPEG` | `1`
  `public static final byte` | `IMG_FORMAT_TIFF` | `4`

- com.rscja.deviceapi.interfaces.IBluetoothReader
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `VERSION_BT_FIRMWARE` | `"FIRMWARE"`
  `public static final java.lang.String` | `VERSION_BT_HARDWARE` | `"HARDWARE"`
  `public static final java.lang.String` | `VERSION_BT_SOFTWARE` | `"SOFTWARE"`

- com.rscja.deviceapi.interfaces.IReader
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final char` | `UPDATE_STM32` | `0`

- com.rscja.deviceapi.interfaces.IUHF
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `Bank_EPC` | `1`
  `public static final int` | `Bank_RESERVED` | `0`
  `public static final int` | `Bank_TID` | `2`
  `public static final int` | `Bank_USER` | `3`
  `public static final int` | `LockBank_ACCESS` | `32`
  `public static final int` | `LockBank_EPC` | `48`
  `public static final int` | `LockBank_KILL` | `16`
  `public static final int` | `LockBank_TID` | `64`
  `public static final int` | `LockBank_USER` | `80`
  `public static final int` | `LockMode_LOCK` | `16`
  `public static final int` | `LockMode_OPEN` | `32`
  `public static final int` | `LockMode_PLOCK` | `48`
  `public static final int` | `LockMode_POPEN` | `64`
  `public static final char` | `UPDATE_UHF` | `1`

- com.rscja.scanner.IScanner
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `FORMAT_ASCII` | `1`
  `public static final int` | `FORMAT_DECIMAL` | `6`
  `public static final int` | `FORMAT_DEFAULT` | `0`
  `public static final int` | `FORMAT_GB18030` | `6`
  `public static final int` | `FORMAT_GB2312` | `2`
  `public static final int` | `FORMAT_GBK` | `5`
  `public static final int` | `FORMAT_HEX` | `5`
  `public static final int` | `FORMAT_UNICODE` | `4`
  `public static final int` | `FORMAT_UTF8` | `3`
  `public static final int` | `FUNCTION_14443A` | `3`
  `public static final int` | `FUNCTION_15693` | `4`
  `public static final int` | `FUNCTION_1D` | `0`
  `public static final int` | `FUNCTION_2D` | `2`
  `public static final int` | `FUNCTION_2D_H` | `1`
  `public static final int` | `FUNCTION_LF_ANIMAL` | `6`
  `public static final int` | `FUNCTION_LF_EM4450` | `9`
  `public static final int` | `FUNCTION_LF_HDX` | `8`
  `public static final int` | `FUNCTION_LF_HID` | `10`
  `public static final int` | `FUNCTION_LF_HITAG` | `7`
  `public static final int` | `FUNCTION_LF_ID` | `5`
  `public static final int` | `FUNCTION_LF_NEEDLE` | `12`
  `public static final int` | `FUNCTION_UHF` | `11`

- com.rscja.team.mtk.DeviceConfiguration_mtk
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `C6000_6762` | `"C6000_6762"`
  `public static final java.lang.String` | `C90_6762_10` | `"C90"`

- com.rscja.team.mtk.DeviceConfiguration_mtk.Platform
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `MTK` | `"mtk"`
  `public static final java.lang.String` | `QUACOMM` | `"qualcomm"`

- com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DECODE_CANCEL` | `-1`
  `public static final int` | `DECODE_ENGINE_ERROR` | `-3`
  `public static final int` | `DECODE_FAILURE` | `-2`
  `public static final int` | `DECODE_SUCCESS` | `1`
  `public static final int` | `DECODE_TIMEOUT` | `0`

- com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `INT_GM` | `56`
  `public static final int` | `INT_INDUSTRIAL_2_5` | `55`
  `public static final int` | `INT_ISBT_128` | `53`
  `public static final int` | `INT_OCR` | `57`
  `public static final int` | `INT_STANDARD_2_5` | `54`
  `public static final java.lang.String` | `STR_GM` | `"GM"`
  `public static final java.lang.String` | `STR_INDUSTRIAL_2_5` | `"INDUSTRIAL_2_5"`
  `public static final java.lang.String` | `STR_ISBT_128` | `"ISBT_128"`
  `public static final java.lang.String` | `STR_OCR` | `"OCR"`
  `public static final java.lang.String` | `STR_STANDARD_2_5` | `"STANDARD_2_5"`

- com.rscja.team.qcom.DeviceConfiguration_qcom
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `C60_MTK_6765_110` | `"C60_6765_110"`
  `public static final java.lang.String` | `C60_QCM2150_100` | `"C60_QCM2150_100"`
  `public static final java.lang.String` | `C60_SMD450_100` | `"C60_SMD450_100"`
  `public static final java.lang.String` | `C61_SMD450_90` | `"C61_SMD450_90"`
  `public static final java.lang.String` | `C61P_SM6115_110` | `"C61P_SM6115_110"`
  `public static final java.lang.String` | `C66_8953` | `"C66_8953"`
  `public static final java.lang.String` | `C66_SMD450_90` | `"C66_SMD450_90"`
  `public static final java.lang.String` | `C66P_SM6115_110` | `"C66P_SM6115_110"`
  `public static final java.lang.String` | `H100_8953` | `"H100_8953"`
  `public static final java.lang.String` | `MC50_4350_120` | `"MC50_4350_120"`
  `public static final java.lang.String` | `P80_8786_130` | `"P80_8786_130"`
  `public static final java.lang.String` | `P80_8953` | `"P80_8953"`
  `public static final java.lang.String` | `P80_8953_90` | `"P80_8953_90"`

- com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `CPU_MTK_6735` | `"6735"`
  `public static final java.lang.String` | `CPU_MTK_6763` | `"6763"`
  `public static final java.lang.String` | `CPU_MTK_6765` | `"6765"`
  `public static final java.lang.String` | `CPU_MTK_8786` | `"8786"`
  `public static final java.lang.String` | `CPU_QUACOMM_4350` | `"4350"`
  `public static final java.lang.String` | `CPU_QUACOMM_8909` | `"8909"`
  `public static final java.lang.String` | `CPU_QUACOMM_8953` | `"8953"`
  `public static final java.lang.String` | `CPU_QUACOMM_QCM2150` | `"qcm2150"`
  `public static final java.lang.String` | `CPU_QUACOMM_SM6115` | `"sm6115"`
  `public static final java.lang.String` | `CPU_QUACOMM_SMD450` | `"smd450"`
  `public static final java.lang.String` | `CPU_RK_3568` | `"3568"`
  `public static final java.lang.String` | `MTK` | `"mtk"`
  `public static final java.lang.String` | `QUACOMM` | `"qualcomm"`
  `public static final java.lang.String` | `RK` | `"rockchip"`

- com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `ACTION_GET_LAST_DEC_IMAGE` | `"com.rscja.scanner.action.GET_LAST_DEC_IMAGE"`
  `public static final java.lang.String` | `ACTION_SCAN_PARAMETER` | `"com.rscja.scanner.barcode.ZEBRA_PARAMETER_RESPONSE"`
  `public static final java.lang.String` | `DEC_IMAGE_KEY` | `"imageData"`

- com.rscja.team.qcom.r1.hf.HFBase
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public final int` | `COMMAND_15693_SELECT` | `165`
  `public final int` | `COMMAND_ACTIVATEIDLE` | `65`
  `public final int` | `COMMAND_ANTICOLL` | `66`
  `public final int` | `COMMAND_ANTICOLLINVENTORY` | `174`
  `public final int` | `COMMAND_AUTHENTICATION` | `69`
  `public final int` | `COMMAND_COS_COMMAND` | `103`
  `public final int` | `COMMAND_DECREMENT` | `74`
  `public final int` | `COMMAND_FM1216RESET` | `57`
  `public final int` | `COMMAND_GET_MUL_BLOCK` | `172`
  `public final int` | `COMMAND_GET_SYSTEM_INFO` | `171`
  `public final int` | `COMMAND_HALT` | `68`
  `public final int` | `COMMAND_HALT_TYPEB` | `99`
  `public final int` | `COMMAND_INCREMENT` | `75`
  `public final int` | `COMMAND_INITVAL` | `72`
  `public final int` | `COMMAND_INVENTORY` | `160`
  `public final int` | `COMMAND_LOCK_AFI` | `168`
  `public final int` | `COMMAND_LOCK_BLOCK` | `164`
  `public final int` | `COMMAND_LOCK_DSFID` | `170`
  `public final int` | `COMMAND_READ` | `70`
  `public final int` | `COMMAND_READ_SM` | `162`
  `public final int` | `COMMAND_READVAL` | `73`
  `public final int` | `COMMAND_REQUESTA` | `64`
  `public final int` | `COMMAND_RESET_TO_READY` | `166`
  `public final int` | `COMMAND_RESTORE` | `76`
  `public final int` | `COMMAND_SELECT` | `67`
  `public final int` | `COMMAND_TRANSFER` | `77`
  `public final int` | `COMMAND_TRANSFERCOMMAND` | `173`
  `public final int` | `COMMAND_TYPEARATS` | `80`
  `public final int` | `COMMAND_TYPEAREST` | `81`
  `public final int` | `COMMAND_TYPEB_GET_UID` | `101`
  `public final int` | `COMMAND_TYPEBREST` | `100`
  `public final int` | `COMMAND_ULANTICOLL` | `78`
  `public final int` | `COMMAND_ULWRITE` | `79`
  `public final int` | `COMMAND_WRITE` | `71`
  `public final int` | `COMMAND_WRITE_AFI` | `167`
  `public final int` | `COMMAND_WRITE_DSFID` | `169`
  `public final int` | `COMMAND_WRITE_SM` | `163`

- com.rscja.team.qcom.scanner.utility.ScannerParameterUtility_qcom
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `key_barcodeBroadcastAction` | `"BarcodeBroadcastAction"`
  `public static final java.lang.String` | `key_BarcodeNotRepeat` | `"BarcodeNotRepeat"`
  `public static final java.lang.String` | `key_cbBarcode2D_s` | `"Barcode2D"`
  `public static final java.lang.String` | `key_cbEnter` | `"Enter"`
  `public static final java.lang.String` | `key_cbERKOS` | `"ReleaseScanKeySotpScan"`
  `public static final java.lang.String` | `key_cbSpace` | `"Space"`
  `public static final java.lang.String` | `key_cbTab` | `"Tab"`
  `public static final java.lang.String` | `key_Continuous` | `"BarcodeContinuousScan"`
  `public static final java.lang.String` | `key_ContinuousIntervalTime` | `"BarcodeContinuousScanIntervalTime"`
  `public static final java.lang.String` | `key_ContinuousIntervalTimeUHF` | `"UHFContinuousScanIntervalTime"`
  `public static final java.lang.String` | `key_ContinuousMode` | `"BarcodeContinuousScanMode"`
  `public static final java.lang.String` | `key_ContinuousTimeOut` | `"BarcodeContinuousScanTimeOut"`
  `public static final java.lang.String` | `key_ContinuousTimeOutUHF` | `"UHFContinuousScanTimeOut"`
  `public static final java.lang.String` | `key_ContinuousUHF` | `"UHFContinuous"`
  `public static final java.lang.String` | `key_debug` | `"Scanner_Debug"`
  `public static final java.lang.String` | `key_endIndex` | `"EndIndex"`
  `public static final java.lang.String` | `key_etBroadcastKey` | `"BarcodeBroadcastDataKey"`
  `public static final java.lang.String` | `key_failureBroadcast` | `"ScanFailureBroadcast"`
  `public static final java.lang.String` | `key_failureSound` | `"ScanFailureSound"`
  `public static final java.lang.String` | `key_filterChars` | `"FilterChars"`
  `public static final java.lang.String` | `key_firstInit` | `"Scanner_FirstInit"`
  `public static final java.lang.String` | `key_firstSetScanP` | `"Scanner_FirstSetScanP"`
  `public static final java.lang.String` | `key_format_Barcode` | `"BarcodeFormat"`
  `public static final java.lang.String` | `key_format_RFID` | `"RFIDFormat"`
  `public static final java.lang.String` | `key_GS1Parsing` | `"GS1Parsing"`
  `public static final java.lang.String` | `key_IlluminationPowerLevel` | `"IlluminationPowerLevel"`
  `public static final java.lang.String` | `key_InterceptScanKey` | `"InterceptScanKey"`
  `public static final java.lang.String` | `key_LF_Last4Bytes` | `"RFID_LF_Last4Bytes"`
  `public static final java.lang.String` | `key_Mirror` | `"CoAsiaMirror"`
  `public static final java.lang.String` | `key_prefix` | `"Prefix"`
  `public static final java.lang.String` | `key_ScanAuxiliaryLight` | `"ScanAuxiliaryLight"`
  `public static final java.lang.String` | `key_Scanner_Enable` | `"Scanner_Enable"`
  `public static final java.lang.String` | `key_scanOnRelease` | `"ScanOnRelease"`
  `public static final java.lang.String` | `key_sort` | `"Scanner_Sort"`
  `public static final java.lang.String` | `key_Sound` | `"SuccessSound"`
  `public static final java.lang.String` | `key_startIndex` | `"StartIndex"`
  `public static final java.lang.String` | `key_suffix` | `"Suffix"`
  `public static final java.lang.String` | `key_target` | `"OutputMode"`
  `public static final java.lang.String` | `key_TimeOut` | `"ScanTimeOut"`
  `public static final java.lang.String` | `key_Vibrate` | `"Vibrate"`

- com.rscja.team.qcom.service.BLEService_qcom
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final java.lang.String` | `ACTION_DATA_AVAILABLE` | `"com.nordicsemi.nrfUART.ACTION_DATA_AVAILABLE"`
  `public static final java.lang.String` | `ACTION_GATT_DISCONNECTED` | `"com.nordicsemi.nrfUART.ACTION_GATT_DISCONNECTED"`
  `public static final java.lang.String` | `ACTION_GATT_SERVICES_DISCOVERED` | `"com.nordicsemi.nrfUART.ACTION_GATT_SERVICES_DISCOVERED"`
  `public static final java.lang.String` | `ACTION_SEARCH_DEVICES` | `"com.nordicsemi.nrfUART.ACTION_SEARCH_DEVICES"`
  `public static final java.lang.String` | `BT_DEVICE` | `"device"`
  `public static final java.lang.String` | `BT_RECORD` | `"record"`
  `public static final java.lang.String` | `BT_RSSI` | `"rssi"`
  `public static final java.lang.String` | `DEVICE_DOES_NOT_SUPPORT_UART` | `"com.nordicsemi.nrfUART.DEVICE_DOES_NOT_SUPPORT_UART"`
  `public static final java.lang.String` | `EXTRA_DATA` | `"com.nordicsemi.nrfUART.EXTRA_DATA"`

- com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Modifier and Type | Constant Field | Value
  --- | --- | ---
  `public static final int` | `DATABITS_5` | `5`
  `public static final int` | `DATABITS_6` | `6`
  `public static final int` | `DATABITS_7` | `7`
  `public static final int` | `DATABITS_8` | `8`
  `public static final int` | `FLOWCONTROL_NONE` | `0`
  `public static final int` | `FLOWCONTROL_RTSCTS_IN` | `1`
  `public static final int` | `FLOWCONTROL_RTSCTS_OUT` | `2`
  `public static final int` | `FLOWCONTROL_XONXOFF_IN` | `4`
  `public static final int` | `FLOWCONTROL_XONXOFF_OUT` | `8`
  `public static final int` | `PARITY_EVEN` | `2`
  `public static final int` | `PARITY_MARK` | `3`
  `public static final int` | `PARITY_NONE` | `0`
  `public static final int` | `PARITY_ODD` | `1`
  `public static final int` | `PARITY_SPACE` | `4`
  `public static final int` | `STOPBITS_1` | `1`
  `public static final int` | `STOPBITS_1_5` | `3`
  `public static final int` | `STOPBITS_2` | `2`