A B C D E F G H I J K L M N O P Q R S T U V W X Z

## A

A - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
A4_8953_90 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
A4_RK_3568_110 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
A4C8_RK_3568_110 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
A4OptoCoupler3Off(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4OptoCoupler3Off(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A4OptoCoupler3On(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4OptoCoupler3On(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A4OptoCoupler4Off(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4OptoCoupler4Off(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A4OptoCoupler4On(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4OptoCoupler4On(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A4WgData0Off(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4WgData0Off(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A4WgData0On(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4WgData0On(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A4WgData1Off(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4WgData1Off(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A4WgData1On(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A4WgData1On(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A8_8909 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
A8_8953_90 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
A8UhfOutput3Off(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A8UhfOutput3Off(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A8UhfOutput3On(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A8UhfOutput3On(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A8UhfOutput4Off(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A8UhfOutput4Off(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
A8UhfOutput4On(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
A8UhfOutput4On(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ACTION_DATA_AVAILABLE - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
ACTION_GATT_DISCONNECTED - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
ACTION_GATT_SERVICES_DISCOVERED - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
ACTION_GET_LAST_DEC_IMAGE - Static variable in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
ACTION_SCAN_KEYBOARD_HELPER_PARAM_RESPONSE - Static variable in class com.rscja.barcode.BarcodeUtility
ACTION_SCAN_PARAMETER - Static variable in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
ACTION_SEARCH_DEVICES - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
ACTION_USB_PERMISSION - Static variable in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
ACTION_USB_PERMISSION - Static variable in class com.rscja.deviceapi.RFIDWithUHFUSB
addBleDevice(String, Context) - Method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
  增加蓝牙设备
addCmd(UHFProtocolProtocolParseBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
addCmdList(UHFDataHandleBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfhandler.HFR1UsbDataHandle
addCmdList(UHFDataHandleBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
addCmdList(UHFDataHandleBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfhandler.UHFRxBLEDataHandle
addCmdList(UHFDataHandleBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfhandler.UHFRxUsbDataHandle
addCmdList(UHFDataHandleBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfhandler.UHFUR4DataHandle
addCmdList(UHFDataHandleBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfhandler.UHFUrAxDataHandle
addCmdList(UHFProtocolProtocolParseBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfparse.UHFBLEProtocolParse
addCmdList(UHFProtocolProtocolParseBase.CMDInfo) - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
addData(float, float, float) - Method in class com.rscja.team.qcom.utility.GyroAngle
addLiveAPP(String[]) - Method in interface com.rscja.system.ISystemInterfaces
  增加保活APP
ADDR - Static variable in class com.rscja.team.mtk.utility.FileUtils
angleX - Variable in class com.rscja.team.qcom.utility.GyroAngle
angleY - Variable in class com.rscja.team.qcom.utility.GyroAngle
angleZ - Variable in class com.rscja.team.qcom.utility.GyroAngle
AnimalEntity - Class in com.rscja.deviceapi.entity
  动物标签数据实体类
  animal tag data entity
AnimalEntity(long, long, long, long, long) - Constructor for class com.rscja.deviceapi.entity.AnimalEntity
  构造函数
  Constructor
AnimalEntity() - Constructor for class com.rscja.deviceapi.entity.AnimalEntity
AntennaConnectState - Class in com.rscja.deviceapi.entity
AntennaConnectState(AntennaEnum, boolean) - Constructor for class com.rscja.deviceapi.entity.AntennaConnectState
AntennaEnum - Enum in com.rscja.deviceapi.enums
AntennaPowerEntity - Class in com.rscja.deviceapi.entity
AntennaPowerEntity() - Constructor for class com.rscja.deviceapi.entity.AntennaPowerEntity
AntennaState - Class in com.rscja.deviceapi.entity
AntennaState(AntennaEnum, boolean) - Constructor for class com.rscja.deviceapi.entity.AntennaState
AntInfo() - Constructor for class com.rscja.custom.UHFSFForUrxNetwork.AntInfo
antLedSwitch(int, boolean) - Method in interface com.rscja.team.qcom.urax.IURAxDevice
antLedSwitch(int, boolean) - Method in class com.rscja.team.qcom.urax.QcomURAxDevice
antLedSwitch(int, boolean) - Method in class com.rscja.team.qcom.urax.RKURA4C8Device
antLedSwitch(int, boolean) - Method in class com.rscja.team.qcom.urax.RKURAxDevice
Auth_ActiveFile(byte, byte[], byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Auth_ActiveFile(byte, byte[], byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Auth_CertificationChain(byte, byte, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Auth_CertificationChain(byte, byte, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Auth_RequestRandom() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Auth_RequestRandom() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Auth_SendData(byte[], byte[], byte[], byte[], byte[], int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Auth_SendData(byte[], byte[], byte[], byte[], byte[], int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Auth_UserInfo(byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Auth_UserInfo(byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
AuthenticateInfo() - Constructor for class com.rscja.custom.M775Authenticate.AuthenticateInfo
authentication(byte, byte, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  验证14443A卡(Authentication 14443A card)
authentication(byte, byte, byte[]) - Method in class com.rscja.team.qcom.r1.hf.HF14443A
  验证14443A卡(Authentication 14443A card)
autoEnroll(int, int) - Method in class com.rscja.deviceapi.Fingerprint
  刷指定次数指纹，模块自动完成注册功能
  Scan fingerprint in specified number, module complete registered function automatically
autoEnroll(int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  刷指定次数指纹，模块自动完成注册功能
  Scan fingerprint in specified number, module complete registered function automatically
autoEnroll(int, int) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  刷指定次数指纹，模块自动完成注册功能
  Scan fingerprint in specified number, module complete registered function automatically
autoInventoryTag(String, int) - Method in class com.rscja.team.qcom.deviceapi.UHFUrxAutoInventoryTagFactory_qcom
autoMatch(int, int, int) - Method in class com.rscja.deviceapi.Fingerprint
  刷指定次数指纹，自动完成比对功能
  Scan fingerprint in specified number, complete comparison function automatically
autoMatch(int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  刷指定次数指纹，自动完成比对功能
  Scan fingerprint in specified number, complete comparison function automatically
autoMatch(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  刷指定次数指纹，自动完成比对功能
  Scan fingerprint in specified number, complete comparison function automatically

A B C D E F G H I J K L M N O P Q R S T U V W X Z