A B C D E F G H I J K L M N O P Q R S T U V W X Z

## U

U - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
UartSwitch(String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UartSwitch(String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHF706_CloseAndDisconnect() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHF706_CloseAndDisconnect() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHF706_OpenAndConnect(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHF706_OpenAndConnect(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFAuthenticate(int, int, int, String) - Method in interface com.rscja.custom.interfaces.IM775Authenticate
UHFAuthenticate() - Method in interface com.rscja.custom.interfaces.IM775Authenticate
UHFAuthenticate(int, int, int, String) - Method in class com.rscja.custom.M775Authenticate
  认证函数(Authentication function)
UHFAuthenticate() - Method in class com.rscja.custom.M775Authenticate
  认证函数(Authentication function)
UHFAuthenticate(int, int, int, String) - Method in class com.rscja.team.mtk.custom.M775Authenticate_mtk
UHFAuthenticate() - Method in class com.rscja.team.mtk.custom.M775Authenticate_mtk
UHFAuthenticate(int, int, int, String) - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
UHFAuthenticate() - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
UHFAuthenticateCommon(int, int, int, byte[], int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFAuthenticateCommon(int, int, int, byte[], int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UhfBase - Class in com.rscja.deviceapi
UhfBase() - Constructor for class com.rscja.deviceapi.UhfBase
UhfBase.ErrorCode - Class in com.rscja.deviceapi
UHFBLEProtocolParse - Class in com.rscja.team.qcom.uhfparse
UHFBLEProtocolParse() - Constructor for class com.rscja.team.qcom.uhfparse.UHFBLEProtocolParse
UHFBlockEraseDataRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBlockEraseDataRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBlockEraseDataSendData(byte[], char, int, int, byte[], char, int, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBlockEraseDataSendData(byte[], char, int, int, byte[], char, int, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.BleDevice
  数据块操作
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  数据块操作
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  数据块操作
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
UHFBlockPermalock(char[], char, char, char, char[], char, char, char, char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
UHFBlockPermalock(char[], char, char, char, char[], char, char, char, char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  数据块操作
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
UHFBlockPermalock_Ex(char[], char, int, int, char[], char, char, int, char, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBlockPermalock_Ex(char[], char, int, int, char[], char, char, int, char, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBlockWriteData(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBlockWriteData(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBlockWriteDataRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBlockWriteDataRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBlockWriteDataSendData(byte[], char, int, int, byte[], char, int, char, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBlockWriteDataSendData(byte[], char, int, int, byte[], char, int, char, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTAuthentication(char[], char, int, int, char[], char, int, int, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTAuthentication(char[], char, int, int, char[], char, int, int, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTDeleteAllTagToFlash() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTDeleteAllTagToFlash() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTDeleteAllTagToFlashRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTDeleteAllTagToFlashRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTDeleteAllTagToFlashSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTDeleteAllTagToFlashSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTEncReadUser(int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTEncReadUser(int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTEncWriteUser(int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTEncWriteUser(int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTEndUpdate() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTEndUpdate() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTEraseData(char[], char, int, char, char[], char, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTEraseData(char[], char, int, char, char[], char, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTFreHopSet(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTFreHopSet(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetAllTagNumFromFlash() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetAllTagNumFromFlash() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetAllTagNumFromFlashRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetAllTagNumFromFlashRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetAllTagNumFromFlashSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetAllTagNumFromFlashSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetBarcode(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetBarcode(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetBattery() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetBattery() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetCW() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetCW() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetGen2(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetGen2(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetPower() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetPower() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetPowerValueRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetPowerValueRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetSendCmd(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetSendCmd(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetTag(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetTag(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetTagDataFromFlash(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetTagDataFromFlash(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetTagDataFromFlashRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetTagDataFromFlashRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTGetTagDataFromFlashSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTGetTagDataFromFlashSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTInventorySingle(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTInventorySingle(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTKeydataMac(byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTKeydataMac(byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTKill(char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTKill(char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTLockMemEx(char[], char, int, int, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTLockMemEx(char[], char, int, int, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTOpen2DRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTOpen2DRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTR2000Temperature(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTR2000Temperature(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTR2000Version(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTR2000Version(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTReadData(char[], char, int, int, char[], char, int, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTReadData(char[], char, int, int, char[], char, int, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTReadEpcTidUserMode(int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTReadEpcTidUserMode(int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTReBootAPP(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTReBootAPP(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetBeep(byte) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetBeep(byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetBeepRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetBeepRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetCW(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetCW(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetEpcTidUserMode(int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetEpcTidUserMode(int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetGen2(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetGen2(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetPower(byte) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetPower(byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetProtocolType(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetProtocolType(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSetR6Workmode(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSetR6Workmode(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTStartInventory() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTStartInventory() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTStartUpdate() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTSTM32Version(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTSTM32Version(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTStopInventory() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTStopInventory() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTUHFGBTagLock(char[], char, int, int, char[], int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTUHFGBTagLock(char[], char, int, int, char[], int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTUHFGetProtocolType() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTUHFGetProtocolType() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTUpdateData(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTUpdateData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFBTWriteData(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFBTWriteData(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFCheckOpMode(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFCheckOpMode(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFCloseAndDisconnect() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFCloseAndDisconnect() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFCSYX - Class in com.rscja.custom
  MQTT是长沙盈芯，定制接口
UHFCSYX.IUHFInventoryCallback - Interface in com.rscja.custom
UHFCSYX.TagAuthenticationResponseInfo - Class in com.rscja.custom
UHFCSYX_A4NetWork - Class in com.rscja.custom
UHFCSYX_A4NetWork() - Constructor for class com.rscja.custom.UHFCSYX_A4NetWork
UHFCSYX_qcom - Class in com.rscja.team.qcom.custom
UHFCSYXForURx - Class in com.rscja.custom
UHFDataHandleBase - Class in com.rscja.team.qcom.uhfhandler
UHFDataHandleBase() - Constructor for class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
UHFDataHandleBase.CMDInfo - Class in com.rscja.team.qcom.uhfhandler
UHFDeactivate(int, char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFDeactivate(int, char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFDecryptSM4(char, char[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFDecryptSM4(char, char[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFDecSM4(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFDecSM4(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFDecUSER(int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFDecUSER(int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFDwell(int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFDwell(int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFEncryptSM4(char, char[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFEncryptSM4(char, char[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFEncSM4(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFEncSM4(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFEncUSER(int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFEncUSER(int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFEraseData(char[], char, int, char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFEraseData(char[], char, int, char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFEraseDataEx(char[], char, int, char, char[], char, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFEraseDataEx(char[], char, int, char, char[], char, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFEraseDataSingle(char[], char, int, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFEraseDataSingle(char[], char, int, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFFlafCrcOff() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFFlafCrcOff() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFFlagCrcOn() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFFlagCrcOn() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFFree(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFFree(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGBTagLock(char[], char, int, int, char[], int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGBTagLock(char[], char, int, int, char[], int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGBTagLockRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGBTagLockRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGBTagLockSendData(byte[], char, int, int, byte[], char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGBTagLockSendData(byte[], char, int, int, byte[], char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetANT() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetANT(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：获取天线设置 输出：buf--2bytes, 共16bits,
UHFGetANTConnectState(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：获取天线设置 输出：buf--2bytes, 共16bits,
UHFGetANTPower(byte[], int[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetANTRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetANTRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetANTSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：获取天线设置 输出：buf--2bytes, 共16bits,
UHFGetANTSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：获取天线设置 输出：buf--2bytes, 共16bits,
UHFGetANTState(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetANTWorkTime(byte, int[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：获取天线工作时间 输入：antnum -- 天线号 输出：WorkTime -- 工作时间 ，单位ms, 范围 10-65535ms 返回：0：获取成功 -1：获取失败
UHFGetANTWorkTime(byte, int[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：获取天线工作时间 输入：antnum -- 天线号 输出：WorkTime -- 工作时间 ，单位ms, 范围 10-65535ms 返回：0：获取成功 -1：获取失败
UHFGetBeep() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetBeep() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetBID() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetBID() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetBTFrequency() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetBTFrequency() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetCalibrationData(char[], char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetCalibrationData(char[], char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetCW() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetCW() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetCWRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetCWRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetCWSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetCWSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetDestIp(byte[], int[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetDestIP(byte[], int[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetEPCTIDMode() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetEPCTIDMode() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetEPCTIDModeRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetEPCTIDModeRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetEPCTIDModeSendData(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetEPCTIDModeSendData(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetEPCTIDUSERAddrLength() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：设置EPC+TID+USER 区地址和长度 输出： char[0] : 状态，0成功 char[1] : 数据长度，5 char[2] 盘点模式： 0x00为盘点EPC； 0x01为盘点EPC+TID； 0x02为EPC+TID+USER char[3] TID地址：盘点TID的起始地址，单位word（2 Byte），模式为0x01时有效 char[4] TID长度：盘点TID的长度，单位word（2 Byte），模式为0x01时有效 char[5] USER地址：盘点USER区的起始地址，单位word（2 Byte），模式为0x02时有效 char[6] USER长度：盘点USER区的长度，单位word（2 Byte），模式为0x02时有效
UHFGetEPCTIDUSERAddrLength() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：设置EPC+TID+USER 区地址和长度 输出： char[0] : 状态，0成功 char[1] : 数据长度，5 char[2] 盘点模式： 0x00为盘点EPC； 0x01为盘点EPC+TID； 0x02为EPC+TID+USER char[3] TID地址：盘点TID的起始地址，单位word（2 Byte），模式为0x01时有效 char[4] TID长度：盘点TID的长度，单位word（2 Byte），模式为0x01时有效 char[5] USER地址：盘点USER区的起始地址，单位word（2 Byte），模式为0x02时有效 char[6] USER长度：盘点USER区的长度，单位word（2 Byte），模式为0x02时有效
UHFGetEPCTIDUSERMode() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetEPCTIDUSERMode() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetFastInventoryMode(int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetFastInventoryMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetFrequency() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetFrequency() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetFrequency_Ex() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetFrequency_Ex() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetGen2RecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetGen2RecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetGen2SendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetGen2SendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetHardwareVersionType() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetHardwareVersionType() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetHwType() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetHwType() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetHwTypeM3() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetHwTypeM3() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetIoControl() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：获取继电器和 IO 控制输出设置状态 返回值：null -- 执行失败 data：2字节，output1: 0:低电平 1：高电平 output2: 0:低电平 1：高电平
UHFGetIoControl(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：获取继电器和 IO 控制输出设置状态 返回值：null -- 执行失败 data：2字节，output1: 0:低电平 1：高电平 output2: 0:低电平 1：高电平
UHFGetIp(byte[], int[], byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetIp(byte[], int[], byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetIpRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetIpRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetIpSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetIpSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetMode() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetMode() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetMultiDataReceived() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetMultiDataReceived() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetOnChipRSSI(char[], char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetOnChipRSSI(char[], char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetOnChipRSSIAndTempCode(char[], char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetOnChipRSSIAndTempCode(char[], char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetParam(char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetParam(char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetPower() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetPower() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetPowerRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetPowerRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetPowerSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetPowerSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetProtocolType() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetProtocolType() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetProtocolTypeRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetProtocolTypeRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetProtocolTypeSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetProtocolTypeSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetPwm() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetPwm() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetReaderBeepRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetReaderBeepRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetReaderBeepSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetReaderBeepSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetReceived() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetReceived() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetReceived_EX() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetReceived_EX() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetReceived_EX2(char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetReceived_EX2(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetReceived_EX_R2000() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetReceived_EX_R2000() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetRegionRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetRegionRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetRegionSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetRegionSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetRFLink() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetRFLink() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetRSSI() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetRSSI() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSensorCode(char[], char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  zjx 20191127 温度标签增加通讯命令 -------- start --------
UHFGetSensorCode(char[], char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  zjx 20191127 温度标签增加通讯命令 -------- start --------
UHFGetSingelMode() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSingelMode() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSleepTimeRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSleepTimeRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSleepTimeSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSleepTimeSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGETSM4(byte[], byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSM4() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGETSM4(byte[], byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSM4() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSoftwareVersionRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSoftwareVersionRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSoftwareVersionSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSoftwareVersionSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSTM32VersionRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSTM32VersionRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetSTM32VersionSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetSTM32VersionSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTagfocusRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTagfocusRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTagfocusSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTagfocusSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTagsDataRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTagsDataRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTagsDataSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTagsDataSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTemperatureRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTemperatureRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTemperatureSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTemperatureSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTempertureCode(char[], char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTempertureCode(char[], char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTempProtectVal() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTempProtectVal() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfGetTempTagReceived() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFJieCe
  获取温度标签的所有信息
uhfGetTempTagReceived() - Method in class com.rscja.custom.RFIDWithUHFJieCe
  获取温度标签的所有信息
UHFGetTempTagReceived(char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
uhfGetTempTagReceived() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
  获取温度标签的所有信息
UHFGetTempTagReceived(char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetTempTagReceived2(char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetTempTagReceived2(char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfGetTempTagReceived_OnChipRSSI_TempeCode() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFJieCe
  获取温度标签数据,不包含calibrationData 、sensorCode的信息
uhfGetTempTagReceived_OnChipRSSI_TempeCode() - Method in class com.rscja.custom.RFIDWithUHFJieCe
  获取温度标签数据,不包含calibrationData 、sensorCode的信息
uhfGetTempTagReceived_OnChipRSSI_TempeCode() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
  获取温度标签数据,不包含calibrationData 、sensorCode的信息
UHFGetTriggerWorkModePara(byte[], int[], int[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetVersion() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetVersion() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFGetWorkMode() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFGetWorkMode() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInit(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInit(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInitRegFile(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInitRegFile(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventory(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventory(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventory_EX(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventory_EX(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventory_EX_BankPtrCnt(char, char, char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventory_EX_BankPtrCnt(char, char, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventory_EX_cnt(char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventory_EX_cnt(char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventoryBank(char[], char, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventoryBank(char[], char, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventoryBID(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventoryBID(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventoryRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventoryRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingle() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingle() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingle_EX() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingle_EX() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingle_R2000() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingle_R2000() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingle_sf() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingle_sf() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingle_tc(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingle_tc(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingleEPCTIDUSER(int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingleEPCTIDUSER(int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingleRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingleRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventorySingleSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventorySingleSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventoryTempTag(char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventoryTempTag(char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventoryTempTag2(char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventoryTempTag2(char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFInventoryTID(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFInventoryTID(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfJump2Boot() - Method in class com.rscja.deviceapi.BleDevice
  uhf进入boot模式 ，开始升级之前需要调用此函数
  UHF enter boot mode, need to call this formula before upgrade
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.BleDevice
uhfJump2Boot() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
uhfJump2Boot(int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
uhfJump2Boot() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  uhf进入boot模式 ，开始升级之前需要调用此函数
  UHF enter boot mode, need to call this formula before upgrade
uhfJump2Boot(int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  uhf进入boot模式 ，开始升级之前需要调用此函数
  UHF enter boot mode, need to call this formula before upgrade
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4NetWork.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4RS232.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8NetWork.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8RS232.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  uhf进入boot模式 ，开始升级之前需要调用此函数
  UHF enter boot mode, need to call this formula before upgrade
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
UHFJump2Boot() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
uhfJump2Boot() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfJump2Boot(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfJump2Boot() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
UHFJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  uhf进入boot模式 ，开始升级之前需要调用此函数
  UHF enter boot mode, need to call this formula before upgrade
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
uhfJump2Boot() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
uhfJump2Boot(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
UHFJump2BootRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFJump2BootRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfJump2BootSendData(char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
UHFJump2BootSendData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFJump2BootSendData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfJump2BootSendData(char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
uhfJump2BootSTM32() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUSB
uhfJump2BootSTM32() - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
uhfJump2BootSTM32() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  升级STM32主板需要调用此函数进入boot模式
  Upgrade STM32 mainboard that need to call this function to enter boot mode.
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  升级STM32主板需要调用此函数进入boot模式
  Upgrade STM32 mainboard that need to call this function to enter boot mode.
UHFJump2BootSTM32() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
uhfJump2BootSTM32() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
UHFJump2BootSTM32() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfJump2BootSTM32() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
  升级STM32主板需要调用此函数进入boot模式
  Upgrade STM32 mainboard that need to call this function to enter boot mode.
uhfJump2BootSTM32() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
uhfJump2BootSTM32() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
uhfJump2BootSTM32() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
uhfJump2BootSTM32() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
uhfJump2BootSTM32() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
  升级STM32主板需要调用此函数进入boot模式
  Upgrade STM32 mainboard that need to call this function to enter boot mode.
uhfJumpToMainboardBoot() - Method in class com.rscja.deviceapi.BleDevice
  升级STM32主板需要调用此函数进入boot模式
  Upgrade STM32 mainboard that need to call this function to enter boot mode.
uhfJumpToMainboardBoot() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
uhfJumpToMainboardBoot() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
UHFKillTag(char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFKillTag(char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFKillTagEx(char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFKillTagEx(char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFKillTagRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFKillTagRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFKillTagSendData(byte[], char, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFKillTagSendData(byte[], char, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFKillTagSingle(char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFKillTagSingle(char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFLedOnOff(String, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFLedOnOff(String, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UhfLocation_qcom - Class in com.rscja.team.qcom.deviceapi
UhfLocation_qcom(Context, IUHF) - Constructor for class com.rscja.team.qcom.deviceapi.UhfLocation_qcom
UHFLockMem(char[], char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFLockMem(char[], char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFLockMemEx(char[], char, int, int, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFLockMemEx(char[], char, int, int, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFLockMemSingle(char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFLockMemSingle(char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFLockTagRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFLockTagRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFLockTagSendData(byte[], char, int, int, byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFLockTagSendData(byte[], char, int, int, byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFOpenAndConnect(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFOpenAndConnect(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFOpenAndConnect_Ex(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFOpenAndConnect_Ex(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfPowerOff_11() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfPowerOn_11() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfProtocolParse - Variable in class com.rscja.team.qcom.socket.SocketManageA4
UHFProtocolParseBase - Class in com.rscja.deviceapi
UHFProtocolParseBase() - Constructor for class com.rscja.deviceapi.UHFProtocolParseBase
UHFProtocolParseBase() - Constructor for class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
UHFProtocolParseBLE - Class in com.rscja.team.qcom.deviceapi
UHFProtocolParseBLE() - Constructor for class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
UHFProtocolParseBleByJava_qcom - Class in com.rscja.team.qcom.deviceapi
UHFProtocolParseByJava - Class in com.rscja.team.qcom.deviceapi
  java 解析R2\R5\R6 uhf协议
UHFProtocolParseByJava() - Constructor for class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
UHFProtocolParseUrA4_qcom - Class in com.rscja.team.qcom.rs232utils
UHFProtocolParseUrA4_qcom() - Constructor for class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
UHFProtocolParseUrA8_qcom - Class in com.rscja.team.qcom.rs232utils
UHFProtocolParseUrA8_qcom() - Constructor for class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA8_qcom
UHFProtocolParseUrAxBase_qcom - Class in com.rscja.team.qcom.rs232utils
UHFProtocolParseUrAxBase_qcom() - Constructor for class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
UHFProtocolParseUrxByJava_qcom - Class in com.rscja.team.qcom.deviceapi
  java 解析UR4 协议
UHFProtocolParseUSBByJava_qcom - Class in com.rscja.team.qcom.deviceapi
  R6、R3 usb通讯特有数据解析
UHFProtocolParseUSBByJava_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.UHFProtocolParseUSBByJava_qcom
UHFProtocolParseUtils_qcom - Class in com.rscja.team.qcom.rs232utils
UHFProtocolParseUtils_qcom() - Constructor for class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom
UHFProtocolParseUtils_qcom.CMDInfo - Class in com.rscja.team.qcom.rs232utils
UHFProtocolProtocolParseBase - Class in com.rscja.team.qcom.uhfparse
UHFProtocolProtocolParseBase() - Constructor for class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
UHFProtocolProtocolParseBase.CMDInfo - Class in com.rscja.team.qcom.uhfparse
UhfRadarLocation_qcom - Class in com.rscja.team.qcom.deviceapi
UhfRadarLocation_qcom(Context, IUHF) - Constructor for class com.rscja.team.qcom.deviceapi.UhfRadarLocation_qcom
UHFReadData(char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadData(char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadData_EX(char[], char, int, char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadData_EX(char[], char, int, char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadData_Ex2(char[], char, int, int, char[], char, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadData_Ex2(char[], char, int, int, char[], char, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadDataRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadDataRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadDataSendData(byte[], char, int, int, byte[], char, int, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadDataSendData(byte[], char, int, int, byte[], char, int, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadDataSingle(char[], char, int, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadDataSingle(char[], char, int, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadMultiTemp(int, int, int, byte[], int, int, int[], int[], float[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadMultiTemp(int, int, int, byte[], int, int, int[], int[], float[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadQTData(char[], char, int, char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadQTData(char[], char, int, char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadQTData_Ex(char[], char, int, int, char[], char, int, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadQTData_Ex(char[], char, int, int, char[], char, int, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadQTDataSingle(char[], char, int, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadQTDataSingle(char[], char, int, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadTagTemp(int, int, int, byte[], float[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadTagTemp(int, int, int, byte[], float[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFReadTagVoltage(int, int, int, byte[], float[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFReadTagVoltage(int, int, int, byte[], float[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFRxBLEDataHandle - Class in com.rscja.team.qcom.uhfhandler
UHFRxBLEDataHandle(IBluetoothReader, KeyEventCallback) - Constructor for class com.rscja.team.qcom.uhfhandler.UHFRxBLEDataHandle
UHFRxUsbDataHandle - Class in com.rscja.team.qcom.uhfhandler
UHFRxUsbDataHandle() - Constructor for class com.rscja.team.qcom.uhfhandler.UHFRxUsbDataHandle
UHFSetANT(int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetANT(byte, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：天线设置 输入：saveflag -- 1:掉电保存， 0：不保存 输入：buf--2bytes, 共16bits, 每bit 置1选择对应天线
UHFSetANT(int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetANT(byte, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：天线设置 输入：saveflag -- 1:掉电保存， 0：不保存 输入：buf--2bytes, 共16bits, 每bit 置1选择对应天线
UHFSetANTPower(int, byte, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetANTRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetANTRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetANTSendData(char, byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：天线设置 输入：saveflag -- 1:掉电保存， 0：不保存 输入：buf--2bytes, 共16bits, 每bit 置1选择对应天线
UHFSetANTSendData(char, byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：天线设置 输入：saveflag -- 1:掉电保存， 0：不保存 输入：buf--2bytes, 共16bits, 每bit 置1选择对应天线
UHFSetANTWorkTime(byte, byte, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：设置天线工作时间 输入：antnum -- 天线号 输入：saveflag -- 1:掉电保存， 0：不保存 输入：WorkTime -- 工作时间 ，单位ms, 范围 10-65535ms 返回：0：设置成功 -1：设置失败
UHFSetANTWorkTime(byte, byte, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：设置天线工作时间 输入：antnum -- 天线号 输入：saveflag -- 1:掉电保存， 0：不保存 输入：WorkTime -- 工作时间 ，单位ms, 范围 10-65535ms 返回：0：设置成功 -1：设置失败
UHFSetBeep(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetBeep(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetBTFrequency(byte) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetBTFrequency(byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetCW(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetCW(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetCWRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetCWRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetCWSendData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetCWSendData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetDestIp(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetDestIp(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetEPCTIDMode(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetEPCTIDMode(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetEPCTIDModeRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetEPCTIDModeRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetEPCTIDModeSendData(char, char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetEPCTIDModeSendData(char, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetEPCTIDUSERAddrLength(char, char, char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：设置EPC+TID+USER 区地址和长度 输入：mode 盘点模式： 0x00为盘点EPC； 0x01为盘点EPC+TID； 0x02为EPC+TID+USER TID_addr TID地址：盘点TID的起始地址，单位word（2 Byte），模式为0x01时有效 TID_length TID长度：盘点TID的长度，单位word（2 Byte），模式为0x01时有效 USER_addr USER地址：盘点USER区的起始地址，单位word（2 Byte），模式为0x02时有效 USER_length USER长度：盘点USER区的长度，单位word（2 Byte），模式为0x02时有效
UHFSetEPCTIDUSERAddrLength(char, char, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：设置EPC+TID+USER 区地址和长度 输入：mode 盘点模式： 0x00为盘点EPC； 0x01为盘点EPC+TID； 0x02为EPC+TID+USER TID_addr TID地址：盘点TID的起始地址，单位word（2 Byte），模式为0x01时有效 TID_length TID长度：盘点TID的长度，单位word（2 Byte），模式为0x01时有效 USER_addr USER地址：盘点USER区的起始地址，单位word（2 Byte），模式为0x02时有效 USER_length USER长度：盘点USER区的长度，单位word（2 Byte），模式为0x02时有效
UHFSetEPCUserMode(char, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetEPCUserMode(char, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFastID(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFastID(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFastInventoryMode(int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFastInventoryMode(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFilter(char, char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFilter(char, char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFilter_Ex(char, char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFilter_Ex(char, char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFilterRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFilterRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFilterSendData(char, char, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFilterSendData(char, char, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFrequency(char, char, char[], char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFrequency(char, char, char[], char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetFrequency_EX(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetFrequency_EX(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetGen2RecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetGen2RecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetGen2SendData(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetGen2SendData(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetInventoryMode(int, int, int, int, int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetInventoryMode(int, int, int, int, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetIOControl(byte, byte, byte) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：继电器和 IO 控制输出设置 输入：output1: 0:低电平 1：高电平 output2: 0:低电平 1：高电平 outStatus： 0：断开 1：闭合 返回值：0：设置成功 -1：设置失败
UHFSetIOControl(byte, byte, byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：继电器和 IO 控制输出设置 输入：output1: 0:低电平 1：高电平 output2: 0:低电平 1：高电平 outStatus： 0：断开 1：闭合 返回值：0：设置成功 -1：设置失败
UHFSetIp(byte[], int, byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetIp(byte[], int, byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetIpRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetIpRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetIpSendData(byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetIpSendData(byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetJumpFrequencyRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetJumpFrequencyRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetJumpFrequencySendData(char, int[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetJumpFrequencySendData(char, int[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetMode(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetMode(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetParam(char, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetParam(char, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetPower(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetPower(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetPowerOnDynamic(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetPowerOnDynamic(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetPowerRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetPowerRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetPowerSendData(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetPowerSendData(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetProtocolType(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetProtocolType(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetProtocolTypeRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetProtocolTypeRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetProtocolTypeSendData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetProtocolTypeSendData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetPwm(int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetPwm(int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetReaderBeepRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetReaderBeepRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetReaderBeepSendData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetReaderBeepSendData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetRegionRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetRegionRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetRegionSendData(char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetRegionSendData(char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetRFLink(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetRFLink(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetSingelMode(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetSingelMode(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetSleepTimeRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetSleepTimeRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetSleepTimeSendData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetSleepTimeSendData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSETSM4(char, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetSM4(char, byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSETSM4(char, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetSM4(char, byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetSoftReset() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  功能：设置软件复位
UHFSetSoftReset() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  功能：设置软件复位
UHFSetSoftResetRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetSoftResetRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetSoftResetSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  20200519 begin
UHFSetSoftResetSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  20200519 begin
UHFSetTagFocus(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetTagFocus(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetTagfocusRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetTagfocusRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetTagfocusSendData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetTagfocusSendData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetTempProtectVal(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetTempProtectVal(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetTriggerWorkModePara(byte, int, int, byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSetWorkMode(byte) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFSetWorkMode(byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFSFForUrxNetwork - Class in com.rscja.custom
UHFSFForUrxNetwork() - Constructor for class com.rscja.custom.UHFSFForUrxNetwork
UHFSFForUrxNetwork.AntInfo - Class in com.rscja.custom
UHFStartLogging(int, int, int, byte[], float, float, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStartLogging(int, int, int, byte[], float, float, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFStartReadDataFromMultiTag(char, char[], char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStartReadDataFromMultiTag(char, char[], char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfStartUpdate() - Method in class com.rscja.deviceapi.BleDevice
  开始升级uhf模块
  Start upgrade UHF module
uhfStartUpdate() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
uhfStartUpdate() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  开始升级uhf模块
  Start upgrade UHF module
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4NetWork.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4RS232.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8NetWork.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8RS232.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  开始升级uhf模块
  Start upgrade UHF module
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
UHFStartUpdate() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
uhfStartUpdate() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfStartUpdate() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
UHFStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  开始升级uhf模块
  Start upgrade UHF module
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
uhfStartUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
UHFStartUpdateRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStartUpdateRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfStartUpdateSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
UHFStartUpdateSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStartUpdateSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfStartUpdateSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
UHFStopGet() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStopGet() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFStopInventoryRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStopInventoryRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFStopInventorySendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStopInventorySendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFStopLogging(int, int, int, byte[], long) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStopLogging(int, int, int, byte[], long) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfStopUpdate() - Method in class com.rscja.deviceapi.BleDevice
  停止升级uhf模块，uhf模块升级完成后需要调用此函数
  Stop upgrade UHF module, call this formula after module has been upgraded.
uhfStopUpdate() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
uhfStopUpdate() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  停止升级uhf模块，uhf模块升级完成后需要调用此函数
  Stop upgrade UHF module, call this formula after module has been upgraded.
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  停止升级uhf模块，uhf模块升级完成后需要调用此函数
  Stop upgrade UHF module, call this formula after module has been upgraded.
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
UHFStopUpdate() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
uhfStopUpdate() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfStopUpdate() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
UHFStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  停止升级uhf模块，uhf模块升级完成后需要调用此函数
  Stop upgrade UHF module, call this formula after module has been upgraded.
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
uhfStopUpdate() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
UHFStopUpdateRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStopUpdateRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFStopUpdateSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
UHFStopUpdateSendData() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFStopUpdateSendData() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFStopUpdateSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
UHFTAGInfo - Class in com.rscja.deviceapi.entity
UHFTAGInfo() - Constructor for class com.rscja.deviceapi.entity.UHFTAGInfo
UHFTAGInfo.ChipInfo - Class in com.rscja.deviceapi.entity
UHFTAGInfo.ChipInfo.Builder - Class in com.rscja.deviceapi.entity
UHFTamperAPI - Class in com.rscja.custom
  阿联酋Acube 定制接口
UHFTamperAPI.TamperInfo - Class in com.rscja.custom
UHFTamperAPI_qcom - Class in com.rscja.team.qcom.custom
UHFTCPTagsDataParseRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFTCPTagsDataParseRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFTemperatureSensors - Class in com.rscja.custom
UHFTemperatureSensors.IUHFInventoryTemperatureTagCallback - Interface in com.rscja.custom
UHFTemperatureSensors.TemperatureTag - Class in com.rscja.custom
UHFTemperatureTag - Class in com.rscja.custom
UHFTemperatureTag.InventoryTemperatureTagCallback - Interface in com.rscja.custom
UHFTemperatureTag.RFIDWithUHFBLEN51 - Class in com.rscja.custom
UHFTemperatureTag.RFIDWithUHFBLEN52 - Class in com.rscja.custom
UHFTemperatureTag.TemperatureTagInfo - Class in com.rscja.custom
UHFTemperatureTagsAPI - Class in com.rscja.custom
UHFTemperatureTagsAPI.IUHFInventoryTempCallback - Interface in com.rscja.custom
UHFTemperatureTagsAPI.MultipleTemperatureInfo - Class in com.rscja.custom
UHFTemperatureTagsAPI.TagState - Enum in com.rscja.custom
  温度标签状态枚举值
UHFTemperatureTagsAPI.TempertureInfo - Class in com.rscja.custom
  温度标签实体对象
UHFTemperatureTagsAPI_mtk - Class in com.rscja.team.mtk.custom
UHFTemperatureTagsAPI_qcom - Class in com.rscja.team.qcom.custom
UHFTemperatureTagsBLEAPI - Class in com.rscja.team.qcom.custom
UHFToBoot(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFToBoot(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFUartFoxconn - Class in com.rscja.custom
UHFUartFoxconn_mtk - Class in com.rscja.team.mtk.custom
UHFUartFoxconn_qcom - Class in com.rscja.team.qcom.custom
UhfUartManage_qcom - Class in com.rscja.team.qcom.rs232utils
UhfUartManage_qcom(String, int) - Constructor for class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
UHFUartTemperatureTag - Class in com.rscja.custom
UHFUartTemperatureTag.InventoryTemperatureTagCallback - Interface in com.rscja.custom
UHFUartTemperatureTag.TemperatureTagInfo - Class in com.rscja.custom
UhfUartUR4Manage_qcom - Class in com.rscja.team.qcom.rs232utils
UhfUartUR4Manage_qcom() - Constructor for class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
UhfUartUR4Manage_qcom.CheckConnectState - Interface in com.rscja.team.qcom.rs232utils
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.BleDevice
  升级uhf模块，发送uhf固件数据
  Upgrade UHF module, send UHF firmware data
uhfUpdating(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
uhfUpdating(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  升级uhf模块，发送uhf固件数据
  Upgrade UHF module, send UHF firmware data
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  升级uhf模块，发送uhf固件数据
  Upgrade UHF module, send UHF firmware data
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
UHFUpdating(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
uhfUpdating(byte[]) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
UHFUpdating(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  升级uhf模块，发送uhf固件数据
  Upgrade UHF module, send UHF firmware data
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
uhfUpdating(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
UHFUpdatingRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFUpdatingRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfUpdatingSendData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
UHFUpdatingSendData(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFUpdatingSendData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
uhfUpdatingSendData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
uhfur4DataHandle - Variable in class com.rscja.team.qcom.socket.SocketManageUR4
UHFUR4DataHandle - Class in com.rscja.team.qcom.uhfhandler
UHFUR4DataHandle() - Constructor for class com.rscja.team.qcom.uhfhandler.UHFUR4DataHandle
UHFUrAxDataHandle - Class in com.rscja.team.qcom.uhfhandler
UHFUrAxDataHandle() - Constructor for class com.rscja.team.qcom.uhfhandler.UHFUrAxDataHandle
UHFUrxAutoInventoryTagFactory_qcom - Class in com.rscja.team.qcom.deviceapi
UHFUrxNetWorkAutoInventoryTag_qcom - Class in com.rscja.team.qcom.deviceapi
UHFUrxNetWorkAutoInventoryTag_qcom(String, int) - Constructor for class com.rscja.team.qcom.deviceapi.UHFUrxNetWorkAutoInventoryTag_qcom
UHFUSBGetTagsDataRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFUSBGetTagsDataRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UhfUtils - Class in com.rscja.utility
UhfUtils() - Constructor for class com.rscja.utility.UhfUtils
UHFVerifyVoltage() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFVerifyVoltage() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
uhfWorkState(boolean) - Method in interface com.rscja.scanner.OnUhfWorkStateListener
  UHF 是否正在盘点
  Working status of UHF
UHFWriteCalibrationData(char[], char, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteCalibrationData(char[], char, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteData(char[], char, int, char, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteData(char[], char, int, char, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteData_Ex2(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteData_Ex2(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteDataRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteDataRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteDataSendData(byte[], char, int, int, byte[], char, int, char, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteDataSendData(byte[], char, int, int, byte[], char, int, char, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteDataSingle(char[], char, int, char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteDataSingle(char[], char, int, char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteQTData(char[], char, int, char, char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteQTData(char[], char, int, char, char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteQTData_Ex(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteQTData_Ex(char[], char, int, int, char[], char, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteQTDataSingle(char[], char, int, char, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteQTDataSingle(char[], char, int, char, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFWriteScreenBlock(byte[], byte, int, int, byte[], byte, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHFWriteScreenBlock(byte[], byte, int, int, byte[], byte, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHFXSAPI - Class in com.rscja.custom
UHFXSAPI.Bank - Enum in com.rscja.custom
UHTSetR6WorkmodeRecvData(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHTSetR6WorkmodeRecvData(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UHTSetR6WorkmodeSendData(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UHTSetR6WorkmodeSendData(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Um7ProtocolConfig(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Um7ProtocolConfig(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UNKNOWN - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
unregisterReceiver() - Method in class com.rscja.team.mtk.utility.BatteryManage
unvarnished_transfer(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
unvarnished_transfer(byte[]) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
unvarnished_transfer(byte[]) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
unvarnished_transfer(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
upChar(Fingerprint.BufferEnum) - Method in class com.rscja.deviceapi.Fingerprint
  上传指定缓冲区中的指纹特征数据
  Upload fingerprint feature data of specified buffer zone
upChar(FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  将暂存在RamBuffer中的指纹模板上传到主机
upChar(Fingerprint.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  上传指定缓冲区中的指纹特征数据
  Upload fingerprint feature data of specified buffer zone
upChar(FingerprintWithZAZ.BufferEnum, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  将暂存在RamBuffer中的指纹模板上传到主机
upChar(Fingerprint.BufferEnum) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  上传指定缓冲区中的指纹特征数据
  Upload fingerprint feature data of specified buffer zone
upChar(FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  将暂存在RamBuffer中的指纹模板上传到主机
update(Observable, Object) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
update(ConnectionStatus) - Method in class com.rscja.team.qcom.socket.SocketManageA4
update(ConnectionStatus) - Method in class com.rscja.team.qcom.socket.SocketManageUR4
Update_ReadInfo() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Update_ReadInfo() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UPDATE_STM32 - Static variable in interface com.rscja.deviceapi.interfaces.IReader
UPDATE_UHF - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
Upgrade(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPSAM
  固件升级
  Firmware upgrade
Upgrade(int, int, int, byte[]) - Method in class com.rscja.deviceapi.PSAM
  固件升级
  Firmware upgrade
Upgrade(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.PSAM_mtk
  固件升级
  Firmware upgrade
Upgrade(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.PSAM_qcom
  固件升级
  Firmware upgrade
upgradeFont(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
upgradeFont(int, int, int, byte[]) - Method in class com.rscja.deviceapi.Printer
upgradeFont(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
upgradeFW(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
upgradeFW(int, int, int, byte[]) - Method in class com.rscja.deviceapi.Printer
upgradeFW(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
upImage(int, String) - Method in class com.rscja.deviceapi.Fingerprint
  上传指纹图像文件
  Upload finerprint image file
upImage(int, String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  上传指纹图像文件
  Upload finerprint image file
upImage(int, String) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  上传指纹图像文件
  Upload finerprint image file
upImageData(int, String, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  上传指纹图像到外部文件
upImageData(int, String, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  上传指纹图像到外部文件
upImageData(int, String, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  上传指纹图像到外部文件
upImageISO(int, String) - Method in class com.rscja.deviceapi.Fingerprint
  上传指纹ISO图像文件
  Upload fingerprint ISO image file
upImageISO(int, String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  上传指纹ISO图像文件
  Upload fingerprint ISO image file
upImageISO(int, String) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  上传指纹ISO图像文件
  Upload fingerprint ISO image file
UrxUsb_qcom - Class in com.rscja.team.qcom.usb
UrxUsb_qcom(UsbBase_qcom) - Constructor for class com.rscja.team.qcom.usb.UrxUsb_qcom
UsbBase_qcom - Class in com.rscja.team.qcom.usb
UsbBase_qcom() - Constructor for class com.rscja.team.qcom.usb.UsbBase_qcom
UsbBase_qcom.DataCallback - Interface in com.rscja.team.qcom.usb
UsbFingerprint - Class in com.rscja.deviceapi
UsbFingerprint_mtk - Class in com.rscja.team.mtk.deviceapi
UsbFingerprint_qcom - Class in com.rscja.team.qcom.deviceapi
UsbPL2302 - Class in com.rscja.team.qcom.usb.pl2302
  Created by xxj on 01/15.
UsbPL2302() - Constructor for class com.rscja.team.qcom.usb.pl2302.UsbPL2302
UsbSerialPort_qcom - Interface in com.rscja.team.qcom.usb.pl2302
UsbSerialPortImpl_qcom - Class in com.rscja.team.qcom.usb.pl2302
UsbSerialPortImpl_qcom(UsbDeviceConnection) - Constructor for class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
UsbToFingerprint() - Method in interface com.rscja.deviceapi.interfaces.IUsbFingerprint
UsbToFingerprint() - Method in class com.rscja.deviceapi.UsbFingerprint
UsbToFingerprint(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UsbToFingerprint() - Method in class com.rscja.team.mtk.deviceapi.UsbFingerprint_mtk
UsbToFingerprint(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UsbToFingerprint() - Method in class com.rscja.team.qcom.deviceapi.UsbFingerprint_qcom
UsbToHost() - Method in interface com.rscja.deviceapi.interfaces.IUsbFingerprint
UsbToHost() - Method in class com.rscja.deviceapi.UsbFingerprint
UsbToHost(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
UsbToHost() - Method in class com.rscja.team.mtk.deviceapi.UsbFingerprint_mtk
UsbToHost(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
UsbToHost() - Method in class com.rscja.team.qcom.deviceapi.UsbFingerprint_qcom

A B C D E F G H I J K L M N O P Q R S T U V W X Z