A B C D E F G H I J K L M N O P Q R S T U V W X Z

## O

off() - Method in class com.rscja.scanner.led.ScanLed
  关闭LED灯
  Switch off LED light
off(Context) - Method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  关闭LED灯
  Switch off LED light
off() - Method in class com.rscja.team.mtk.scanner.led.C6000_6762_ScanLed_mtk
off() - Method in class com.rscja.team.mtk.scanner.led.C7X_6765_ScanLed_mtk
off() - Method in class com.rscja.team.mtk.scanner.led.C90_6762_ScanLed_mtk
off() - Method in class com.rscja.team.mtk.scanner.led.ScanLed_mtk
  关闭LED灯
  Switch off LED light
off(Context) - Method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  关闭LED灯
  Switch off LED light
off() - Method in class com.rscja.team.qcom.scanner.led.C60_6765_11_ScanLed_qcom
off() - Method in class com.rscja.team.qcom.scanner.led.C60_qcm2150_10_ScanLed_qcom
off() - Method in class com.rscja.team.qcom.scanner.led.C61_smd450_90_ScanLed_qcom
off() - Method in class com.rscja.team.qcom.scanner.led.C66_smd450_90_ScanLed_qcom
off() - Method in class com.rscja.team.qcom.scanner.led.C66m_sm6115_10_ScanLed_qcom
off() - Method in class com.rscja.team.qcom.scanner.led.MC50_4350_12_ScanLed_qcom
off() - Method in class com.rscja.team.qcom.scanner.led.P80_8786_130_ScanLed_qcom
off() - Method in class com.rscja.team.qcom.scanner.led.P80_8953_90_ScanLed_qcom
on() - Method in class com.rscja.scanner.led.ScanLed
  打开LED灯
  Switch on LED light
On(Context) - Method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  打开LED灯
  Switch on LED light
on() - Method in class com.rscja.team.mtk.scanner.led.C6000_6762_ScanLed_mtk
on() - Method in class com.rscja.team.mtk.scanner.led.C7X_6765_ScanLed_mtk
on() - Method in class com.rscja.team.mtk.scanner.led.C90_6762_ScanLed_mtk
on() - Method in class com.rscja.team.mtk.scanner.led.ScanLed_mtk
  打开LED灯
  Switch on LED light
On(Context) - Method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  打开LED灯
  Switch on LED light
on() - Method in class com.rscja.team.qcom.scanner.led.C60_6765_11_ScanLed_qcom
on() - Method in class com.rscja.team.qcom.scanner.led.C60_qcm2150_10_ScanLed_qcom
on() - Method in class com.rscja.team.qcom.scanner.led.C61_smd450_90_ScanLed_qcom
on() - Method in class com.rscja.team.qcom.scanner.led.C66_smd450_90_ScanLed_qcom
on() - Method in class com.rscja.team.qcom.scanner.led.C66m_sm6115_10_ScanLed_qcom
on() - Method in class com.rscja.team.qcom.scanner.led.MC50_4350_12_ScanLed_qcom
on() - Method in class com.rscja.team.qcom.scanner.led.P80_8786_130_ScanLed_qcom
on() - Method in class com.rscja.team.qcom.scanner.led.P80_8953_90_ScanLed_qcom
onAccuracyChanged(Sensor, int) - Method in class com.rscja.team.qcom.deviceapi.UhfRadarLocation_qcom
onBarcodeImage(byte[]) - Method in interface com.rscja.barcode.BarcodeDecoder.IBarcodeImageCallback
onComplete(boolean, byte[], int, int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.EnrollCallBack
  获取完指纹之后被回调
  call-back after fingerprint acquired
onComplete(boolean, byte[], int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.GRABCallBack
  获取完图像之后被回调
  call-back after acquiring image
onComplete(boolean, int, int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.IdentificationCallBack
onComplete(boolean, byte[], int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.PtCaptureCallBack
  获取完指纹模版数据之后被回调
  call-back after fingerprint template data acquired
onComplete(boolean, int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.TemplateVerifyCallBack
onComplete(boolean, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.EnrollCallBack
  获取完指纹之后被回调
  call-back after fingerprint acquired
onComplete(boolean, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.GrabCallBack
onComplete(boolean, int, String, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.IdentificationCallBack
onComplete(boolean, byte[], int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.PtCaptureCallBack
  获取完指纹模版数据之后被回调
  call-back after fingerprint
onComplete(boolean, int) - Method in interface com.rscja.deviceapi.FingerprintWithMorpho.TemplateVerifyCallBack
onComplete(boolean, byte[], int) - Method in interface com.rscja.deviceapi.FingerprintWithTLK1NC.IUPImageCallback
  获取完图像之后被回调
  call-back after acquiring image
onDecodeComplete(BarcodeEntity) - Method in interface com.rscja.barcode.BarcodeDecoder.DecodeCallback
onDecodeComplete(BarcodeResult) - Method in interface com.rscja.deviceapi.BluetoothReader.DecodeCallback
onDecodeComplete(BarcodeEntity) - Method in interface com.rscja.team.mtk.barcode.BarcodeDecoder_mtk.DecodeCallback
onKeyDown(int) - Method in interface com.rscja.deviceapi.interfaces.KeyEventCallback
onKeyUp(int) - Method in interface com.rscja.deviceapi.interfaces.KeyEventCallback
OnLowBattery(BatteryEntity) - Method in interface com.rscja.deviceapi.interfaces.OnLowBatteryListener
OnLowBatteryListener - Interface in com.rscja.deviceapi.interfaces
onPictureTaken(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IBarcodePictureCallback
onReceive(Context, Intent) - Method in class com.rscja.team.qcom.service.BLEService_qcom.BluetoothStateReceiver
onSensorChanged(SensorEvent) - Method in class com.rscja.team.qcom.deviceapi.UhfRadarLocation_qcom
onStatusChanged(ConnectionStatus) - Method in interface com.rscja.deviceapi.interfaces.IConnectionStatusChangedListener
OnUhfWorkStateListener - Interface in com.rscja.scanner
  uhf 工作状态发生变化时回调的接口定义. Interface definition for a callback to be invoked when UHF working state changes.
onVideoFrame(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeVideoCallback
open(Context) - Method in class com.rscja.barcode.BarcodeDecoder
  打开二维扫描设备
  Switch on 2D scanning device
open(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.barcode.BarcodeUtility
  打开指定功能 Switch on designated function
open(Context) - Method in class com.rscja.deviceapi.Barcode1D
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.deviceapi.Barcode1D
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.deviceapi.Barcode2D
  打开二维扫描设备
  Switch on 1D scanning device.
open(Context) - Method in class com.rscja.deviceapi.Barcode2D
  打开二维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.deviceapi.Infrared
  打开红外模块,默认1200波特率
  Switch on infared module, default 1200 baud rate
open(int) - Method in class com.rscja.deviceapi.Infrared
  打开红外模块
  Switch on infared module
open(int, int) - Method in class com.rscja.deviceapi.Infrared
  打开红外模块
  Switch on infared module
open(int, int, int, int) - Method in class com.rscja.deviceapi.Infrared
  打开红外模块
  Switch on infared module
open(Context) - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  打开二维扫描设备
  Switch on 1D scanning device.
open(Context) - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  打开二维扫描设备
  Switch on 1D scanning device.
open(Context, BarcodeUtility.ModuleType) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  打开指定功能 Switch on designated function
open() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  打开红外模块,默认1200波特率
  Switch on infared module, default 1200 baud rate
open(int) - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  打开红外模块
  Switch on infared module
open(int, int) - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  打开红外模块
  Switch on infared module
open(int, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  打开红外模块
  Switch on infared module
open() - Method in interface com.rscja.deviceapi.interfaces.ILedLight
  打开LED灯
  Switch on LED
open() - Method in class com.rscja.deviceapi.LedLight
  打开LED灯
  Switch on LED
open(Context) - Method in interface com.rscja.scanner.IScanner
  打开键盘助手总开关
  Switch on keyboardemulator
open(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
open(Context) - Method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
open(Context) - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  打开二维扫描设备
  Switch on 2D scanning device
open(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  打开指定功能 Switch on designated function
open(Context) - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  打开二维扫描设备
  Switch on 1D scanning device.
open(Context) - Method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  打开二维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  打开红外模块,默认1200波特率
  Switch on infared module, default 1200 baud rate
open(int) - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  打开红外模块
  Switch on infared module
open(int, int) - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  打开红外模块
  Switch on infared module
open(int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  打开红外模块
  Switch on infared module
open() - Method in class com.rscja.team.mtk.deviceapi.LedLight_mtk
  打开LED灯
  Switch on LED
open(Context) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
open(Context) - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
open(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  打开指定功能 Switch on designated function
open(Context) - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  打开一维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  打开二维扫描设备
  Switch on 1D scanning device.
open(Context) - Method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  打开二维扫描设备
  Switch on 1D scanning device.
open() - Method in class com.rscja.team.qcom.deviceapi.LedLight_qcom
  打开LED灯
  Switch on LED
open() - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
open() - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
open(Context) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
open(UsbDeviceConnection) - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Opens and initializes the port.
open(UsbDeviceConnection) - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
openAuxiliaryLight(Context) - Method in interface com.rscja.deviceapi.interfaces.IScanerLedLight
  打开扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
openAuxiliaryLight(Context) - Method in class com.rscja.deviceapi.ScanerLedLight
openAuxiliaryLight(Context) - Method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  打开扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
openAuxiliaryLight(Context) - Method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  打开扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
openBuzzer() - Method in interface com.rscja.team.qcom.urax.IURAxDevice
openBuzzer() - Method in class com.rscja.team.qcom.urax.QcomURAxDevice
openBuzzer() - Method in class com.rscja.team.qcom.urax.RKURA4C8Device
openBuzzer() - Method in class com.rscja.team.qcom.urax.RKURAxDevice
openKeyboardHelper(Context) - Method in class com.rscja.barcode.BarcodeUtility
  打开键盘助手功能总开关 Switch on main function switch of keyboardemulator
openKeyboardHelper(Context) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  打开键盘助手功能总开关 Switch on main function switch of keyboardemulator
openKeyboardHelper(Context) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  打开键盘助手功能总开关 Switch on main function switch of keyboardemulator
openKeyboardHelper(Context) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  打开键盘助手功能总开关 Switch on main function switch of keyboardemulator
openLed() - Method in class com.rscja.deviceapi.BluetoothReader
  打开led
openLED() - Method in class com.rscja.deviceapi.Infrared
  打开辅助灯
  Open LED
openLED() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  打开辅助灯
  Open LED
openLed() - Method in interface com.rscja.deviceapi.interfaces.IReader
  打开led
openLed() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  打开led
openLED() - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  打开辅助灯
  Open LED
openLed() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
openLed() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
  打开led
openLed() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
  打开led
openLedSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
openLedSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
openPort(UsbDevice) - Method in class com.rscja.team.qcom.usb.pl2302.UsbPL2302
openPort(UsbDevice) - Method in class com.rscja.team.qcom.usb.RxUsb_qcom
openPort(UsbDevice) - Method in class com.rscja.team.qcom.usb.UrxUsb_qcom
openPort(UsbDevice) - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
openPrinterSerialPort(boolean) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
openPrinterSerialPort(boolean) - Method in class com.rscja.deviceapi.Printer
openPrinterSerialPort(boolean) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
openScanLed() - Method in interface com.rscja.team.qcom.urax.IURAxDevice
openScanLed() - Method in class com.rscja.team.qcom.urax.QcomURAxDevice
openScanLed() - Method in class com.rscja.team.qcom.urax.RKURA4C8Device
openScanLed() - Method in class com.rscja.team.qcom.urax.RKURAxDevice
openSerail(String, int, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  打开串口
openSerail(String, int, int, int, int) - Method in class com.rscja.deviceapi.Module
  打开串口
OpenSerail(String, int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
openSerail(String, int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  打开串口
OpenSerail(String, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
openSerail(String, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  打开串口
openSerail(String, int) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
openSerail(String, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  打开串口
openSerialPort(String, int) - Method in class com.rscja.team.qcom.serialportapi.SerialportAPI
openUhfSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
openWifi() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
openWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  打开wifi
openWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  打开wifi
openWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  打开wifi
openWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  打开wifi
openWifiSendData(boolean) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
openWorkLed() - Method in interface com.rscja.team.qcom.urax.IURAxDevice
openWorkLed() - Method in class com.rscja.team.qcom.urax.QcomURAxDevice
openWorkLed() - Method in class com.rscja.team.qcom.urax.RKURA4C8Device
openWorkLed() - Method in class com.rscja.team.qcom.urax.RKURAxDevice
OTG_GPIO_OFF(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
OTG_GPIO_OFF(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
OTG_GPIO_ON(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
OTG_GPIO_ON(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
output1Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio 3 off
output1Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio 3 off
output1Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output1Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  gpio 3 off
output1Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio 3 off
output1Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output1Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio 3 off
output1Off() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output1Off() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output1Off() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
output1On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio 3 on
output1On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio 3 on
output1On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output1On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  gpio 3 on
output1On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio 3 on
output1On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output1On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio 3 on
output1On() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output1On() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output1On() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
output2Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio 4 off
output2Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio 4 off
output2Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output2Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  gpio 4 off
output2Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio 4 off
output2Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output2Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio 4 off
output2Off() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output2Off() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output2Off() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
output2On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio 4 on
output2On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio 4 on
output2On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output2On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  gpio 4 on
output2On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio 4 on
output2On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output2On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio 4 on
output2On() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output2On() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output2On() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
output3Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio OptoCoupler3 off
output3Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8
output3Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio OptoCoupler3 off
output3Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output3Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
output3Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
output3Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
output3Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
output3Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio OptoCoupler3 off
output3Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output3Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio OptoCoupler3 off
output3Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
output3Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
output3Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
  gpio OptoCoupler3 off
output3Off() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output3Off() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output3Off() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
output3On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio OptoCoupler3 on
output3On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8
output3On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio OptoCoupler3 on
output3On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output3On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
output3On() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
output3On() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
output3On() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
output3On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio OptoCoupler3 on
output3On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output3On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio OptoCoupler3 on
output3On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
output3On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
output3On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
  gpio OptoCoupler3 on
output3On() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output3On() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output3On() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
output4Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio OptoCoupler4 off
output4Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8
output4Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio OptoCoupler4 off
output4Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output4Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
output4Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
output4Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
output4Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
output4Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio OptoCoupler4 off
output4Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output4Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio OptoCoupler4 off
output4Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
output4Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
output4Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
  gpio OptoCoupler4 off
output4Off() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output4Off() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output4Off() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
output4On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio OptoCoupler4 on
output4On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8
output4On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio OptoCoupler4 on
output4On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
output4On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
output4On() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
output4On() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
output4On() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
output4On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio OptoCoupler4 on
output4On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
output4On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio OptoCoupler4 on
output4On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
output4On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
output4On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
  gpio OptoCoupler4 on
output4On() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
output4On() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
output4On() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
outputOnAndOff(List<GPOEntity>) - Method in interface com.rscja.deviceapi.interfaces.IUHFA4
outputOnAndOff(List<GPOEntity>) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  控制全部GPO输出
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  控制全部GPO输出
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  控制全部GPO输出
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  控制全部GPO输出
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
outputOnAndOff(List<GPOEntity>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
outputOnAndOffSendData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
outputWgData0Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio WgData0 off
outputWgData0Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio WgData0 off
outputWgData0Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
outputWgData0Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
outputWgData0Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio WgData0 off
outputWgData0Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
outputWgData0Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio WgData0 off
outputWgData0Off() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
outputWgData0Off() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
outputWgData0Off() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
outputWgData0On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio WgData0 on
outputWgData0On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio WgData0 on
outputWgData0On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
outputWgData0On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
outputWgData0On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio WgData0 on
outputWgData0On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
outputWgData0On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio WgData0 on
outputWgData0On() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
outputWgData0On() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
outputWgData0On() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
outputWgData1Off() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio WgData1 off
outputWgData1Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio WgData1 off
outputWgData1Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
outputWgData1Off() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
outputWgData1Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio WgData1 off
outputWgData1Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
outputWgData1Off() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio WgData1 off
outputWgData1Off() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
outputWgData1Off() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
outputWgData1Off() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio
outputWgData1On() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  gpio WgData1 on
outputWgData1On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  gpio WgData1 on
outputWgData1On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
outputWgData1On() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
outputWgData1On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  gpio WgData1 on
outputWgData1On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
outputWgData1On() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  gpio WgData1 on
outputWgData1On() - Method in interface com.rscja.team.qcom.urax.IURA4Gpio
outputWgData1On() - Method in class com.rscja.team.qcom.urax.QcomURA4Gpio
outputWgData1On() - Method in class com.rscja.team.qcom.urax.RKURA4Gpio

A B C D E F G H I J K L M N O P Q R S T U V W X Z