## Uses of Interface
com.rscja.custom.interfaces.IM775Authenticate

- Packages that use IM775Authenticate
  Package | Description
  --- | ---
  com.rscja.custom |
  com.rscja.team.mtk.custom |
  com.rscja.team.qcom.custom |

- - ### Uses of IM775Authenticate in com.rscja.custom

    Classes in com.rscja.custom that implement IM775Authenticate
    Modifier and Type | Class and Description
    --- | ---
    `class` | `M775Authenticate` 英频杰特殊标签定制 Special label customization 第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 盘点标签之前先要设置回调函数`M775Authenticate.setInventoryCallback(IUHFInventoryCallback)`,然后调用盘点函数`RFIDWithUHFUART.startInventoryTag()`开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。 For parameter setting, after the connection is successful, call the corresponding function to set parameters and read/write operations.

  - ### Uses of IM775Authenticate in com.rscja.team.mtk.custom

    Classes in com.rscja.team.mtk.custom that implement IM775Authenticate
    Modifier and Type | Class and Description
    --- | ---
    `class` | `M775Authenticate_mtk`

  - ### Uses of IM775Authenticate in com.rscja.team.qcom.custom

    Classes in com.rscja.team.qcom.custom that implement IM775Authenticate
    Modifier and Type | Class and Description
    --- | ---
    `class` | `M775Authenticate_qcom`