com.rscja.team.qcom.deviceapi

## Class RFIDWithISO14443B_qcom

- java.lang.Object
- - com.rscja.team.qcom.deviceapi.Device_qcom
  - - com.rscja.team.qcom.deviceapi.RFIDBase_qcom
    - - com.rscja.team.qcom.deviceapi.RFIDWithISO14443B_qcom

- All Implemented Interfaces:
    IRFIDBase, IRFIDWithISO14443B

      public class RFIDWithISO14443B_qcom
      extends RFIDBase_qcom
      implements IRFIDWithISO14443B

  RFID模块ISO14443B协议操作类
  RFID module ISO14443B protocol operation type

  注意：
  Attention:
  1、使用前请确认您的机器已安装此模块。
  1. Make sure this module is installed before using.
  2、要正常使用模块需要在\libs\armeabi\目录放置libDeviceAPI.so文件
  2. Put libDeviceAPI.so file in directoy \libs\armeabi\ then module can be used normally.
  3、在操作设备前需要调用 `RFIDBase_qcom.init()` 打开设备，使用完后调用 `RFIDBase_qcom.free()` 关闭设备
  3. call `RFIDBase_qcom.init()` to switch on the device before operating, call `RFIDBase_qcom.free()` to switch off the device after using.

  Author:
    liuruifeng

- - ### Method Summary

    All Methods Static Methods Instance Methods Concrete Methods
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithISO14443B_qcom` | `getInstance()` 获取ISO14443B协议操作实例 Acquire ISO14443B protocol operation Instance
    `java.lang.String` | `getUID()` 获取卡片ID Acquire card ID
    `byte[]` | `getUIDBytes()` 获取卡片ID Acquire card ID
    `java.lang.String` | `reset()` CPU卡复位操作指令 CPU card reset operation commande
    `java.lang.String` | `sendCommand(java.lang.String cmd)` CPU卡 T=CL发送COS指令 CPU card T=CL send COS command

    - ### Methods inherited from class com.rscja.team.qcom.deviceapi.RFIDBase_qcom

      `free, getVersion, init, init, rfidUpgrade`

    - ### Methods inherited from class com.rscja.team.qcom.deviceapi.Device_qcom

      `isPowerOn`

    - ### Methods inherited from class java.lang.Object

      `equals, getClass, hashCode, notify, notifyAll, toString, wait, wait, wait`

    - ### Methods inherited from interface com.rscja.deviceapi.interfaces.IRFIDBase

      `free, getVersion, init, init, isPowerOn, rfidUpgrade`

- - ### Method Detail

    - #### getInstance

          public static RFIDWithISO14443B_qcom getInstance()
                                                    throws ConfigurationException

      获取ISO14443B协议操作实例
      Acquire ISO14443B protocol operation Instance
      Returns:
        ISO14443B协议操作实例
        ISO14443B protocol operation Instance
      Throws:
        `ConfigurationException` - 配置错误异常
        Configuration err.

    - #### getUID

          public java.lang.String getUID()

      获取卡片ID
      Acquire card ID
      Specified by:
        `getUID` in interface `IRFIDWithISO14443B`
      Returns:
        失败返回null
        failure return null

    - #### getUIDBytes

          public byte[] getUIDBytes()

      获取卡片ID
      Acquire card ID
      Specified by:
        `getUIDBytes` in interface `IRFIDWithISO14443B`
      Returns:
        失败返回null
        failure return null

    - #### sendCommand

          public java.lang.String sendCommand(java.lang.String cmd)

      CPU卡 T=CL发送COS指令
      CPU card T=CL send COS command
      Specified by:
        `sendCommand` in interface `IRFIDWithISO14443B`
      Parameters:
        `cmd` - COS指令内容
        COS command content
      Returns:
        CPU卡返回的COS指令内容
        CPU card return COS command

    - #### reset

          public java.lang.String reset()

      CPU卡复位操作指令
      CPU card reset operation commande
      Specified by:
        `reset` in interface `IRFIDWithISO14443B`
      Returns:
        CPU卡返回的reset操作数据
        CPU card return reset operation data