## Uses of Class
com.rscja.deviceapi.entity.ReaderIPEntity

- Packages that use ReaderIPEntity
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.entity |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.qcom.deviceapi |
  com.rscja.team.qcom.rs232utils |

- - ### Uses of ReaderIPEntity in com.rscja.deviceapi

    Methods in com.rscja.deviceapi that return ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `ReaderIPEntity` | RFIDWithUHFUrxUart.`getDestIP()` 获取目标IP
    `ReaderIPEntity` | RFIDWithUHFUrxUsbToUart.`getDestIP()`
    `ReaderIPEntity` | RFIDWithUHFUrxNetwork.`getDestIP()`
    `ReaderIPEntity` | RFIDWithUHFA8NetWork.`getReaderCurrentIp()` 获取设备当前的IP地址
    `ReaderIPEntity` | RFIDWithUHFA4NetWork.`getReaderCurrentIp()` 获取设备当前的IP地址
    `ReaderIPEntity` | RFIDWithUHFA4RS232.`getReaderCurrentIp()` 获取设备当前的IP地址
    `ReaderIPEntity` | RFIDWithUHFA8RS232.`getReaderCurrentIp()` 获取设备当前的IP地址
    `ReaderIPEntity` | RFIDWithUHFUrxUart.`getUhfReaderIP()` 获取UHF读写器IP
    `ReaderIPEntity` | RFIDWithUHFUrxUsbToUart.`getUhfReaderIP()`
    `ReaderIPEntity` | RFIDWithUHFUrxNetwork.`getUhfReaderIP()`

    Methods in com.rscja.deviceapi with parameters of type ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFUrxUart.`setDestIP(ReaderIPEntity readerIPEntity)` 设置目标IP
    `boolean` | RFIDWithUHFUrxUsbToUart.`setDestIP(ReaderIPEntity readerIPEntity)`
    `boolean` | RFIDWithUHFUrxNetwork.`setDestIP(ReaderIPEntity readerIPEntity)`
    `boolean` | RFIDWithUHFA8NetWork.`setEthernetConfigInfo(ReaderIPEntity ipconfig)` 设置以太网IP地址
    `boolean` | RFIDWithUHFA4NetWork.`setEthernetConfigInfo(ReaderIPEntity ipconfig)` 设置以太网IP地址
    `boolean` | RFIDWithUHFA4RS232.`setEthernetConfigInfo(ReaderIPEntity ipconfig)` 设置以太网IP地址
    `boolean` | RFIDWithUHFA8RS232.`setEthernetConfigInfo(ReaderIPEntity ipconfig)` 设置以太网IP地址
    `boolean` | RFIDWithUHFUrxUart.`setUhfReaderIP(ReaderIPEntity readerIPEntity)` 设置UHF读写器IP
    `boolean` | RFIDWithUHFUrxUsbToUart.`setUhfReaderIP(ReaderIPEntity readerIPEntity)`
    `boolean` | RFIDWithUHFUrxNetwork.`setUhfReaderIP(ReaderIPEntity readerIPEntity)`

  - ### Uses of ReaderIPEntity in com.rscja.deviceapi.entity

    Methods in com.rscja.deviceapi.entity that return ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `ReaderIPEntity` | WifiConfig.`getStaticIpConfig()`

    Methods in com.rscja.deviceapi.entity with parameters of type ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `void` | WifiConfig.`setStaticIpConfig(ReaderIPEntity staticIpconfig)`

  - ### Uses of ReaderIPEntity in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces that return ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `ReaderIPEntity` | IUHFURx.`getDestIP()` 获取目标IP
    `ReaderIPEntity` | IUHFURAxExtend.`getReaderCurrentIp()`
    `ReaderIPEntity` | IUHFURx.`getUhfReaderIP()` 获取UHF读写器IP
    `ReaderIPEntity` | IUHFProtocolParseUrx.`parseGetReaderDestIpData(byte[] inData)`
    `ReaderIPEntity` | IUHFProtocolParseUrx.`parseGetReaderIpData(byte[] inData)`

    Methods in com.rscja.deviceapi.interfaces with parameters of type ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | IUHFURx.`setDestIP(ReaderIPEntity readerIPEntity)` 设置目标IP
    `boolean` | IUHFURAxExtend.`setEthernetConfigInfo(ReaderIPEntity ipconfig)`
    `byte[]` | IUHFProtocolParseUrx.`setReaderDestIpSendData(ReaderIPEntity uhfconfig)`
    `byte[]` | IUHFProtocolParseUrx.`setReaderIpSendData(ReaderIPEntity uhfconfig)`
    `boolean` | IUHFURx.`setUhfReaderIP(ReaderIPEntity readerIPEntity)` 设置UHF读写器IP

  - ### Uses of ReaderIPEntity in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi that return ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `ReaderIPEntity` | RFIDWithUHFUrxUsbToUart_qcom.`getDestIP()`
    `ReaderIPEntity` | RFIDWithUHFUrxUart_qcom.`getDestIP()` 获取目标IP
    `ReaderIPEntity` | RFIDWithUHFUrxUart2_qcom.`getDestIP()`
    `ReaderIPEntity` | RFIDWithUHFUrxNetwork_qcom.`getDestIP()`
    `ReaderIPEntity` | RFIDWithUHFUrxUsbToUart_qcom.`getUhfReaderIP()`
    `ReaderIPEntity` | RFIDWithUHFUrxUart_qcom.`getUhfReaderIP()` 获取UHF读写器IP
    `ReaderIPEntity` | RFIDWithUHFUrxUart2_qcom.`getUhfReaderIP()`
    `ReaderIPEntity` | RFIDWithUHFUrxNetwork_qcom.`getUhfReaderIP()`
    `ReaderIPEntity` | UHFProtocolParseUrxByJava_qcom.`parseGetReaderDestIpData(byte[] inData)`
    `ReaderIPEntity` | UHFProtocolParseUrxByJava_qcom.`parseGetReaderIpData(byte[] inData)`

    Methods in com.rscja.team.qcom.deviceapi with parameters of type ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFUrxUsbToUart_qcom.`setDestIP(ReaderIPEntity readerIPEntity)`
    `boolean` | RFIDWithUHFUrxUart_qcom.`setDestIP(ReaderIPEntity readerIPEntity)` 设置目标IP
    `boolean` | RFIDWithUHFUrxUart2_qcom.`setDestIP(ReaderIPEntity readerIPEntity)`
    `boolean` | RFIDWithUHFUrxNetwork_qcom.`setDestIP(ReaderIPEntity readerIPEntity)`
    `byte[]` | UHFProtocolParseUrxByJava_qcom.`setReaderDestIpSendData(ReaderIPEntity uhfconfig)`
    `byte[]` | UHFProtocolParseUrxByJava_qcom.`setReaderIpSendData(ReaderIPEntity uhfconfig)`
    `boolean` | RFIDWithUHFUrxUsbToUart_qcom.`setUhfReaderIP(ReaderIPEntity readerIPEntity)`
    `boolean` | RFIDWithUHFUrxUart_qcom.`setUhfReaderIP(ReaderIPEntity readerIPEntity)` 设置UHF读写器IP
    `boolean` | RFIDWithUHFUrxUart2_qcom.`setUhfReaderIP(ReaderIPEntity readerIPEntity)`
    `boolean` | RFIDWithUHFUrxNetwork_qcom.`setUhfReaderIP(ReaderIPEntity readerIPEntity)`

  - ### Uses of ReaderIPEntity in com.rscja.team.qcom.rs232utils

    Methods in com.rscja.team.qcom.rs232utils that return ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `ReaderIPEntity` | UHFProtocolParseUrAxBase_qcom.`parseGetEthernetIpv6ConfigResultData(byte[] inData)`
    `ReaderIPEntity` | UHFProtocolParseUrAxBase_qcom.`parseUHFCurrentIpConfigResultData(byte[] inData)`

    Methods in com.rscja.team.qcom.rs232utils with parameters of type ReaderIPEntity
    Modifier and Type | Method and Description
    --- | ---
    `byte[]` | UHFProtocolParseUrAxBase_qcom.`setEthernetConfigInfoSendData(ReaderIPEntity inData)`