## Uses of Class
com.rscja.deviceapi.RFIDWithUHFUART

- Packages that use RFIDWithUHFUART
  Package | Description
  --- | ---
  com.rscja.custom |
  com.rscja.deviceapi |

- - ### Uses of RFIDWithUHFUART in com.rscja.custom

    Subclasses of RFIDWithUHFUART in com.rscja.custom
    Modifier and Type | Class and Description
    --- | ---
    `class` | `M775Authenticate` 英频杰特殊标签定制 Special label customization 第一步:通过`init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 盘点标签之前先要设置回调函数`M775Authenticate.setInventoryCallback(IUHFInventoryCallback)`,然后调用盘点函数`startInventoryTag()`开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`stopInventory()`函数。 For parameter setting, after the connection is successful, call the corresponding function to set parameters and read/write operations.
    `class` | `RFIDWithUHFJieCe`
    `class` | `UHFCSYX` MQTT是长沙盈芯，定制接口
    `class` | `UHFTamperAPI` 阿联酋Acube 定制接口
    `class` | `UHFTemperatureTagsAPI`
    `class` | `UHFUartFoxconn`
    `class` | `UHFXSAPI`

  - ### Uses of RFIDWithUHFUART in com.rscja.deviceapi

    Subclasses of RFIDWithUHFUART in com.rscja.deviceapi
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFAxBase`
    `class` | `RFIDWithUHFRLM`

    Methods in com.rscja.deviceapi that return RFIDWithUHFUART
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithUHFUART` | RFIDWithUHFUART.`getInstance()` 获取UHF操作实例 Acquire UHF operation Instance