A B C D E F G H I J K L M N O P Q R S T U V W X Z

## G

G - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
GBTagLockSendData(String, char, int, int, String, char, char, char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
GBTagLockSendData(String, char, int, int, String, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
Gen2Entity - Class in com.rscja.deviceapi.entity
Gen2Entity() - Constructor for class com.rscja.deviceapi.entity.Gen2Entity
genChar(Fingerprint.BufferEnum) - Method in class com.rscja.deviceapi.Fingerprint
  生成特征值（存于指定缓存区）
  Generate feature value( save in specified buffer zone)
genChar(Fingerprint.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  生成特征值（存于指定缓存区）
  Generate feature value( save in specified buffer zone)
genChar(Fingerprint.BufferEnum) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  生成特征值（存于指定缓存区）
  Generate feature value( save in specified buffer zone)
generate(FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  生成模版
generate(FingerprintWithZAZ.BufferEnum, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  生成模版
generate(FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  生成模版
generateImg(byte[], String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  生成bmp图片
  Generate bmp
generateImg(byte[], String) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
generateImg(byte[], String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  生成bmp图片
  Generate bmp
generateImg(byte[], String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
generateImg(byte[], String) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  生成bmp图片
  Generate bmp
generateImg(byte[], String) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
generateImg(byte[], String) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  生成bmp图片
  Generate bmp
generateImg(byte[], String) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.BleDevice
  获取锁定码
  Get lock code
generateLockCode(ArrayList<Integer>, int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
generateLockCode(ArrayList<Integer>, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取锁定码
  Get lock code
generateLockCode(ArrayList<Integer>, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取锁标签的锁定码
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取锁定码
  Get lock code
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
generateLockCode(ArrayList<Integer>, int) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
generateLockCode(ArrayList<Integer>, int) - Static method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取锁定码
  Get lock code
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
genericFunction(char, char[], char) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
genericFunction(char, char[], char) - Method in class com.rscja.deviceapi.RFIDWithISO15693
genericFunction(char, char[], char) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
genericFunction(char, char[], char) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
genericFunction_ex(char, char, char[], int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
genericFunction_ex(char, char, char[], int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
genericFunction_ex(char, char, char[], int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
genericFunction_ex(char, char, char[], int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
GetAccState() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
GetAccState() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getAddress() - Method in class com.rscja.deviceapi.BleDevice.BleDeviceInfo
getAfi() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getAFI() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取AFI值
  acquire AFI value
getAimId() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
getAllBleDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
  获取所有的ble设备
getAllTagTotalFromFlash() - Method in class com.rscja.deviceapi.BleDevice
  获取R2、R6 缓存的标签数量
  Acquire tag amounts in buffer of R2 and R6.
getAllTagTotalFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getAllTagTotalFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  获取R2、R6 缓存的标签数量
  Acquire tag amounts in buffer of R2 and R6.
getAllTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getAllTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getAllTagTotalFromFlash() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getAllTagTotalFromFlash() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getAllTagTotalFromFlash() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getAllTagTotalFromFlash() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getAmbientTemperature() - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
getAndroidDeviceHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取android设备的硬件版本
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取android设备的硬件版本
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取android设备的硬件版本
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取android设备的硬件版本
getAndroidDeviceHardwareVersionSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getAndroidDeviceRebootSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getAngle() - Method in class com.rscja.deviceapi.entity.RadarLocationEntity
  获取标签的方位角 (Get the azimuth of the label)
getAngleValue(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFRadarLocationCallback
  获取设备方位角 (Obtain the device azimuth)
getAnimalFlag() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的AnimalFlag
  acquire AnimalFlag of animal tag
getAnt() - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
getAnt() - Method in class com.rscja.custom.UHFSFForUrxNetwork.AntInfo
getAnt() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getAnt() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getAnt() - Method in class com.rscja.deviceapi.entity.AntennaPowerEntity
getAnt() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getANT() - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
  获取当前设置的天线
getANT() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取天线
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  获取当前设置的天线
  Acquire current antenna
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
  获取当前设置的天线
  Acquire current antenna
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
  获取当前设置的天线
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取天线
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getANT() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  获取当前设置的天线
  Acquire current antenna
getANT() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
  获取当前设置的天线
  Acquire current antenna
getANT() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
  获取当前设置的天线
getANT() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getANT() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getANT() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取天线
getANT() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getAntennaConnectState() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
getAntennaConnectState() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
  获取天线连接状态
getAntennaConnectState() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getAntennaConnectState() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getAntennaConnectState() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getAntennaConnectState() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
getAntennaConnectState() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getAntennaConnectState() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getAntennaConnectState() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
getAntennaConnectState() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getAntennaConnectStateSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getAntennaConnectStateSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getAntennaName() - Method in class com.rscja.deviceapi.entity.AntennaConnectState
getAntennaName() - Method in class com.rscja.deviceapi.entity.AntennaState
getAntennaPower(AntennaEnum) - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
  获取单个天线的功率
getAntennaPower() - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取天线功率
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取天线功率
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取天线功率
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取天线功率
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getAntennaPower(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getAntennaPower(AntennaEnum) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
getAntennaPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
getAntennaPower(AntennaEnum) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getAntennaPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getAntennaPower(AntennaEnum) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getAntennaPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getAntennaPower(AntennaEnum) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
getAntennaPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
getAntennaPower(AntennaEnum) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getAntennaPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getAntSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getAntSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getAntSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getAntWorkTimeSendData(byte) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getAntWorkTimeSendData(byte) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getAntWorkTimeSendData(byte) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getAppWhiteList() - Method in interface com.rscja.system.ISystemInterfaces
  获取App白名单列表
getAxGPIOInputStatusSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getBalance() - Method in class com.rscja.deviceapi.CardWithBYL
  获取余额和有效期
getBalance() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  获取余额和有效期
getBalance() - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
  获取余额和有效期
getBarcodeBytesData() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  条码原始数据
getBarcodeBytesData() - Method in class com.rscja.deviceapi.entity.BarcodeResult
getBarcodeCodeID() - Method in class com.rscja.deviceapi.entity.BarcodeResult
getBarcodeContinuousScanIntervalTime() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  连续扫描间隔时间
  continuous scanning intervals
getBarcodeContinuousScanTimeOut() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  连续扫描超时时间
  continuous scanning time-out
getBarcodeData() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  条码数据
getBarcodeDataCodeIdContainType() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getBarcodeDecoder() - Method in class com.rscja.barcode.BarcodeFactory
getBarcodeDecoder() - Method in class com.rscja.team.mtk.barcode.barcode2d.Barcode2DFactory_mtk
getBarcodeDecoder() - Method in class com.rscja.team.mtk.barcode.BarcodeFactory_mtk
getBarcodeDecoder() - Method in class com.rscja.team.qcom.barcode.barcode2d.Barcode2DFactory_qcom
  获取条码解码器
getBarcodeDecoder() - Method in class com.rscja.team.qcom.barcode.BarcodeFactory_qcom
getBarcodeFormat() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  条码编码格式
  barcode decoding format
getBarcodeName(int) - Method in class com.rscja.barcode.BarcodeSymbolUtility
  获取条码名称(get barcode name)
getBarcodeName() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  条码类型
getBarcodeName(int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeSymbolUtility
getBarcodeName(int) - Method in class com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
  获取条码名称(get barcode name)
getBarcodeName(int) - Method in class com.rscja.team.qcom.barcode.BarcodeSymbolUtility_qcom
  获取条码名称(get barcode name)
getBarcodeSSIID() - Method in class com.rscja.deviceapi.entity.BarcodeResult
getBarcodeSymbology() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  symbologyCode 条码类型code
getBarcodeTypeByCodeId(String) - Static method in class com.rscja.deviceapi.entity.BarcodeResult
getBarcodeTypeBySSIID(int) - Static method in class com.rscja.deviceapi.entity.BarcodeResult
getBarcodeTypeInSSIID() - Method in class com.rscja.deviceapi.BluetoothReader
getBarcodeTypeInSSIID() - Method in interface com.rscja.deviceapi.interfaces.IReader
getBarcodeTypeInSSIID() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getBarcodeTypeInSSIID() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getBarcodeTypeInSSIID() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getBarcodeTypeInSSIID() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getBattery() - Method in class com.rscja.deviceapi.BleDevice
  获取电池电量
  Acquire battery capacity
getBattery() - Method in class com.rscja.deviceapi.BluetoothReader
getBattery() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getBattery() - Method in interface com.rscja.deviceapi.interfaces.IReader
  获取电池电量
  Acquire battery capacity
getBattery() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getBattery() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getBattery() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getBattery() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getBattery() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getBatteryHealth() - Static method in class com.rscja.utility.BatteryUtils
  电池健康状况，单位 %.
  Battery health status, unit %.
getBatterySendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取电量的发送数据
getBatterySendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getBatteryUniqueId() - Static method in class com.rscja.utility.BatteryUtils
  电池ID.
  Battery ID.
getBaudrate() - Method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  获取波特率
  Acquire baud rate
getBaudrate() - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  获取波特率
  Acquire baud rate
getBeep() - Method in class com.rscja.deviceapi.BluetoothReader
getBeep() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
getBeep() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getBeep() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getBeepSendData(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取设置蜂鸣器的发送数据
getBeepSendData(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
  获取设置蜂鸣器的发送数据
getBeepSendData(boolean) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getBeepSendData(boolean) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getBeepSendData(boolean) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getBlackWhiteListState() - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
getBlackWhiteListState() - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
getBleDeviceByMac(String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
  通过蓝牙地址获取蓝牙设备
getBleDeviceInfo() - Method in class com.rscja.deviceapi.BleDevice
getBleDeviceInfo() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getBleDeviceInfo() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getBleHardwareVersion() - Method in class com.rscja.deviceapi.BleDevice
  获取蓝牙硬件版本
getBleHardwareVersion() - Method in class com.rscja.deviceapi.BluetoothReader
getBleHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getBleHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
getBleHardwareVersion() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getBleHardwareVersion() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getBleHardwareVersion() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getBluetoothDevice() - Method in class com.rscja.deviceapi.BleDevice.BleDeviceInfo
getBluetoothDeviceAddress() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothData
getBluetoothDeviceAddress() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getBluetoothDeviceAddress() - Method in class com.rscja.team.qcom.service.BLEService_qcom
getBluetoothVersion() - Method in class com.rscja.deviceapi.BleDevice
  获取蓝牙版本号(acquire Bluetooth version)
getBluetoothVersion() - Method in class com.rscja.deviceapi.BluetoothReader
getBluetoothVersion() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getBluetoothVersion() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  获取蓝牙版本号(acquire Bluetooth version)
getBluetoothVersion() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getBluetoothVersion() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getBluetoothVersion() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getBrokenId(int, int, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
getBrokenId(int, int, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
getBrokenId(int, int, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
getBTConnectStatus() - Method in class com.rscja.team.qcom.service.BLEService_qcom
getBytes(char[]) - Static method in class com.rscja.utility.StringUtility
  char类型数组转byte类型数组
getCalibrationData() - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
getCalibrationData() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getCalibrationData() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getCD() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Gets the CD (Carrier Detect) bit from the underlying UART.
getCD() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getChars(byte[]) - Static method in class com.rscja.utility.StringUtility
  byte类型数组转char类型数组
getChipInfo() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getChipType() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo
getCmd(int, int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom
getCmdList() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom
getCmdList(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom
getCmdList(int, int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom
getCmdList(int) - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
getCmdList(int, int) - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
getCmdList() - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
getCmdList(int) - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
getCmdList(int, int) - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
getCodeId(String) - Method in class com.rscja.team.qcom.barcode.symbol.CoAsiaBarcodeSymbol_qcom
getConnectionStatus() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
getConnectionStatus() - Method in class com.rscja.team.qcom.usb.pl2302.UsbPL2302
getConnectionStatus() - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
getConnectStatus() - Method in class com.rscja.deviceapi.BleDevice
  获取UHF连接状态
  Acquire UHF connection status
getConnectStatus() - Method in class com.rscja.deviceapi.BluetoothReader
getConnectStatus() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getConnectStatus() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  获取蓝牙连接状态(Acquire Bluetooth connection status)
getConnectStatus() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取UHF连接状态
  Acquire UHF connection status
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取UHF连接状态
  Acquire UHF connection status
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getConnectStatus() - Method in class com.rscja.deviceapi.UhfBase
getConnectStatus() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getConnectStatus() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取UHF连接状态
  Acquire UHF connection status
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getConnectStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getConnectStatus() - Method in class com.rscja.team.qcom.socket.SocketManageA4
getConnectStatus() - Method in class com.rscja.team.qcom.socket.SocketManageUR4
getControlWork() - Method in class com.rscja.deviceapi.entity.GPIOInfo
getCount() - Method in class com.rscja.custom.UHFSFForUrxNetwork.AntInfo
getCount() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getCountryID() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的国家代码
  acquire national code of animal tag
getCpuType() - Method in class com.rscja.CWDeviceInfo
getCTS() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Gets the CTS (Clear To Send) bit from the underlying UART.
getCTS() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getCurrentCapacity() - Static method in class com.rscja.utility.BatteryUtils
  实际容量，单位mAh.
  Battery Actual capacity, unit mAh.
getCurrentCharge() - Static method in class com.rscja.utility.BatteryUtils
  可用容量，单位mAh.
  Battery Available capacity, unit mAh.
getCurrentNumber() - Method in class com.rscja.custom.UHFTemperatureTagsAPI.MultipleTemperatureInfo
getCW() - Method in class com.rscja.deviceapi.BleDevice
  获取连续波设置
  Acquire CW setup
getCW() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getCW() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取连续波设置
  Acquire CW setup
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取连续波设置
  Acquire CW setup
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getCW() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getCW() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getCW() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getCW() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getCW() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getCW() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getCW() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getCW() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取连续波设置
  Acquire CW setup
getCW() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getCW() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getCWSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getCWSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getCycleCount() - Static method in class com.rscja.utility.BatteryUtils
  循环次数.
  Cycle count.
getData() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取数据，仅对数据文件类型有效
  acquire data, it is only valid for data file type only
getData() - Method in class com.rscja.deviceapi.entity.GPIOInfo
getData() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签数据
  acquire tag data
getData() - Method in class com.rscja.team.qcom.http.NetResult_qcom
getData(byte[]) - Method in class com.rscja.team.qcom.usb.R1HFUSB
getData(byte[]) - Method in interface com.rscja.team.qcom.usb.UsbBase_qcom.DataCallback
getDataBlock() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的DataBlock
  acquire DataBlock of animal tag
getDecoderSVersionInfo() - Method in class com.rscja.barcode.BarcodeDecoder
  返回扫描头和解码库信息
getDecoderSVersionInfo() - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  返回扫描头和解码库信息
getDecodeTime() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  解码时间
getDesfid() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getDESFID() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取DESFID值
  acquire DESFID value
getDestIP() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取目标IP
getDestIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getDestIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取目标IP
getDestIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getDestIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getDestIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getDestIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取目标IP
getDestIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getDeviceInfo() - Static method in class com.rscja.CWDeviceInfo
getDeviceInfo() - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  获取模块的设备信息
getDeviceInfo() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  获取模块的设备信息
getDeviceInfo() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  获取模块的设备信息
getDeviceInfoFromFile() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
getDeviceInfoFromFile() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
getDeviceList(Context) - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
  获取 USB 设备列表
getDeviceName() - Method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  获取设备名
  Acquire device name
getDeviceName() - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  获取设备名
  Acquire device name
getDevices(BluetoothDevice, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.ScanBTCallback
getDeviceVersion() - Method in class com.rscja.deviceapi.FingerprintSM206B
  获取指纹模块固件版本
getDeviceVersion() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
getDeviceVersion() - Method in class com.rscja.team.qcom.deviceapi.FingerprintSM206B_qcom
getDns1() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getDns2() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getDSR() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Gets the DSR (Data Set Ready) bit from the underlying UART.
getDSR() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getDTR() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Gets the DTR (Data Terminal Ready) bit from the underlying UART.
getDTR() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getEmptyId(int, int) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  获取指定编号范围内可注册的首个编号
getEmptyId(int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  获取指定编号范围内可注册的首个编号
getEmptyId(int, int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  获取指定编号范围内可注册的首个编号
getEncryptionType() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取加密方式
  acquire encryption method
getEngineExtrasInfo() - Method in class com.rscja.barcode.Barcode2DSHardwareInfo
  扫描头额外的扩展信息
getEngineExtrasInfo() - Method in interface com.rscja.barcode.IBarcode2DSHardwareInfo
getEngineExtrasInfo() - Method in class com.rscja.team.mtk.barcode.Barcode2DSHardwareInfo_mtk
getEngineExtrasInfo() - Method in class com.rscja.team.qcom.barcode.Barcode2DSHardwareInfo_qcom
  扫描头的额外信息
getEngineName() - Method in class com.rscja.barcode.Barcode2DSHardwareInfo
  扫描头型号
getEngineName() - Method in interface com.rscja.barcode.IBarcode2DSHardwareInfo
getEngineName() - Method in class com.rscja.team.mtk.barcode.Barcode2DSHardwareInfo_mtk
getEngineName() - Method in class com.rscja.team.qcom.barcode.Barcode2DSHardwareInfo_qcom
  扫描头型号
getEnrollCount(int, int, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
getEnrollCount(int, int, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
getEnrollCount(int, int, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
getEpc() - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
getEpc() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getEpc() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getEPC() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getEPCAndTIDUserMode() - Method in class com.rscja.custom.UHFXSAPI
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.BleDevice
  获取当前循环盘点的模式(EPC或者EPC+TID或者EPC+TID+USER)
  Acquire current scan mode(EPC or EPC+TID or EPC+TID+USER)
getEPCAndTIDUserMode() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getEPCAndTIDUserMode() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  设置R6工作模式
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取当前循环盘点的模式(EPC或者EPC+TID或者EPC+TID+USER)
  Acquire current scan mode(EPC or EPC+TID or EPC+TID+USER)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getEPCAndTIDUserMode() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
  设置R6工作模式
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取当前循环盘点的模式(EPC或者EPC+TID或者EPC+TID+USER)
  Acquire current scan mode(EPC or EPC+TID or EPC+TID+USER)
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getEPCAndTIDUserMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getEPCAndTIDUserModeEx(int[], int[], int[], int[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getEpcBytes() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getEPCTIDModeSendData(char, char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getEPCTIDModeSendData(char, char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getErrCode() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
getErrCode() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUSB
getErrCode() - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
getErrCode() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  获取`RFIDWithUHFUrxUsbToUart.init(android.hardware.usb.UsbDevice, android.content.Context)`失败的错误码
  Acquire `RFIDWithUHFUrxUsbToUart.init(android.hardware.usb.UsbDevice, android.content.Context)` error codes of failure.
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  获取`RFIDWithUHFUSB.init(android.hardware.usb.UsbDevice, android.content.Context)`失败的错误码
  Acquire `RFIDWithUHFUSB.init(android.hardware.usb.UsbDevice, android.content.Context)` error codes of failure.
getErrCode() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getErrCode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getErrCode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getErrCode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getErrCode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
getErrCode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
  获取`RFIDWithUHFUrxUsbToUart_qcom.init(android.hardware.usb.UsbDevice, android.content.Context)`失败的错误码
  Acquire `RFIDWithUHFUrxUsbToUart_qcom.init(android.hardware.usb.UsbDevice, android.content.Context)` error codes of failure.
getErrCode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
  获取`RFIDWithUHFUSB_qcom.init(android.hardware.usb.UsbDevice, android.content.Context)`失败的错误码
  Acquire `RFIDWithUHFUSB_qcom.init(android.hardware.usb.UsbDevice, android.content.Context)` error codes of failure.
getErrorMsg(int) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
getEthernetIpAssignModeSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getEthernetIpConfig() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取以太网配置信息
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取以太网配置信息
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取以太网配置信息
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取以太网配置信息
getEthernetIpConfigSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getEthernetIpv6ConfigSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getEthernetMac() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4NetWork
getEthernetMac() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4RS232
getEthernetMac() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8NetWork
getEthernetMac() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8RS232
getEthernetMac() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
getEthernetMac() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
getEthernetMac() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
getEthernetMac() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
getEx10SDKFirmware() - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
getEx10SDKFirmware() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getEx10SDKFirmware() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getEx10SDKFirmware() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getExtraData(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getFactory() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo
getFactoryAndChip(String) - Static method in class com.rscja.utility.UhfUtils
  根据tid匹配厂家名称和芯片型号
getFastID() - Method in class com.rscja.deviceapi.BleDevice
getFastID() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getFastID() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
getFastID() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getFastID() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getFastID() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getFastID() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getFastID() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getFastID() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getFastIDSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getFastIDSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getFastInventoryMode() - Method in interface com.rscja.deviceapi.interfaces.IUHF
getFastInventoryMode() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  getFastInventoryMode
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  getFastInventoryMode
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  getFastInventoryMode
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  getFastInventoryMode
getFastInventoryMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  getFastInventoryMode
getFastInventoryMode() - Method in class com.rscja.deviceapi.UhfBase
getFastInventoryMode() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getFastInventoryMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getFastInventoryMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getFastInventoryMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getFastInventoryMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
  getFastInventoryMode
getFastInventoryMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
  getFastInventoryMode
getFileNo() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件号
  acquire file number
getFileSize() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件大小，仅对数据文件类型有效
  acquire file size, it is valid for data file type only
getFileType() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件类型
  acquire file type
getFilterChars() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  过滤字符串
  Filter string
getFingersCount() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取模块中采集的指纹数量
  Acquire collected fingerprint amounts in module.
getFingersCount() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取模块中采集的指纹数量
  Acquire collected fingerprint amounts in module.
getFingersCount() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  获取模块中采集的指纹数量
  Acquire collected fingerprint amounts in module.
getFingersCount() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  获取模块中采集的指纹数量
  Acquire collected fingerprint amounts in module.
getFingerTemplate() - Method in class com.rscja.deviceapi.FingerprintSM206B
  获取指纹模板数据，用户录入 1 次指纹，生成 256 字节指纹特征值
getFingerTemplate() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
getFingerTemplate() - Method in class com.rscja.team.qcom.deviceapi.FingerprintSM206B_qcom
getFrequencyMode() - Method in class com.rscja.deviceapi.BleDevice
  读取模块的工作模式
  Read work mode of module
getFrequencyMode() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getFrequencyMode() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
getFrequencyMode() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取模块的工作模式
  Read work mode of module
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取模块的工作模式
  Read work mode of module
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getFrequencyMode() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getFrequencyMode() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  读取模块的工作模式
  Read work mode of module
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getFrequencyMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getFrequencyModeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getFrequencyModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getFrequencyPoint() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getFullData() - Method in class com.rscja.deviceapi.entity.GPIOInfo
getGateway() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getGen2() - Method in class com.rscja.deviceapi.BleDevice
getGen2() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getGen2() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取Gen2参数
  Acquire Gen2 parameter
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
GetGen2() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
getGen2() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getGen2() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getGen2() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
GetGen2() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getGen2() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getGen2() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getGen2() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getGen2() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getGen2() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
getGen2() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getGen2() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getGen2SendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getGen2SendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getGpiName() - Method in class com.rscja.deviceapi.entity.GPIStateEntity
getGPIOCmd() - Method in class com.rscja.team.qcom.uhfhandler.UHFUrAxDataHandle
getGpiState() - Method in class com.rscja.deviceapi.entity.GPIStateEntity
getGpoName() - Method in class com.rscja.deviceapi.entity.GPOEntity
getGpoState() - Method in class com.rscja.deviceapi.entity.GPOEntity
getHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取硬件版本
  read hardware version
getHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
getHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithLF
  读取硬件版本
  read hardware version
getHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getHardwareVersion() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getHardwareVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  读取硬件版本
  read hardware version
getHardwareVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getHardwareVersion() - Method in class com.rscja.team.qcom.service.BLEService_qcom
getHexChallenge() - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
getHexTagResponse() - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
getHexTagsShortenedTID() - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
getHF14443A() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取14443A操作对象 (Get the 14443A operation object)
getHF14443B() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取14443B操作对象 (Get the 14443B operation object)
getHF15693() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取15693操作对象 (Get the 15693 operation object)
getHFVersion() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取高频版本号(Get the HF version)
getId() - Method in class com.rscja.deviceapi.entity.HF14443RequestEntity
getId() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签ID
  acquire tag ID
getId() - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
  获取指纹模块ID(十六进制)
  Acquire fingerprint module ID (hex)
getID() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹ID
  Acquire fingerprint ID
getID() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取指纹ID
  Acquire fingerprint ID
getID() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  获取指纹ID
  Acquire fingerprint ID
getID() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  获取指纹ID
  Acquire fingerprint ID
getIDAndPowerWithWattmeter() - Method in class com.rscja.deviceapi.Infrared
  获取电表ID和电能值,97标准
  Acquire powermeter ID and energy value, 97 standard
getIDAndPowerWithWattmeter(int) - Method in class com.rscja.deviceapi.Infrared
  获取电表ID和电能值
  Acquire powermeter ID and energy value
getIDAndPowerWithWattmeter() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  获取电表ID和电能值,97标准
  Acquire powermeter ID and energy value, 97 standard
getIDAndPowerWithWattmeter(int) - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  获取电表ID和电能值
  Acquire powermeter ID and energy value
getIDAndPowerWithWattmeter() - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  获取电表ID和电能值,97标准
  Acquire powermeter ID and energy value, 97 standard
getIDAndPowerWithWattmeter(int) - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  获取电表ID和电能值
  Acquire powermeter ID and energy value
getIdBytes() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签ID
  acquire tag ID
getIdData() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取64bit的识别号数据，十六进制表示
  acquire 64bit identification number, hexdecimal
getImage() - Method in class com.rscja.deviceapi.Fingerprint
  获取指纹图像（存于模块图像缓存区）
  Acquire fingerprint image( save in buffer zone of module image)
getImage() - Method in class com.rscja.deviceapi.FingerprintSM206B
getImage(int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  从采集器采集指纹图像并保存于 ImageBuffer 中
getImage() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取指纹图像（存于模块图像缓存区）
  Acquire fingerprint image( save in buffer zone of module image)
getImage() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
getImage(int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  从采集器采集指纹图像并保存于 ImageBuffer 中
getImage() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  获取指纹图像（存于模块图像缓存区）
  Acquire fingerprint image( save in buffer zone of module image)
getImage() - Method in class com.rscja.team.qcom.deviceapi.FingerprintSM206B_qcom
getImage(int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  从采集器采集指纹图像并保存于 ImageBuffer 中
getIndex() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getInputStatus() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取输入口状态
getInputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getInputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取输入口状态
getInputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getInputStatus() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  功能：获取继电器和 IO 控制输出设置状态 返回值：null -- 执行失败 data：2字节 第一个字节：output1: 0:低电平 1：高电平 第二个字节: output2: 0:低电平 1：高电平
getInputStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getInputStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getInputStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取输入口状态
getInputStatus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getInsertIndex(List<UHFTAGInfo>, UHFTAGInfo, boolean[], int) - Static method in class com.rscja.team.qcom.utility.CheckUtils
getInsertIndex(List<UHFTAGInfo>, UHFTAGInfo, boolean[]) - Static method in class com.rscja.utility.UhfUtils
getInstance() - Static method in class com.rscja.barcode.Barcode2DSHardwareInfo
getInstance() - Static method in class com.rscja.barcode.BarcodeFactory
getInstance() - Static method in class com.rscja.barcode.BarcodeSymbolUtility
getInstance() - Static method in class com.rscja.barcode.BarcodeUtility
  获取条码操作实例 Acquire barcode operation Instance.
getInstance() - Static method in class com.rscja.custom.M775Authenticate
  实例化M775Authenticate对象(Instantiating M775Authenticate Object)
getInstance() - Static method in class com.rscja.custom.RFIDWithUHFJieCe
getInstance() - Static method in class com.rscja.custom.UHFCSYX
getInstance() - Static method in class com.rscja.custom.UHFCSYXForURx
getInstance() - Static method in class com.rscja.custom.UHFTamperAPI
getInstance() - Static method in class com.rscja.custom.UHFTemperatureSensors
getInstance() - Static method in class com.rscja.custom.UHFTemperatureTag
getInstance() - Static method in class com.rscja.custom.UHFTemperatureTagsAPI
getInstance() - Static method in class com.rscja.custom.UHFUartFoxconn
getInstance() - Static method in class com.rscja.custom.UHFUartTemperatureTag
getInstance() - Static method in class com.rscja.custom.UHFXSAPI
getInstance() - Static method in class com.rscja.deviceapi.Barcode1D
  获取一维条码操作实例
  Acquire 1D barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.Barcode2D
  获取二维条码操作实例
  * Acquire 2D barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.BluetoothReader
  Get BluetoothReader
getInstance() - Static method in class com.rscja.deviceapi.CardWithBYL
  获取RFID低频操作实例
getInstance() - Static method in class com.rscja.deviceapi.Fingerprint
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.FingerprintSM206B
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithMorpho
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithTLK1NC
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithZAZ
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.deviceapi.Infrared
getInstance() - Static method in class com.rscja.deviceapi.LedLight
  获取LED灯操作实例
  Acquire LED operation example
getInstance() - Static method in class com.rscja.deviceapi.Module
  获取操作实例
  Acquire operation Instance
getInstance() - Static method in class com.rscja.deviceapi.Printer
  获取打印机模块操作实例
  Acquire printer module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.PSAM
  获取PSAM操作实例
  Acquire PSAM operation Instance
getInstance() - Static method in class com.rscja.deviceapi.R1HFAndPsamManage
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443A
  获取ISO14443A协议操作实例
  Acquire ISO14443A protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  获取ISO14443A CPU卡协议操作实例
  Acquire ISO14443A CPU card protocol operation example
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取ISO14443B协议操作实例
  Acquire ISO14443B protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO15693
  获取ISO15693协议操作实例
  Acquire ISO15693 protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithLF
  获取RFID低频操作实例
  Acquire RFID LF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA4
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA8
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFBLE
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFRLM
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUART
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUSB
getInstance() - Static method in class com.rscja.deviceapi.ScanerLedLight
  获取LED灯操作实例
  Acquire LED light operation example
getInstance() - Static method in class com.rscja.deviceapi.UsbFingerprint
getInstance() - Static method in class com.rscja.scanner.led.ScanLedManage
getInstance() - Static method in class com.rscja.system.SystemInterfacesFactory
getInstance() - Static method in class com.rscja.team.mtk.barcode.barcode2d.Barcode2DFactory_mtk
getInstance() - Static method in class com.rscja.team.mtk.barcode.BarcodeFactory_mtk
getInstance() - Static method in class com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
getInstance() - Static method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  获取条码操作实例 Acquire barcode operation Instance.
getInstance() - Static method in class com.rscja.team.mtk.barcode.symbol.DlBarcodeSymbol_mtk
getInstance() - Static method in class com.rscja.team.mtk.custom.M775Authenticate_mtk
getInstance() - Static method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
getInstance() - Static method in class com.rscja.team.mtk.custom.UHFUartFoxconn_mtk
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  获取一维条码操作实例
  Acquire 1D barcode operation Instance.
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  获取二维条码操作实例
  * Acquire 2D barcode operation Instance.
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.DeviceAPI
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.LedLight_mtk
  获取LED灯操作实例
  Acquire LED operation example
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.Module_mtk
  获取操作实例
  Acquire operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  获取打印机模块操作实例
  Acquire printer module operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.PSAM_mtk
  获取PSAM操作实例
  Acquire PSAM operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A4CPU_mtk
  获取ISO14443A CPU卡协议操作实例
  Acquire ISO14443A CPU card protocol operation example
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  获取ISO14443A协议操作实例
  Acquire ISO14443A protocol operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443B_mtk
  获取ISO14443B协议操作实例
  Acquire ISO14443B protocol operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
  获取ISO15693协议操作实例
  Acquire ISO15693 protocol operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  获取LED灯操作实例
  Acquire LED light operation example
getInstance() - Static method in class com.rscja.team.mtk.deviceapi.UsbFingerprint_mtk
getInstance() - Static method in class com.rscja.team.mtk.scanner.led.ScanLedManage_mtk
getInstance() - Static method in class com.rscja.team.mtk.system.SystemInterfacesFactory_mtk
getInstance() - Static method in class com.rscja.team.mtk.system.SystemPropValues_mtk
getInstance() - Static method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
getInstance() - Static method in class com.rscja.team.mtk.utility.BatteryManage
getInstance() - Static method in class com.rscja.team.qcom.barcode.barcode2d.Barcode2DFactory_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.BarcodeFactory_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.BarcodeSymbolUtility_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  获取条码操作实例 Acquire barcode operation Instance.
getInstance() - Static method in class com.rscja.team.qcom.barcode.symbol.CoAsiaBarcodeSymbol_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.symbol.DlBarcodeSymbol_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.symbol.HoneywellBarcodeSymbol_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.symbol.IdataBarcodeSymbol_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.symbol.MobyDataBarcodeSymbol_qcom
getInstance() - Static method in class com.rscja.team.qcom.barcode.symbol.ZebraBarcodeSymbol_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.UHFCSYX_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.UHFTamperAPI_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
getInstance() - Static method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
getInstance() - Static method in class com.rscja.team.qcom.custom.UHFUartFoxconn_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  获取一维条码操作实例
  Acquire 1D barcode operation Instance.
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  获取二维条码操作实例
  * Acquire 2D barcode operation Instance.
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
  Get BluetoothReader
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
  获取RFID低频操作实例
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance.
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.FingerprintSM206B_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  获取操作实例
  Acquire operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.LedLight_qcom
  获取LED灯操作实例
  Acquire LED operation example
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.Module_qcom
  获取操作实例
  Acquire operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.PSAM_qcom
  获取PSAM操作实例
  Acquire PSAM operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A4CPU_qcom
  获取ISO14443A CPU卡协议操作实例
  Acquire ISO14443A CPU card protocol operation example
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  获取ISO14443A协议操作实例
  Acquire ISO14443A protocol operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443B_qcom
  获取ISO14443B协议操作实例
  Acquire ISO14443B protocol operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
  获取ISO15693协议操作实例
  Acquire ISO15693 protocol operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  获取RFID低频操作实例
  Acquire RFID LF operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  获取LED灯操作实例
  Acquire LED light operation example
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBleByJava_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.UHFUrxAutoInventoryTagFactory_qcom
getInstance() - Static method in class com.rscja.team.qcom.deviceapi.UsbFingerprint_qcom
getInstance() - Static method in class com.rscja.team.qcom.scanner.led.ScanLedManage_qcom
getInstance() - Static method in class com.rscja.team.qcom.serialportapi.SerialportAPI
getInstance() - Static method in class com.rscja.team.qcom.system.SystemInterfacesFactory_qcom
getInstance() - Static method in class com.rscja.team.qcom.system.SystemPropValues_qcom
getIntegerSomeBit(int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  取整数的某一位
  get one place of integer
getIntegerSomeBit(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  取整数的某一位
  get one place of integer
getIntegerSomeBit(int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  取整数的某一位
  get one place of integer
getIntegerSomeBit(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  取整数的某一位
  get one place of integer
getInterceptTrimLeft() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  截取左边字符串
  Capture string on left
getInterceptTrimRight() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  截取右边字符串
  capture string on right
getInventoryModeEntity() - Method in class com.rscja.deviceapi.entity.TagInfoRule
  获取盘点模式
getInventoryParameter() - Method in class com.rscja.deviceapi.entity.TagInfoRule
  获取盘点参数
getInventorySingleTagSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取开启单次盘点标签的发送数据
getInventorySingleTagSendData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getInventorySingleTagSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getIOControlSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getIOControlSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getIp() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIP() - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  获取端口
getIpv6Dns1() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Dns2() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Ip1() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Ip2() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Ip3() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getKeyboardHelperParam(Context) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
getKeyMode() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getKillSendData(String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取销毁标签的发送数据
getKillSendData(String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getLastBarcodeCmd(int, int, int) - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
getLastCmd(int, int, int) - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
getLastCmd(int, int) - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
getLastDecImage(BarcodeDecoder.IBarcodeImageCallback) - Method in class com.rscja.barcode.BarcodeDecoder
getLastDecImage(Context) - Method in interface com.rscja.scanner.IScanner
getLastDecImage(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
getLastDecImage(Context) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
getLastDecImage(BarcodeDecoder.IBarcodeImageCallback) - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
getLastDecImage(Context) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
GetLastError() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
GetLastError() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getLBTMode() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getLBTMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getLinkFrequency() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  Link Frequency 设置(Link Frequency setting)
getLocationValue(int, boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFLocationCallback
  获取定位数据 (Obtain location data)
getLocationValue(List<RadarLocationEntity>) - Method in interface com.rscja.deviceapi.interfaces.IUHFRadarLocationCallback
  获取定位数据 (Obtain location data)
getLockSendData(String, int, int, int, String, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取锁标签需要发送的数据
getLockSendData(String, int, int, int, String, String) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getMainboardVersion() - Method in class com.rscja.deviceapi.BleDevice
  获取主板吧版本
getMainboardVersion() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getMainboardVersion() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getManufactor() - Method in class com.rscja.barcode.Barcode2DSHardwareInfo
  扫描头厂家
getManufactor() - Method in interface com.rscja.barcode.IBarcode2DSHardwareInfo
getManufactor() - Method in class com.rscja.team.mtk.barcode.Barcode2DSHardwareInfo_mtk
getManufactor() - Method in class com.rscja.team.qcom.barcode.Barcode2DSHardwareInfo_qcom
  扫描头厂家名称
getManufactureDate() - Static method in class com.rscja.utility.BatteryUtils
  生产日期.
  Battery production date.
getMaxQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
getMaxValue() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取最大值，仅对值文件类型有效
  acquire maximum value, it is valid for value file type only
getMessage(int) - Method in class com.rscja.deviceapi.CardWithBYL
  将错误代码转换为语义消息
getMessage(int) - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  将错误代码转换为语义消息
getMessage(int) - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
  将错误代码转换为语义消息
getMessageHex() - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
getMessages() - Method in class com.rscja.team.qcom.http.NetResult_qcom
getMinQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
getMinValue() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取最小值，仅对值文件类型有效
  acquire minimum value, it is valid for value file type only
getMode() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
  获取盘点模式(Get inventory mode)
getModel() - Method in class com.rscja.CWDeviceInfo
getModel() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  获取设备型号
  Acquire device model NO.
getModel() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  获取设备型号
  Acquire device model NO.
getModelAndCpu() - Method in class com.rscja.CWDeviceInfo
getMorphoDescriptor() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
getMorphoDescriptor() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
getMorphoDescriptor() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
getMorphoDescriptor() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
getMorphoPIDSN() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  获取指纹版本
  acquire fingerprint version
getMorphoPIDSN() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  获取指纹版本
  acquire fingerprint version
getMorphoPIDSN() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  获取指纹版本
  acquire fingerprint version
getMorphoPIDSN() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  获取指纹版本
  acquire fingerprint version
getMorphoSecurityLevel() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
getMorphoSecurityLevel() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
getMorphoSecurityLevel() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
getMorphoSecurityLevel() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
getName() - Method in class com.rscja.deviceapi.BleDevice.BleDeviceInfo
getNationalID() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的NationalID信息
  acquire national infor of animal tag
getNetworkClass(Activity) - Static method in class com.rscja.utility.NetUtils
getNetworkType() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getNetworkType(Activity) - Static method in class com.rscja.utility.NetUtils
  获取当前网络类型
getNewSymbolId(int) - Method in class com.rscja.team.mtk.barcode.symbol.DlBarcodeSymbol_mtk
getNewSymbolId(int) - Method in interface com.rscja.team.mtk.barcode.symbol.IBarcodeSymbol_mtk
getNewSymbolId(int) - Method in class com.rscja.team.qcom.barcode.symbol.CoAsiaBarcodeSymbol_qcom
getNewSymbolId(int) - Method in class com.rscja.team.qcom.barcode.symbol.DlBarcodeSymbol_qcom
getNewSymbolId(int) - Method in class com.rscja.team.qcom.barcode.symbol.HoneywellBarcodeSymbol_qcom
getNewSymbolId(int) - Method in interface com.rscja.team.qcom.barcode.symbol.IBarcodeSymbol_qcom
getNewSymbolId(int) - Method in class com.rscja.team.qcom.barcode.symbol.IdataBarcodeSymbol_qcom
getNewSymbolId(int) - Method in class com.rscja.team.qcom.barcode.symbol.MobyDataBarcodeSymbol_qcom
getNewSymbolId(int) - Method in class com.rscja.team.qcom.barcode.symbol.ZebraBarcodeSymbol_qcom
getNewTagTotalFromFlash() - Method in class com.rscja.deviceapi.BleDevice
getNewTagTotalFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getNewTagTotalFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
getNewTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getNewTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getNewTagTotalFromFlash() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getNewTagTotalFromFlash() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getNewTagTotalFromFlash() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getNewTagTotalFromFlash() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getOriginalUID() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取标签原始的UID
  acquire original UID of tag
getOutputMode() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  输出模式
  Output mode
getParam(int) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  根据指定的参数类型，读取设备参数
getParam(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  根据指定的参数类型，读取设备参数
getParam(int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  根据指定的参数类型，读取设备参数
getParam_zebra(Context, int) - Method in interface com.rscja.scanner.IScanner
getParam_zebra(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
getParam_zebra(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
getParam_zebra(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
getParameter(int) - Method in class com.rscja.barcode.BarcodeDecoder
getParameter(byte[]) - Method in class com.rscja.deviceapi.BluetoothReader
getParameter(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IReader
getParameter(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getParameter(int) - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
getParameter(byte[]) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getParameter(byte[]) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getParameter(byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getParameterSendData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getPartNumber() - Static method in class com.rscja.utility.BatteryUtils
  部件号.
  Part number.
getPassword() - Method in class com.rscja.deviceapi.entity.WifiConfig
getPc() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getPhase() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getPlatform() - Method in class com.rscja.CWDeviceInfo
getPlatform() - Static method in class com.rscja.team.mtk.barcode.Barcode2DSHardwareInfo_mtk
getPlatform() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
getPlatform() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
getPointDouble(int, double) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointDouble(int, int) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointDouble(int, long) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointDouble(int, String) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointFloat(int, float) - Static method in class com.rscja.utility.NumberTool
getPort() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getPort() - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  获取端口
getPortNumber() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Port number within driver.
getPortNumber() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getPower() - Method in class com.rscja.deviceapi.BleDevice
  读取模块的功率
  Read module output power
getPower() - Method in class com.rscja.deviceapi.entity.AntennaPowerEntity
getPower() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getPower() - Method in interface com.rscja.deviceapi.interfaces.ISingleAntenna
  读取模块的功率
  Read module output power
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getPower() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getPower() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getPower() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getPower() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getPowerSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取功率的发送数据
getPowerSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getPrefix() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  前缀
getPrefix() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  Prefix
getPressure() - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
getPrintCodePage() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
getPrintCodePage() - Method in class com.rscja.deviceapi.Printer
getPrintCodePage() - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
getPrinterType() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
getPrinterType() - Method in class com.rscja.deviceapi.Printer
getPrinterType() - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
getProgress(int, int, int) - Method in interface com.rscja.team.qcom.http.IDownLoadProgress_qcom
getProgress(int, int, int) - Method in interface com.rscja.team.qcom.http.IUploadProgress_qcom
getProtocol() - Method in class com.rscja.deviceapi.BleDevice
  获取协议
  Acquire protocol
getProtocol() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getProtocol() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取协议
  Acquire protocol
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取协议
  Acquire protocol
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getProtocol() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getProtocol() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取协议
  Acquire protocol
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getProtocol() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getProtocolSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取协议需要发送数据
getProtocolSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getProxy() - Method in class com.rscja.deviceapi.entity.WifiConfig
getPSAM() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取PSAM操作对象 (Get the PSAM operation object)
getPsamCardID() - Method in class com.rscja.deviceapi.CardWithBYL
  获取psam卡id
getPsamCardID() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  获取psam卡id
getPsamCardID() - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
  获取psam卡id
getPsamId() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
getPsamId() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getPTInfo() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取模块信息
  Acquire module information
getPTInfo() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取模块信息
  Acquire module information
getPTInfo() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  获取模块信息
  Acquire module information
getPTInfo() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  获取模块信息
  Acquire module information
getQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取Q值(Q value)
GetQTPara() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
GetQTPara() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getQueryDR() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的DR参数(DR parameter of the query command)
getQueryM() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的M参数(M parameter of the query command )
getQuerySel() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的sel参数(sel parameter of the query command)
getQuerySession() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的session参数(session parameter of the query command)
getQueryTarget() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的Target参数(Target parameter of the query command)
getQueryTRext() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的TRext参数(TRext parameter of the query command )
getRandomData() - Method in class com.rscja.deviceapi.Fingerprint
  获取随机数，检测模块是否正常
  Acquire random number, detect module is normal or not.
getRandomData() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取随机数，检测模块是否正常
  Acquire random number, detect module is normal or not.
getRandomData() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  获取随机数，检测模块是否正常
  Acquire random number, detect module is normal or not.
getRatedCapacity() - Static method in class com.rscja.utility.BatteryUtils
  额定容量，单位mAh.
  Battery Rated capacity, unit mAh.
getRawData() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取原始数据，十六进制表示
  acquire original data, hexdecimal
getReaderAwaitSleepTime() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  获取读写器等待休眠的时间
getReaderAwaitSleepTime() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getReaderAwaitSleepTime() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getReaderAwaitSleepTime() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getReaderAwaitSleepTime() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getReaderAwaitSleepTime() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getReaderAwaitSleepTimeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getReaderAwaitSleepTimeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getReaderBeepStatusSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getReaderBeepStatusSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getReaderBeepStatusSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getReaderCurrentIp() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取设备当前的IP地址
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取设备当前的IP地址
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取设备当前的IP地址
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取设备当前的IP地址
getReaderDestIpSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getReaderDestIpSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getReaderIpSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getReaderIpSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getReadPermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取读取权限
  acquire read authorization
getReadSendData(String, int, int, int, String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取读标签的发送数据
getReadSendData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getReadTagSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取在循环盘点标签的模式中,读取缓存标签的发送数据
getReadTagSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBleByJava_qcom
getReadTagSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getReadTagSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUSBByJava_qcom
getReadWritePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取读写权限
  acquire read-write authorization
getRemain() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getReserved() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的Reserved信息
  acquire Reserved infor of animal tag
getReserved() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getReservedLength() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
getReservedOffset() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
getResponseHex() - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
getResultCode() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  结果码 `BarcodeDecoder.DECODE_SUCCESS`
  `BarcodeDecoder.DECODE_FAILURE`
  `BarcodeDecoder.DECODE_TIMEOUT`
  `BarcodeDecoder.DECODE_CANCEL`
getResultData() - Method in class com.rscja.deviceapi.entity.InventoryParameter
getRFIDWithUHFA4() - Method in class com.rscja.custom.UHFTemperatureTagsAPI
getRFLink() - Method in class com.rscja.deviceapi.BleDevice
  获取链路参数
  acquire link parameter
getRFLink() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getRFLink() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取链路参数
  acquire link parameter
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取链路参数
  acquire link parameter
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getRFLink() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getRFLink() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取链路参数
  acquire link parameter
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getRFLink() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getRFLinkSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getRFLinkSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getRI() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Gets the RI (Ring Indicator) bit from the underlying UART.
getRI() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getRssi() - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
getRssi() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getRssi() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getRssi() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getRssiCode() - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
getRssiCode() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getRssiCode() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getRTS() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Gets the RTS (Request To Send) bit from the underlying UART.
getRTS() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getScanBarcodeInBlinkModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getScanBarcodeInTriggleModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getScanBarcodeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取扫描条码的发送数据
getScanBarcodeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getScanLed() - Method in class com.rscja.scanner.led.ScanLedManage
getScanLed() - Static method in class com.rscja.team.mtk.scanner.led.C6000_6762_ScanLed_mtk
getScanLed() - Static method in class com.rscja.team.mtk.scanner.led.C7X_6765_ScanLed_mtk
getScanLed() - Static method in class com.rscja.team.mtk.scanner.led.C90_6762_ScanLed_mtk
getScanLed() - Method in class com.rscja.team.mtk.scanner.led.ScanLedManage_mtk
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.C60_6765_11_ScanLed_qcom
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.C60_qcm2150_10_ScanLed_qcom
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.C61_smd450_90_ScanLed_qcom
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.C66_smd450_90_ScanLed_qcom
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.C66m_sm6115_10_ScanLed_qcom
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.MC50_4350_12_ScanLed_qcom
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.P80_8786_130_ScanLed_qcom
getScanLed() - Static method in class com.rscja.team.qcom.scanner.led.P80_8953_90_ScanLed_qcom
getScanLed() - Method in class com.rscja.team.qcom.scanner.led.ScanLedManage_qcom
getScannerInerface() - Static method in class com.rscja.scanner.utility.ScannerUtility
getScannerInerface() - Static method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
getScannerInerface() - Static method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
getScannerParameter(Context) - Method in interface com.rscja.scanner.IScanner
getScannerParameter(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
getScannerParameter(Context) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
getScannerParameter(Context) - Method in class com.rscja.team.qcom.scanner.utility.ScannerParameterUtility_qcom
getScannerParameter(Context) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
getScanResultBroadcastAction() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  Broadcast Action
getScanResultBroadcastKey() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  Broadcast Key
getSecurityType() - Method in class com.rscja.deviceapi.entity.WifiConfig
getSelectAction() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取select 命令的Action参数 (Action parameter of the select command)
getSelectTarget() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取select命令的Target参数 (Target parameter of the select command)
getSelectTruncate() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取select命令的Truncate参数(Truncate parameter of the select command)
getSensorCode() - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
getSensorCode() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getSensorCode() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getSerial() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  The serial number of the underlying UsbDeviceConnection, or `null`.
getSerial() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
getSerialNumber() - Static method in class com.rscja.utility.BatteryUtils
  序列号.
  Serial number.
getSetSoftResetSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getSetSoftResetSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getSetSoftResetSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getShortenedTidHex() - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
getSignalValue() - Method in class com.rscja.deviceapi.entity.TagLocationInfo
getSmartBattery() - Static method in class com.rscja.utility.BatteryUtils
  智能电池.
  Smart battery.
getSN() - Method in interface com.rscja.system.ISystemInterfaces
  获取SN号
getSN() - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
getSN() - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
getSN(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getSN() - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
getSsid() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getSsid() - Method in class com.rscja.deviceapi.entity.WifiConfig
getStartInventoryTagSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取循环盘点标签的发送数据
getStartInventoryTagSendData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getStartInventoryTagSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getStartQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
getStaticIpConfig() - Method in class com.rscja.deviceapi.entity.WifiConfig
getStatus(ConnectionStatus, T) - Method in interface com.rscja.deviceapi.interfaces.ConnectionStatusCallback
getStatus(ConnectionStatus, Object) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
getStatus(ConnectionStatus, Object) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
getStatusMsg(int) - Static method in class com.rscja.deviceapi.FingerprintWithFIPS
getStatusMsg(int) - Static method in class com.rscja.deviceapi.FingerprintWithMorpho
getStatusMsg(int) - Static method in class com.rscja.deviceapi.FingerprintWithTLK1NC
getSTM32Version() - Method in class com.rscja.deviceapi.BluetoothReader
getSTM32Version() - Method in interface com.rscja.deviceapi.interfaces.IReader
  获取stm32版本号(Acquire stm32 version )
getSTM32Version() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getSTM32Version() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getSTM32Version() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getSTM32Version() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getSTM32Version() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getSTM32Version() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
getSTM32Version() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getSTM32Version() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getSTM32VersionSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getSTM32VersionSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getStopInventorySendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取停止循环盘点标签的发送数据
getStopInventorySendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getStopScanBarcodeInBlinkModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getStopScanBarcodeInTriggleModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getSubnetMask() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getSuffix() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
  suffix
getSymbolIdByAIM(String) - Method in class com.rscja.team.mtk.barcode.symbol.DlBarcodeSymbol_mtk
getSymbolIdByAIM(String) - Method in class com.rscja.team.qcom.barcode.symbol.DlBarcodeSymbol_qcom
GetSystemInfo(int, byte[]) - Method in class com.rscja.team.qcom.r1.hf.HF15693
getSystemInterfaces(Context) - Method in class com.rscja.system.SystemInterfacesFactory
getSystemInterfaces(Context) - Method in class com.rscja.team.mtk.system.SystemInterfacesFactory_mtk
getSystemInterfaces(Context) - Method in class com.rscja.team.qcom.system.SystemInterfacesFactory_qcom
getTag() - Method in class com.rscja.deviceapi.entity.RadarLocationEntity
  获取标签值 (Get the value of the label)
getTagCmd() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothData
getTagCmd() - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
getTagCmd() - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
getTagDataFromFlash() - Method in class com.rscja.deviceapi.BleDevice
  获取R2、R6缓存的标签信息
  Acquire tag information in buffer of R2 and R6
getTagDataFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getTagDataFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  获取R2、R6缓存的标签信息
  Acquire tag information in buffer of R2 and R6
getTagDataFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getTagDataFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getTagDataFromFlash() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getTagDataFromFlash() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getTagDataFromFlash() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getTagDataFromFlash() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getTagfocus() - Method in class com.rscja.deviceapi.BleDevice
getTagfocus() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getTagfocus() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
getTagfocus() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getTagfocus() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getTagfocus() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getTagfocus() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getTagfocus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getTagfocus() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getTagfocusSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getTagfocusSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getTagInfo() - Method in class com.rscja.team.qcom.socket.SocketManageUR4
getTagLocate(Context) - Method in interface com.rscja.deviceapi.interfaces.IHandheldRFID
getTagLocate(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getTagLocate(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getTagLocate(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getTagLocate(Context) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getTagLocate(Context) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getTagLocate(Context) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getTagLocate(Context) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getTagLocate(Context) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getTagLocationInfo() - Method in class com.rscja.deviceapi.entity.TagLocationEntity
getTamper() - Method in class com.rscja.custom.UHFTamperAPI.TamperInfo
getTcpServiceVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取UHF TCP服务版本
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取UHF TCP服务版本
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取UHF TCP服务版本
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取UHF TCP服务版本
getTeam() - Method in class com.rscja.CWDeviceInfo
getTempCount() - Method in class com.rscja.custom.UHFTemperatureTagsAPI.TempertureInfo
getTempeCode() - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
getTempeCode() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getTempeCode() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getTemperature() - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
getTemperature() - Method in class com.rscja.custom.UHFTemperatureTagsAPI.TempertureInfo
getTemperature() - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
getTemperature() - Method in class com.rscja.deviceapi.BleDevice
  获取模块温度
  Acquire module Temperature
getTemperature() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getTemperature() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取模块温度
  Acquire module Temperature
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取模块温度
  Acquire module Temperature
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
GetTemperature() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
getTemperature() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getTemperature() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
GetTemperature() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取模块温度
  Acquire module Temperature
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getTemperature() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getTemperatureByContactResistance() - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
getTemperatureSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取模块温度
getTemperatureSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getTemperture() - Method in class com.rscja.custom.UHFTemperatureTagsAPI.MultipleTemperatureInfo
getTid() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getTidBytes() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getTimestamp() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getTotal() - Method in class com.rscja.custom.UHFTemperatureTagsAPI.MultipleTemperatureInfo
getTriggerWorkModePara() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取触发工作模式参数
getTriggerWorkModePara() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getTriggerWorkModePara() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取触发工作模式参数
getTriggerWorkModePara() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getTriggerWorkModePara() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getTriggerWorkModePara() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getTriggerWorkModePara() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取触发工作模式参数
getTriggerWorkModePara() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getTriggerWorkModeParaSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getTriggerWorkModeParaSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getTurnkey() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
getType() - Method in class com.rscja.deviceapi.entity.HF14443RequestEntity
getType() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getType() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签类型
  acquire tag type
getUart() - Method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  获取串口路径
  Acquire serial port directory
getUart() - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  获取串口路径
  Acquire serial port directory
getUhfBank() - Method in class com.rscja.deviceapi.entity.RadarLocationEntity
  获取标签的类型 (Get the type of label) `#IUHF.Bank_RESERVED`、`#IUHF.Bank_EPC`、`#IUHF.Bank_TID`、`#IUHF.Bank_USER`
getUHFCurrentIpConfigSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getUhfReaderIP() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取UHF读写器IP
getUhfReaderIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getUhfReaderIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取UHF读写器IP
getUhfReaderIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getUhfReaderIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getUhfReaderIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getUhfReaderIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取UHF读写器IP
getUhfReaderIP() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getUhfSoftwareVersion() - Method in class com.rscja.deviceapi.BleDevice
  读取UHF模块版本号
  Read UHF module version
getUhfSoftwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
getUhfSoftwareVersion() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
getUhftagInfo() - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
getUhftagInfo() - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
getUhftagInfo() - Method in class com.rscja.custom.UHFSFForUrxNetwork.AntInfo
getUhftagInfo() - Method in class com.rscja.custom.UHFTamperAPI.TamperInfo
getUhftagInfo() - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
getUhftagInfo() - Method in class com.rscja.custom.UHFTemperatureTagsAPI.TempertureInfo
getUhftagInfo() - Method in class com.rscja.deviceapi.entity.TagLocationEntity
getUHFTAGInfo() - Method in class com.rscja.team.qcom.usb.UrxUsb_qcom
getUHFUrAxDataHandle() - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
getUHFUrAxDataHandle() - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
getUHFUrAxDataHandle() - Method in class com.rscja.team.qcom.socket.SocketManageA4
getUhfvalidData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
getUhfvalidData(AbstractQueue<Byte>, int, boolean) - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
getUid() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getUID() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUID() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUID() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443B_mtk
  获取卡片ID
  Acquire card ID
getUID() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443B_qcom
  获取卡片ID
  Acquire card ID
getUIDBytes() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUIDBytes() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUIDBytes() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443B_mtk
  获取卡片ID
  Acquire card ID
getUIDBytes() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443B_qcom
  获取卡片ID
  Acquire card ID
getUidTypeB() - Method in interface com.rscja.deviceapi.interfaces.IHF14443B
  获取卡片ID (Acquire card ID)
getUidTypeB() - Method in class com.rscja.team.qcom.r1.hf.HF14443B
  获取卡片ID (Acquire card ID)
getUIDWith4450Card() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  获取UID,用于4450Card
  Acquire UID, used for 4450 card
getUIDWith4450Card() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取UID,用于4450Card
  Acquire UID, used for 4450 card
getUIDWith4450Card() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  获取UID,用于4450Card
  Acquire UID, used for 4450 card
getUIDWithHID() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取HID卡
  Read HID card
getUIDWithHID() - Method in class com.rscja.deviceapi.RFIDWithLF
  读取HID卡
  Read HID card
getUIDWithHID() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  读取HID卡
  Read HID card
getUIDWithHitagS() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  获取UID,用于hitag S
  Acquire UID, used for hitag S
getUIDWithHitagS() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取UID,用于hitag S
  Acquire UID, used for hitag S
getUIDWithHitagS() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  获取UID,用于hitag S
  Acquire UID, used for hitag S
getUpdatePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取修改权限
  acquire modify authorization
getUpgradeTcpServiceVersionSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getUsbDevice(Context, int, int) - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
getUsbDeviceConnection() - Method in class com.rscja.team.qcom.usb.pl2302.UsbPL2302
getUsbDeviceConnection() - Method in class com.rscja.team.qcom.usb.RxUsb_qcom
getUsbDeviceConnection() - Method in class com.rscja.team.qcom.usb.UrxUsb_qcom
getUsbDeviceConnection() - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
getUsbDeviceList(Context) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUSB
getUsbDeviceList(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  获取usb列表
getUsbDeviceList(Context) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
  获取usb列表
getUser() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getUserBytes() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getUserLength() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
  获取要盘点的User区长度(User area data length)
getUserOffset() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
  获取要盘点的User区起始地址(User area start address)
getUserSettingSendData(byte) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getValue() - Method in enum com.rscja.barcode.BarcodeUtility.ModuleType
getValue() - Method in enum com.rscja.custom.UHFXSAPI.Bank
getValue() - Method in enum com.rscja.deviceapi.entity.HF15693RequestEntity.TagType
getValue() - Method in class com.rscja.deviceapi.entity.RadarLocationEntity
  获取标签的信号值 (Get the signal value of the tag)
getValue() - Method in enum com.rscja.deviceapi.enums.AntennaEnum
getValue(int) - Static method in enum com.rscja.deviceapi.enums.AntennaEnum
getValue() - Method in enum com.rscja.deviceapi.Fingerprint.BufferEnum
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.FingerprintWithTLK1NC.BufferEnum
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.FingerprintWithZAZ.BufferEnum
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.interfaces.ConnectionStatus
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO14443A.DESFireEncryptionTypekEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO14443A.DESFireFileTypekEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO15693.TagType
getValue() - Method in enum com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk.TagType
getValue() - Method in enum com.rscja.team.qcom.deviceapi.HardwareInterface_qcom.FunctionEnum
getVersion() - Method in class com.rscja.deviceapi.Fingerprint
  获取模块版本
  Acquire module version
getVersion() - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  获取模块的设备信息
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取模块版本
  Acquire module version
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
  获取rfid 版本信息
  Acquire RFID version infor
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取UHF模块版本号
  Read UHF module version
getVersion() - Method in class com.rscja.deviceapi.Printer
getVersion() - Method in class com.rscja.deviceapi.RFIDBase
  获取rfid 版本信息
  Acquire RFID version infor
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取UHF模块版本号
  Read UHF module version
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getVersion() - Static method in class com.rscja.deviceapi.VersionInfo
  获取jar包版本信息
  acquire jar pack version infor
getVersion() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
getVersion() - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
getVersion() - Method in class com.rscja.team.mtk.deviceapi.RFIDBase_mtk
  获取rfid 版本信息
  Acquire RFID version infor
getVersion() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
getVersion() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
getVersion() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  获取模块版本
  Acquire module version
getVersion() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDBase_qcom
  获取rfid 版本信息
  Acquire RFID version infor
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  读取UHF模块版本号
  Read UHF module version
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getVersion() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
getVersion() - Method in class com.rscja.team.qcom.service.BLEService_qcom
getVersions() - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
  获取指纹模块版本号
  Acquire fingerprint module version
getVersionSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getVersionSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
getVoltage() - Method in class com.rscja.deviceapi.entity.BatteryEntity
getWifiInfo() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取wifi热点信息,json格式数据
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取wifi热点信息,json格式数据
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取wifi热点信息,json格式数据
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取wifi热点信息,json格式数据
getWifiInfoSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getWifiIpConfig() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取wifi配置信息
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取wifi配置信息
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取wifi配置信息
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取wifi配置信息
getWifiIpConfigSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getWifiIpv6ConfigSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
getWorkMode() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取工作模式
getWorkMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getWorkMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取工作模式
getWorkMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getWorkMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
getWorkMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
getWorkMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取工作模式
getWorkMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
getWorkModeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getWorkModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
getWritePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取写权限
  acquire write authorization
getWriteSendData(String, int, int, int, String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取写标签的发送数据
getWriteSendData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
GPI1 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPI2 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPI3 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPI4 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPIOInfo - Class in com.rscja.deviceapi.entity
GPIOInfo() - Constructor for class com.rscja.deviceapi.entity.GPIOInfo
GPIStateEntity - Class in com.rscja.deviceapi.entity
GPIStateEntity() - Constructor for class com.rscja.deviceapi.entity.GPIStateEntity
GPIStateEntity(String, int) - Constructor for class com.rscja.deviceapi.entity.GPIStateEntity
GPO1 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPO2 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPO3 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPO4 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPOEntity - Class in com.rscja.deviceapi.entity
GPOEntity(String, int) - Constructor for class com.rscja.deviceapi.entity.GPOEntity
grab() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  采集图像
  Acquire image
grab() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  采集图像
  Acquire image
grab() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  采集图像
  Acquire image
grab() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  采集图像
  Acquire image
GyroAngle - Class in com.rscja.team.qcom.utility
GyroAngle() - Constructor for class com.rscja.team.qcom.utility.GyroAngle

A B C D E F G H I J K L M N O P Q R S T U V W X Z