## Uses of Class
com.rscja.deviceapi.exception.ConfigurationException

- Packages that use ConfigurationException
  Package | Description
  --- | ---
  com.rscja.custom |
  com.rscja.deviceapi |
  com.rscja.team.mtk |
  com.rscja.team.mtk.deviceapi |
  com.rscja.team.qcom |
  com.rscja.team.qcom.custom |
  com.rscja.team.qcom.deviceapi |

- - ### Uses of ConfigurationException in com.rscja.custom

    Methods in com.rscja.custom that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static UHFTemperatureSensors` | UHFTemperatureSensors.`getInstance()`

  - ### Uses of ConfigurationException in com.rscja.deviceapi

    Methods in com.rscja.deviceapi that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithISO15693` | RFIDWithISO15693.`getInstance()` 获取ISO15693协议操作实例 Acquire ISO15693 protocol operation Instance
    `static Module` | Module.`getInstance()` 获取操作实例 Acquire operation Instance
    `static RFIDWithISO14443A` | RFIDWithISO14443A.`getInstance()` 获取ISO14443A协议操作实例 Acquire ISO14443A protocol operation Instance
    `static Infrared` | Infrared.`getInstance()`
    `static CardWithBYL` | CardWithBYL.`getInstance()` 获取RFID低频操作实例
    `static RFIDWithUHFA8` | RFIDWithUHFA8.`getInstance()`
    `static FingerprintWithMorpho` | FingerprintWithMorpho.`getInstance()` 获取指纹模块操作实例 acquire fingerprint module operation eample
    `static FingerprintWithFIPS` | FingerprintWithFIPS.`getInstance()` 获取指纹模块操作实例 Acquire fingerprint module operation Instance
    `static FingerprintWithTLK1NC` | FingerprintWithTLK1NC.`getInstance()`
    `static Barcode1D` | Barcode1D.`getInstance()` 获取一维条码操作实例 Acquire 1D barcode operation Instance.
    `static FingerprintWithZAZ` | FingerprintWithZAZ.`getInstance()` 获取指纹模块操作实例 acquire fingerprint module operation eample
    `static RFIDWithLF` | RFIDWithLF.`getInstance()` 获取RFID低频操作实例 Acquire RFID LF operation Instance
    `static Fingerprint` | Fingerprint.`getInstance()` 获取指纹模块操作实例 Acquire fingerprint module operation Instance.
    `static RFIDWithUHFA4` | RFIDWithUHFA4.`getInstance()`
    `static RFIDWithISO14443B` | RFIDWithISO14443B.`getInstance()` 获取ISO14443B协议操作实例 Acquire ISO14443B protocol operation Instance
    `static Barcode2D` | Barcode2D.`getInstance()` 获取二维条码操作实例 * Acquire 2D barcode operation Instance.
    `static RFIDWithISO14443A4CPU` | RFIDWithISO14443A4CPU.`getInstance()` 获取ISO14443A CPU卡协议操作实例 Acquire ISO14443A CPU card protocol operation example
    `static Printer` | Printer.`getInstance()` 获取打印机模块操作实例 Acquire printer module operation Instance
    `static RFIDWithUHFUART` | RFIDWithUHFUART.`getInstance()` 获取UHF操作实例 Acquire UHF operation Instance

  - ### Uses of ConfigurationException in com.rscja.team.mtk

    Methods in com.rscja.team.mtk that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builder1DConfiguration()` 创建一维条码配置信息 Create 1D barcode config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builder2DConfiguration()` 创建二维条码配置信息 Create 2D barcode config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderA8ExtendedUartConfiguration()` 创建A8扩展串口配置信息
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderBDConfiguration()` 创建北斗配置信息 Create Beidou config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderDefaultConfiguration()`
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderFingerprintConfiguration()` 创建Fingerprint配置信息 Create Fingerprint config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderInfraredConfiguration()` 创建红外配置信息 Create infrared config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderLFConfiguration()` 创建低频配置信息 Create LF config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderPrinterConfiguration()` 创建打印机配置信息 Create printer config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderRFIDConfiguration()` 创建RFID配置信息 Create RFID config infor.
    `static DeviceConfiguration_mtk` | DeviceConfiguration_mtk.`builderUHFConfiguration()` 创建UHF配置信息 Create UHF config infor.

  - ### Uses of ConfigurationException in com.rscja.team.mtk.deviceapi

    Methods in com.rscja.team.mtk.deviceapi that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithUHFUART_mtk` | RFIDWithUHFUART_mtk.`getInstance()` 获取UHF操作实例 Acquire UHF operation Instance
    `static RFIDWithISO15693_mtk` | RFIDWithISO15693_mtk.`getInstance()` 获取ISO15693协议操作实例 Acquire ISO15693 protocol operation Instance
    `static RFIDWithISO14443B_mtk` | RFIDWithISO14443B_mtk.`getInstance()` 获取ISO14443B协议操作实例 Acquire ISO14443B protocol operation Instance
    `static RFIDWithISO14443A_mtk` | RFIDWithISO14443A_mtk.`getInstance()` 获取ISO14443A协议操作实例 Acquire ISO14443A protocol operation Instance
    `static RFIDWithISO14443A4CPU_mtk` | RFIDWithISO14443A4CPU_mtk.`getInstance()` 获取ISO14443A CPU卡协议操作实例 Acquire ISO14443A CPU card protocol operation example
    `static Printer_mtk` | Printer_mtk.`getInstance()` 获取打印机模块操作实例 Acquire printer module operation Instance
    `static Infrared_mtk` | Infrared_mtk.`getInstance()`
    `static FingerprintWithTLK1NC_mtk` | FingerprintWithTLK1NC_mtk.`getInstance()`
    `static FingerprintWithMorpho_mtk` | FingerprintWithMorpho_mtk.`getInstance()` 获取指纹模块操作实例 acquire fingerprint module operation eample
    `static Barcode2D_mtk` | Barcode2D_mtk.`getInstance()` 获取二维条码操作实例 * Acquire 2D barcode operation Instance.
    `static Barcode1D_mtk` | Barcode1D_mtk.`getInstance()` 获取一维条码操作实例 Acquire 1D barcode operation Instance.

  - ### Uses of ConfigurationException in com.rscja.team.qcom

    Methods in com.rscja.team.qcom that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builder1DConfiguration()` 创建一维条码配置信息 Create 1D barcode config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builder2DConfiguration()` 创建二维条码配置信息 Create 2D barcode config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderA8ExtendedUartConfiguration()` 创建A8扩展串口配置信息
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderBDConfiguration()` 创建北斗配置信息 Create Beidou config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderDefaultConfiguration()`
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderFingerprintConfiguration()` 创建Fingerprint配置信息 Create Fingerprint config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderInfraredConfiguration()` 创建红外配置信息 Create infrared config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderLFConfiguration()` 创建低频配置信息 Create LF config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderPrinterConfiguration()` 创建打印机配置信息 Create printer config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderRFIDConfiguration()` 创建RFID配置信息 Create RFID config infor.
    `static DeviceConfiguration_qcom` | DeviceConfiguration_qcom.`builderUHFConfiguration()` 创建UHF配置信息 Create UHF config infor.

  - ### Uses of ConfigurationException in com.rscja.team.qcom.custom

    Methods in com.rscja.team.qcom.custom that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithUHFUARTUAE_qcom` | RFIDWithUHFUARTUAE_qcom.`getInstance()`
    `static RFIDWithUHFShuangYingDianZi_qcom` | RFIDWithUHFShuangYingDianZi_qcom.`getInstance()`

  - ### Uses of ConfigurationException in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi that throw ConfigurationException
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithUHFUART_qcom` | RFIDWithUHFUART_qcom.`getInstance()` 获取UHF操作实例 Acquire UHF operation Instance
    `static RFIDWithUHFA4_qcom` | RFIDWithUHFA4_qcom.`getInstance()`
    `static RFIDWithLF_qcom` | RFIDWithLF_qcom.`getInstance()` 获取RFID低频操作实例 Acquire RFID LF operation Instance
    `static RFIDWithISO15693_qcom` | RFIDWithISO15693_qcom.`getInstance()` 获取ISO15693协议操作实例 Acquire ISO15693 protocol operation Instance
    `static RFIDWithISO14443B_qcom` | RFIDWithISO14443B_qcom.`getInstance()` 获取ISO14443B协议操作实例 Acquire ISO14443B protocol operation Instance
    `static RFIDWithISO14443A_qcom` | RFIDWithISO14443A_qcom.`getInstance()` 获取ISO14443A协议操作实例 Acquire ISO14443A protocol operation Instance
    `static RFIDWithISO14443A4CPU_qcom` | RFIDWithISO14443A4CPU_qcom.`getInstance()` 获取ISO14443A CPU卡协议操作实例 Acquire ISO14443A CPU card protocol operation example
    `static FingerprintWithZAZ_qcom` | FingerprintWithZAZ_qcom.`getInstance()` 获取指纹模块操作实例 acquire fingerprint module operation eample
    `static FingerprintWithTLK1NC_qcom` | FingerprintWithTLK1NC_qcom.`getInstance()`
    `static CardWithBYL_qcom` | CardWithBYL_qcom.`getInstance()` 获取RFID低频操作实例