A B C D E F G H I J K L M N O P Q R S T U V W X Z

## R

R - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
R1HFAndPsamManage - Class in com.rscja.deviceapi
  R1设备高频和PSAM操作类
  R1 device HF and PSAM operation interfaces
  第一步:通过`R1HFAndPsamManage.connect(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`R1HFAndPsamManage.connect(Context context)`
  第二步:获取相关接口对象`R1HFAndPsamManage.getHF14443A()`、`R1HFAndPsamManage.getHF14443B()`、`R1HFAndPsamManage.getHF15693()`、`R1HFAndPsamManage.getPSAM()`
  Step 2:Gets the associated interface object `R1HFAndPsamManage.getHF14443A()`、`R1HFAndPsamManage.getHF14443B()`、`R1HFAndPsamManage.getHF15693()`、`R1HFAndPsamManage.getPSAM()`
  Example Usage:
  public void HFDemo() {   R1HFAndPsamManage rfid = R1HFAndPsamManage.getInstance();   if (!rfid.connect(context)) {    //fail    return;   }   IHF14443A ihf14443A = rfid.getHF14443A();   IHF14443B ihf14443B = rfid.getHF14443B();   IHF15693 ihf15693 = rfid.getHF15693();   IPSAM ipsam = rfid.getPSAM();   HF14443RequestEntity entity = ihf14443A.requestTypeA();   if (entity == null) {    //"Card not found!"    return;   }   byte cMode = 0x60:A ; 0x61:B   byte cBlock;   byte[] txtKey;//6bytes   boolean reuslt = ihf14443A.authentication(cMode, cBlock, txtKey);   if (!reuslt) {    //The key validation fail    return;   }   //................
R1HFUSB - Class in com.rscja.team.qcom.usb
R1HFUSB() - Constructor for class com.rscja.team.qcom.usb.R1HFUSB
R2000_FreHopSet(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
R2000_FreHopSet(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
R2000_OPENMODE() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
R2000_OPENMODE() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RadarLocationEntity - Class in com.rscja.deviceapi.entity
  回调数据实体类型 (Callback data entity type)
RadarLocationEntity() - Constructor for class com.rscja.deviceapi.entity.RadarLocationEntity
RadarLocationEntity.Builder - Class in com.rscja.deviceapi.entity
  标签实体构造器 (Constructor for label entities)
rats() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A4CPU
  CPU卡RATS操作指令
  CPU card RATS operation command
rats() - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡RATS操作指令
  CPU card RATS operation command
rats() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A4CPU_mtk
  CPU卡RATS操作指令
  CPU card RATS operation command
rats() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A4CPU_qcom
  CPU卡RATS操作指令
  CPU card RATS operation command
ratsTypeA() - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  CPU卡RATS操作指令(CPU card RATS operation command)
ratsTypeA() - Method in class com.rscja.team.qcom.r1.hf.HF14443A
  CPU卡RATS操作指令(CPU card RATS operation command)
read(HF15693RequestEntity, int) - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  读卡(Read card)
read(String, RFIDWithISO14443A.KeyType, int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读卡,此函数包含寻卡和验证密钥步骤
  Read card, this formula includes card search and key verfication procedure
read(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读卡，适用于Urltra light标签
  card reading, used for Urltra light tag
read(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  读取块数据
  read block data
read(ISO15693Entity, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
read(int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  读取块数据
  block data
read(String, RFIDWithISO14443A.KeyType, int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡,此函数包含寻卡和验证密钥步骤
  Read card, this formula includes card search and key verfication procedure
read(int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡，适用于Urltra light标签
  card reading, used for Urltra light tag
read(ISO15693Entity, int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
read(int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读取块数据
  read block data
read(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读取块数据
  block data
read(String, RFIDWithISO14443A.KeyType, int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  读卡,此函数包含寻卡和验证密钥步骤
  Read card, this formula includes card search and key verfication procedure
read(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  读卡，适用于Urltra light标签
  card reading, used for Urltra light tag
read(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
  读取块数据
  read block data
read(ISO15693Entity, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
read(int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO15693_mtk
  读取块数据
  block data
read(String, RFIDWithISO14443A.KeyType, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  读卡,此函数包含寻卡和验证密钥步骤
  Read card, this formula includes card search and key verfication procedure
read(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  读卡，适用于Urltra light标签
  card reading, used for Urltra light tag
read(ISO15693Entity, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
read(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
  读取块数据
  read block data
read(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO15693_qcom
  读取块数据
  block data
read(HF15693RequestEntity, int) - Method in class com.rscja.team.qcom.r1.hf.HF15693
  读卡(Read card)
read(byte[], int) - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Reads as many bytes as possible into the destination buffer.
read(byte[], int) - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
readAllData(String, RFIDWithISO14443A.TagType) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读卡，读取卡片所有块中的数据
  Card reading, read data of all blocks in the card
readAllData(String, RFIDWithISO14443A.TagType) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡，读取卡片所有块中的数据
  Card reading, read data of all blocks in the card
readAllData(String, RFIDWithISO14443A.TagType) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  读卡，读取卡片所有块中的数据
  Card reading, read data of all blocks in the card
readAllData(String, RFIDWithISO14443A.TagType) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  读卡，读取卡片所有块中的数据
  Card reading, read data of all blocks in the card
readAnimalTags(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取动物标签信息
  read animal tag infor
readAnimalTags(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读取动物标签信息
  read animal tag infor
readAnimalTags(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  读取动物标签信息
  read animal tag infor
readAuthenticationTagFromBuffer(UHFTAGInfo) - Method in class com.rscja.custom.UHFCSYX_A4NetWork
readAuthenticationTagFromBuffer(UHFTAGInfo) - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
readAuthenticationTagFromBuffer(UHFTAGInfo) - Method in class com.rscja.team.qcom.custom.UHFCSYX_qcom
readBlock(byte) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  读卡(Read card)
readBlock(byte) - Method in class com.rscja.team.qcom.r1.hf.HF14443A
  读卡(Read card)
readBuffData(byte[]) - Method in class com.rscja.team.qcom.serialportapi.SerialPort
readCalibrationData(String, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFJieCe
  读取 Calibration Data
readCalibrationData(String, int, int) - Method in class com.rscja.custom.RFIDWithUHFJieCe
  读取 Calibration Data
readCalibrationData(String, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
  读取 Calibration Data
readCameraState() - Static method in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
  Deprecated.
readCameraStateNew() - Method in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
  读取摄像头工作状态
readCharacteristic(BluetoothGattCharacteristic) - Method in class com.rscja.team.qcom.service.BLEService_qcom
readChipSN() - Method in class com.rscja.deviceapi.Fingerprint
  获取芯片序列号
  acquire chip serial number
readChipSN() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取芯片序列号
  acquire chip serial number
readChipSN() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  获取芯片序列号
  acquire chip serial number
readData(String, int, int, int) - Method in class com.rscja.deviceapi.BleDevice
  读取标签数据
  Read tag data
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.BleDevice
  读取指定标签数据
  Read specific tag data
readData(String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
readData(String, int, int, int, String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
readData(String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
readData(String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
readData(String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取标签数据
  Read tag data
readData(String, int, int, int, String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取指定标签数据
  Read specific tag data
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
readData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取标签数据
  Read tag data
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取指定标签数据
  Read specific tag data
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
readData(String, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
readData(String, int, int, int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
readData(String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  读取标签数据
  Read tag data
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  读取指定标签数据
  Read specific tag data
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
readData(String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
readDataWith4305Card(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读4305卡的某一页（0~31）数据
  read card 4305 data of random page (0-31)
readDataWith4305Card(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读4305卡的某一页（0~31）数据
  read card 4305 data of random page (0-31)
readDataWith4305Card(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  读4305卡的某一页（0~31）数据
  read card 4305 data of random page (0-31)
readDataWithHitagS(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取Hitag S卡中的某一页的数据
  Read data of random page in Hitag S card
readDataWithHitagS(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读取Hitag S卡中的某一页的数据
  Read data of random page in Hitag S card
readDataWithHitagS(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  读取Hitag S卡中的某一页的数据
  Read data of random page in Hitag S card
readDataWithIDCard(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读卡,用于ID卡
  card reading, used for ID card
readDataWithIDCard(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读卡,用于ID卡
  card reading, used for ID card
readDataWithIDCard(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  读卡,用于ID卡
  card reading, used for ID card
ReaderIPEntity - Class in com.rscja.deviceapi.entity
ReaderIPEntity() - Constructor for class com.rscja.deviceapi.entity.ReaderIPEntity
ReaderIPEntity(String, int) - Constructor for class com.rscja.deviceapi.entity.ReaderIPEntity
readFile(String) - Static method in class com.rscja.team.mtk.utility.FileUtils
  读取文件内容
readFlashlightStateNew() - Method in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
readMacSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
ReadMTKScanType() - Static method in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
readMultipleTemperature(int, int, int, String, int, int) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
readMultipleTemperature(int, int) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
readMultipleTemperature(int, int, int, String, int, int) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
  读取多个温度值
readMultipleTemperature(int, int) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
  读取多个温度值
readMultipleTemperature(int, int, int, String, int, int) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
readMultipleTemperature(int, int) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
readMultipleTemperature(int, int, int, String, int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
readMultipleTemperature(int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
readMultipleTemperature(int, int, int, String, int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
readMultipleTemperature(int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
readMultipleTemperatureRequest(int, int, int, byte[], int, int) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
readMultipleTemperatureRequest(int, int, int, byte[], int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
readMultipleTemperatureResponse(byte[], int[], int[], float[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
readMultipleTemperatureResponse(byte[], int[], int[], float[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
readOnChipRSSI(String, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFJieCe
  读取 On-Chip RSSI
readOnChipRSSI(String, int, int) - Method in class com.rscja.custom.RFIDWithUHFJieCe
  读取 On-Chip RSSI
readOnChipRSSI(String, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
  读取 On-Chip RSSI
readOnChipRSSIAndTempCode(String, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFJieCe
  读取 On-Chip RSSI+ Temp Code
readOnChipRSSIAndTempCode(String, int, int) - Method in class com.rscja.custom.RFIDWithUHFJieCe
  读取 On-Chip RSSI+ Temp Code
readOnChipRSSIAndTempCode(String, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
  读取 On-Chip RSSI+ Temp Code
readSensorCode(String, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFJieCe
  读取 Sensor Code
readSensorCode(String, int, int) - Method in class com.rscja.custom.RFIDWithUHFJieCe
  读取 Sensor Code
readSensorCode(String, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
  读取 Sensor Code
readSysPara() - Method in class com.rscja.deviceapi.Fingerprint
  获取系统参数，仅返回版本号
  Acquire system parameter, return version number only
readSysPara() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取系统参数，仅返回版本号
  Acquire system parameter, return version number only
readSysPara() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  获取系统参数，仅返回版本号
  Acquire system parameter, return version number only
readSysParaMore() - Method in class com.rscja.deviceapi.Fingerprint
  获取系统参数
  Acquire system parameter
readSysParaMore() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取系统参数
  Acquire system parameter
readSysParaMore() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  获取系统参数
  Acquire system parameter
readTagEPCAndTamperAlarm(boolean) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFUARTUAE
readTagEPCAndTamperAlarm(boolean) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
readTagFromBuffer() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFShuangYingDianZi
readTagFromBuffer() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFUARTUAE
  同时获取EPC和Tamper Alarm数值
  read return tag info.
readTagFromBuffer() - Method in class com.rscja.custom.UHFXSAPI
readTagFromBuffer() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  Deprecated.
readTagFromBuffer() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
readTagFromBuffer() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
readTagFromBuffer() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
  同时获取EPC和Tamper Alarm数值
  read return tag info.
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
  * Deprecated.
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  获取缓冲区的标签数据
  Get tag data from buffer
  `RFIDWithUHFUrxUart_qcom.startInventoryTag()`启动识别标签之后，在子线程循环调用此函数不断获取缓冲区的标签信息，每次返回一张标签数据
  `RFIDWithUHFUrxUart_qcom.startInventoryTag()` After tag reading has been enabled, call this function in sub threads to get data information continously, return one tag information for each time.
  在调用`RFIDWithUHFUrxUart_qcom.stopInventory()`之后，应当退出子线程。
  After call `RFIDWithUHFUrxUart_qcom.stopInventory()`, exit sub threads.
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
readTagFromBuffer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
readTagFromBufferList() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  Deprecated.
readTagFromBufferList() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  Deprecated.
readTagFromBufferList() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  Deprecated.
readTagFromBufferList() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
readTagFromBufferList() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
readTagFromBufferList() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
readTagFromBufferList() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
  获取缓冲区的标签数据
  Acquire tag data in buffer
  `RFIDWithUHFBLE_qcom.startInventoryTag()`启动识别标签之后，在子线程循环调用此函数不断获取缓冲区的标签信息，此函数只返回EPC数据
  `RFIDWithUHFBLE_qcom.startInventoryTag()` after enable identify tag, acquire tag information in buffer by this function in sub thread, this fucntion will return EPC data only
  在调用`RFIDWithUHFBLE_qcom.stopInventory()`之后，应当退出子线程。
  after call `RFIDWithUHFBLE_qcom.stopInventory()`, exit sub tread.
  备注： 读写器主板版 2.20-2.29 此函数支持输出Rssi,不需要调用readTagFromBufferList_EpcTidUser
readTagFromBufferList() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
readTagFromBufferList_EpcTidUser() - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
  Deprecated.
readTagFromBufferList_EpcTidUser() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  Deprecated.
readTagFromBufferList_EpcTidUser() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
readTagFromBufferList_EpcTidUser() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
readTagFromBufferList_EpcTidUser() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
  获取缓冲区的标签数据
readTagFromBufferList_EpcTidUser() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
  Deprecated.
readTagTemp(int, int, int, String, float[]) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
readTagTemp(int, int, int, String, float[]) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
readTagTemp(int, int, int, String, float[]) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
readTagTemp(int, int, int, String, float[]) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
readTagTemp(int, int, int, String, float[]) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
readTagTempRequest(char, int, int, byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
readTagTempRequest(char, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
readTagTempResponse(byte[], float[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
readTagTempResponse(byte[], float[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
readTagVoltage(int, int, int, String, float[]) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
readTagVoltage(float[]) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
readTagVoltage(int, int, int, String, float[]) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
  读取多个温度值
readTagVoltage(float[]) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
  读取多个温度值
readTagVoltage(int, int, int, String, float[]) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
readTagVoltage(float[]) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
readTagVoltage(int, int, int, String, float[]) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
readTagVoltage(float[]) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
readTagVoltage(int, int, int, String, float[]) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
readTagVoltage(float[]) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
readTagVoltageRequest(int, int, int, byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
readTagVoltageRequest(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
readTagVoltageResponse(byte[], float[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
readTagVoltageResponse(byte[], float[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
readTamperTagFromBuffer() - Method in interface com.rscja.custom.interfaces.IUHFTamperAPI
readTamperTagFromBuffer() - Method in class com.rscja.custom.UHFTamperAPI
readTamperTagFromBuffer() - Method in class com.rscja.team.qcom.custom.UHFTamperAPI_qcom
readTcpServiceState() - Method in class com.rscja.deviceapi.UhfBase
readTempertureCode(String, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFJieCe
  读取 Temperture Code
readTempertureCode(String, int, int) - Method in class com.rscja.custom.RFIDWithUHFJieCe
  读取 Temperture Code
readTempertureCode(String, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFJieCe_qcom
  读取 Temperture Code
readUnsignedInt64(byte[]) - Static method in class com.rscja.utility.StringUtility
  读取无符号位的长整数，64位
readWithNeedleTag() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读数据，针对针管标签
  read data, for needle tube tag
readWithNeedleTag() - Method in class com.rscja.deviceapi.RFIDWithLF
  读数据，针对针管标签
  read data, for needle tube tag
readWithNeedleTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  读数据，针对针管标签
  read data, for needle tube tag
readXmlList() - Static method in class com.rscja.team.mtk.utility.FileUtils
readyUpgradeTcpService() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
rebootDevice() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  重启设备
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  重启设备
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  重启设备
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  重启设备
receive(byte[]) - Method in interface com.rscja.deviceapi.BluetoothReader.OnDataChangeListener
receive() - Method in class com.rscja.deviceapi.Infrared
  接收数据
  Receive data
receive() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  接收数据
  Receive data
receive() - Method in interface com.rscja.deviceapi.interfaces.IModule
  接收数据,读取串口数据会等待1秒钟
  Receive data
receive() - Method in class com.rscja.deviceapi.Module
  接收数据,读取串口数据会等待1秒钟
  Receive data
receive() - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  接收数据
  Receive data
receive() - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  接收数据,读取串口数据会等待1秒钟
  Receive data
receive(HardwareInterface_qcom.FunctionEnum) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  接收数据,读取串口数据
  Receive data
receive(int) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  接收数据,读取串口数据
  Receive data
receive() - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  接收数据,读取串口数据会等待1秒钟
  Receive data
receive() - Method in class com.rscja.team.qcom.socket.SocketTcpIpBase
receive() - Method in class com.rscja.team.qcom.socket.SocketUdpClient
receiveBTData(byte[]) - Method in interface com.rscja.team.qcom.service.BLEService_qcom.IDataCallBack
receiveBytes() - Method in class com.rscja.team.qcom.serialportapi.SerialportAPI
receiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  接收串口数据
  receive serial port data
receiveData(byte[]) - Method in class com.rscja.deviceapi.Printer
  接收串口数据
  receive serial port data
receiveData(byte[]) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  接收串口数据
  receive serial port data
receiveData() - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
receiveData() - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
receiveData() - Method in class com.rscja.team.qcom.socket.SocketManageA4
receiveEx() - Method in interface com.rscja.deviceapi.interfaces.IModule
  接收数据,读取串口数据无等待时间
  Receive data
receiveEx() - Method in class com.rscja.deviceapi.Module
  接收数据,读取串口数据无等待时间
  Receive data
receiveEx() - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  接收数据,读取串口数据无等待时间
  Receive data
receiveEx() - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  接收数据,读取串口数据无等待时间
  Receive data
receiveGPIOData() - Method in class com.rscja.team.qcom.socket.SocketManageA4
receiveOnThread() - Method in class com.rscja.team.qcom.socket.SocketTcpIpBase
receiveOnThread(int) - Method in class com.rscja.team.qcom.socket.SocketTcpIpBase
receiveOnThread() - Method in class com.rscja.team.qcom.socket.SocketUdpClient
receiveOnThread(int) - Method in class com.rscja.team.qcom.socket.SocketUdpClient
receiveTagData() - Method in class com.rscja.team.qcom.socket.SocketManageA4
registerReceiver(Context, OnLowBatteryListener, IUHF) - Method in class com.rscja.team.mtk.utility.BatteryManage
regModel() - Method in class com.rscja.deviceapi.Fingerprint
  合并特征文件。将模板缓冲区1与模板缓冲区2中的模板文件合并生成模板，结果存于模板缓冲区1。
  Combine feature file.
regModel() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  合并特征文件。将模板缓冲区1与模板缓冲区2中的模板文件合并生成模板，结果存于模板缓冲区1。
  Combine feature file.
regModel() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  合并特征文件。将模板缓冲区1与模板缓冲区2中的模板文件合并生成模板，结果存于模板缓冲区1。
  Combine feature file.
releasePrinterGpio() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
releasePrinterGpio() - Method in class com.rscja.deviceapi.Printer
releasePrinterGpio() - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
removeBleDevice(String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
  移除蓝牙设备
removeLiveAPP(String[]) - Method in interface com.rscja.system.ISystemInterfaces
  移除保活APP
request() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  寻卡
  Search card
request() - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  寻卡
  Search card
request() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  寻卡
  Search card
request() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  寻卡
  Search card
request15693() - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  寻卡(Search card)
request15693() - Method in class com.rscja.team.qcom.r1.hf.HF15693
  寻卡(Search card)
Request_WriteSpecialPart(int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Request_WriteSpecialPart(int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
requestGetBeepSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
requestGetEx10SDKFirmware() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
requestGetEx10SDKFirmware() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
requestGetFastInventoryMode() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
requestGetFastInventoryMode() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
requestInventoryTempTag(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
requestSetFastInventoryMode(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
requestSetFastInventoryMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
requestTypeA() - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  寻卡(Search card)
requestTypeA(int) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  寻卡(Search card)
requestTypeA() - Method in class com.rscja.team.qcom.r1.hf.HF14443A
  寻卡(Search card)
requestTypeA(int) - Method in class com.rscja.team.qcom.r1.hf.HF14443A
  寻卡(Search card)
Requset_ReadPart(byte, byte, byte, byte, byte, byte) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Requset_ReadPart(byte, byte, byte, byte, byte, byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Requset_WritePart(byte[], byte, byte, byte, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Requset_WritePart(byte[], byte, byte, byte, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
reset() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A4CPU
  CPU卡复位操作指令
  CPU card reset operation command
reset() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443B
  CPU卡复位操作指令
  CPU card reset operation commande
reset() - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡复位操作指令
  CPU card reset operation command
reset() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  CPU卡复位操作指令
  CPU card reset operation commande
reset() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A4CPU_mtk
  CPU卡复位操作指令
  CPU card reset operation command
reset() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443B_mtk
  CPU卡复位操作指令
  CPU card reset operation commande
reset() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A4CPU_qcom
  CPU卡复位操作指令
  CPU card reset operation command
reset() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443B_qcom
  CPU卡复位操作指令
  CPU card reset operation commande
reset(byte) - Method in interface com.rscja.team.qcom.r1.IPSAM
  重置PSAM卡(reset smart card )
reset(byte) - Method in class com.rscja.team.qcom.r1.psam.PSAM
  重置PSAM卡(reset smart card )
resetScan(Context) - Method in interface com.rscja.scanner.IScanner
  键盘助手恢复出厂设置
  Restore factory setup
resetScan(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
resetScan(Context) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
resetScan(Context) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
resetTypeB() - Method in interface com.rscja.deviceapi.interfaces.IHF14443B
  寻卡(Search card)
resetTypeB() - Method in class com.rscja.team.qcom.r1.hf.HF14443B
  寻卡(Search card)
responseCancel() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  取消当前操作
  Cancel current operation
responseCancel() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  取消当前操作
  Cancel current operation
responseCancel() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  取消当前操作
  Cancel current operation
responseCancel() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  取消当前操作
  Cancel current operation
responseContinue() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  继续当前操作
  Continue current operation
responseContinue() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  继续当前操作
  Continue current operation
responseContinue() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  继续当前操作
  Continue current operation
responseContinue() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  继续当前操作
  Continue current operation
responseGetEx10SDKFirmware(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
responseGetEx10SDKFirmware(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
responseGetFastInventoryMode(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
responseGetFastInventoryMode(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
responseSetFastInventoryMode(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
responseSetFastInventoryMode(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
respparseBeepData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
restoreDefault() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  参数还原默认值
  parameter reset to default
restoreDefault() - Method in class com.rscja.deviceapi.Printer
  参数还原默认值
  parameter reset to default
restoreDefault() - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  参数还原默认值
  parameter reset to default
RESULT_STATUS - Static variable in class com.rscja.barcode.ConstantUtil
ResultData() - Constructor for class com.rscja.deviceapi.entity.InventoryParameter.ResultData
reverse(byte[]) - Static method in class com.rscja.utility.StringUtility
  逆转字节数组
RF_ISO14443A_DESFIRE_AddApp(char[], int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_AddApp(char[], int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_AddStdFile(int, int, char[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_AddStdFile(int, int, char[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_AddValueFile(int, int, char[], int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_AddValueFile(int, int, char[], int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_Auth(int, char[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_Auth(int, char[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ChangeFileSetting(int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ChangeFileSetting(int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ChangeKey(int, char[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ChangeKey(int, char[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ChangeKeySetting(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ChangeKeySetting(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_Cpysel(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_Cpysel(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_CreditValueFile(int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_CreditValueFile(int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_DebitValueFile(int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_DebitValueFile(int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_DelApp(char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_DelApp(char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_DelFile(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_DelFile(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_FormatCard() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_FormatCard() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetApps() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetApps() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetFileIds() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetFileIds() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetFileSetting(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetFileSetting(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetKeySetting() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetKeySetting() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetPiccInfo() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetPiccInfo() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetValueFile(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_GetValueFile(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_RatPss() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_RatPss() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ReadStdFile(int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_ReadStdFile(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_SelApp(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_SelApp(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_WriteStdFile(int, int, int, char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RF_ISO14443A_DESFIRE_WriteStdFile(int, int, int, char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RFID_free(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  RFID_free 模块释放
RFID_free(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  RFID_free 模块释放
RFID_GetVer() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  RFID_GetVer 获取RFID模块硬件版本
RFID_GetVer() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  RFID_GetVer 获取RFID模块硬件版本
RFID_init(String, String, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  RFID_init 模块初始化
RFID_init(String, String, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  RFID_init 模块初始化
RFID_UPDATE(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
RFID_UPDATE(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
RFIDArgumentException - Exception in com.rscja.deviceapi.exception
  参数错误异常
  parameter err
RFIDArgumentException(String) - Constructor for exception com.rscja.deviceapi.exception.RFIDArgumentException
RFIDBase - Class in com.rscja.deviceapi
RFIDBase() - Constructor for class com.rscja.deviceapi.RFIDBase
RFIDBase_mtk - Class in com.rscja.team.mtk.deviceapi
RFIDBase_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDNotFoundException - Exception in com.rscja.deviceapi.exception
  寻卡失败异常
  card searching failed err
RFIDNotFoundException() - Constructor for exception com.rscja.deviceapi.exception.RFIDNotFoundException
RFIDReadFailureException - Exception in com.rscja.deviceapi.exception
  读卡失败异常
  card reading failure err
RFIDReadFailureException() - Constructor for exception com.rscja.deviceapi.exception.RFIDReadFailureException
rfidUpgrade(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
  固件升级
  firmware upgrade
rfidUpgrade(int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDBase
  固件升级
  firmware upgrade
rfidUpgrade(int, int, int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.RFIDBase_mtk
  固件升级
  firmware upgrade
rfidUpgrade(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDBase_qcom
  固件升级
  firmware upgrade
RFIDVerificationException - Exception in com.rscja.deviceapi.exception
  验证失败异常
  verify failure err
RFIDVerificationException() - Constructor for exception com.rscja.deviceapi.exception.RFIDVerificationException
RFIDWithISO14443A - Class in com.rscja.deviceapi
  RFID模块ISO14443A协议操作类
  RFID module ISO 14443A protocol operation type
RFIDWithISO14443A.DESFireEncryptionTypekEnum - Enum in com.rscja.deviceapi
  DESFire卡加密类型
  DESFire card encyption type
RFIDWithISO14443A.DESFireFileTypekEnum - Enum in com.rscja.deviceapi
  DESFire卡文件类型
  DESFire card file typr
RFIDWithISO14443A.KeyType - Enum in com.rscja.deviceapi
  密钥类型，适用于S50和S70标签。
  key type, used for S50 and S70 tags.
RFIDWithISO14443A.TagType - Enum in com.rscja.deviceapi
  M1标签类型定义
  M1 tag type definition
RFIDWithISO14443A4CPU - Class in com.rscja.deviceapi
  RFID模块ISO14443A CPU卡协议操作类
  RFID module ISO14443A CPU card protocol operation type
RFIDWithISO14443A4CPU_mtk - Class in com.rscja.team.mtk.deviceapi
  RFID模块ISO14443A CPU卡协议操作类
  RFID module ISO14443A CPU card protocol operation type
RFIDWithISO14443A4CPU_qcom - Class in com.rscja.team.qcom.deviceapi
  RFID模块ISO14443A CPU卡协议操作类
  RFID module ISO14443A CPU card protocol operation type
RFIDWithISO14443A_mtk - Class in com.rscja.team.mtk.deviceapi
  RFID模块ISO14443A协议操作类
  RFID module ISO 14443A protocol operation type
RFIDWithISO14443A_qcom - Class in com.rscja.team.qcom.deviceapi
  RFID模块ISO14443A协议操作类
  RFID module ISO 14443A protocol operation type
RFIDWithISO14443B - Class in com.rscja.deviceapi
  RFID模块ISO14443B协议操作类
  RFID module ISO14443B protocol operation type
RFIDWithISO14443B_mtk - Class in com.rscja.team.mtk.deviceapi
  RFID模块ISO14443B协议操作类
  RFID module ISO14443B protocol operation type
RFIDWithISO14443B_qcom - Class in com.rscja.team.qcom.deviceapi
  RFID模块ISO14443B协议操作类
  RFID module ISO14443B protocol operation type
RFIDWithISO15693 - Class in com.rscja.deviceapi
  RFID模块ISO15693协议操作类,
  RFID module ISO15639 protocol operation type
RFIDWithISO15693.TagType - Enum in com.rscja.deviceapi
  标签类型
  Tag type
RFIDWithISO15693_mtk - Class in com.rscja.team.mtk.deviceapi
  RFID模块ISO15693协议操作类,
  RFID module ISO15639 protocol operation type
RFIDWithISO15693_mtk.TagType - Enum in com.rscja.team.mtk.deviceapi
  标签类型
  Tag type
RFIDWithISO15693_qcom - Class in com.rscja.team.qcom.deviceapi
  RFID模块ISO15693协议操作类,
  RFID module ISO15639 protocol operation type
RFIDWithLF - Class in com.rscja.deviceapi
  RFID低频（125K）操作类
  RFID LF (125K) operation type
RFIDWithLF_qcom - Class in com.rscja.team.qcom.deviceapi
  RFID低频（125K）操作类
  RFID LF (125K) operation type
RFIDWithUHFA4 - Class in com.rscja.deviceapi
  UHF模块 A4操作类
  UHF module operation type
  第一步:通过`RFIDWithUHFA4.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFA4.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFA4.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFA4.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFA4.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFA4_qcom - Class in com.rscja.team.qcom.deviceapi
  UHF模块 A4操作类
  UHF module operation type
RFIDWithUHFA4NetWork - Class in com.rscja.deviceapi
  操作URA4设备以及UHF模块相关接口。(通过其他android设备控制A4)
  Operate URA4 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA4NetWork.setIPAndPort(String ip, int port)`设置要连接的IP地址, 再通过 `RFIDWithUHFA4NetWork.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA4NetWork.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA4NetWork.setIPAndPort(String ip, int port)`-> `RFIDWithUHFA4NetWork.init(Context context)`.
RFIDWithUHFA4NetWork() - Constructor for class com.rscja.deviceapi.RFIDWithUHFA4NetWork
RFIDWithUHFA4NetWork_qcom - Class in com.rscja.team.qcom.deviceapi
  操作URA4设备以及UHF模块相关接口。
  第一步：连接通过 `RFIDWithUHFAxNetWorkBase_qcom.setIPAndPort(String host, int port)`设置连接的读写IP地址。然后调用 `RFIDWithUHFA4NetWork_qcom.init(Context)`连接读写器。 同时可以设置回调接口 `RFIDWithUHFAxNetWorkBase_qcom.setConnectionStatusCallback(ConnectionStatusCallback)`监听连接状态
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数。
  如果是盘点标签先调用`RFIDWithUHFAxNetWorkBase_qcom.setInventoryCallback(IUHFInventoryCallback)`设置标签回调接口，标签数据会上传到这个接口函数。
  然后在调用`RFIDWithUHFAxNetWorkBase_qcom.startInventoryTag()`函数开始执行盘点。注意:在盘点标签的时候rfid模块只能响应`RFIDWithUHFAxNetWorkBase_qcom.stopInventory()`函数。
  第三步：退出app调用 `RFIDWithUHFA4NetWork_qcom.free()`断开连接，如果断开之前正在盘点，请先停止盘点，在断开连接。
RFIDWithUHFA4NetWork_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
RFIDWithUHFA4RS232 - Class in com.rscja.deviceapi
  操作URA4设备以及UHF模块相关接口。(通过其他android设备控制A4)
  Operate URA4 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA4RS232.setUart(String path)`设置要连接的IP地址, 再通过 `RFIDWithUHFA4RS232.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA4RS232.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA4RS232.setUart(String path)`-> `RFIDWithUHFA4RS232.init(Context context)`.
RFIDWithUHFA4RS232_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFA4RS232_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
RFIDWithUHFA8 - Class in com.rscja.deviceapi
  UHF模块 A8操作类
  UHF module operation type
  第一步:通过`RFIDWithUHFA8.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFA8.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFA8.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFA8.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFA8.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFA8_qcom - Class in com.rscja.team.qcom.deviceapi
  UHF模块 A8操作类
  UHF module operation type
RFIDWithUHFA8NetWork - Class in com.rscja.deviceapi
  操作URA8设备以及UHF模块相关接口。(通过其他android设备控制A8)
  Operate URA8 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA8NetWork.setIPAndPort(String ip, int port)`设置要连接的IP地址, 再通过 `RFIDWithUHFA8NetWork.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA8NetWork.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA8NetWork.setIPAndPort(String ip, int port)`-> `RFIDWithUHFA8NetWork.init(Context context)`.
RFIDWithUHFA8NetWork() - Constructor for class com.rscja.deviceapi.RFIDWithUHFA8NetWork
RFIDWithUHFA8NetWork_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFA8NetWork_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
RFIDWithUHFA8RS232 - Class in com.rscja.deviceapi
  操作URA8设备以及UHF模块相关接口。(通过其他android设备控制A8)
  Operate URA8 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA8RS232.setUart(String path)`设置要连接的IP地址, 再通过 `RFIDWithUHFA8RS232.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA8RS232.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA8RS232.setUart(String path)`-> `RFIDWithUHFA8RS232.init(Context context)`.
RFIDWithUHFA8RS232_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFA8RS232_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
RFIDWithUHFAxBase - Class in com.rscja.deviceapi
RFIDWithUHFAxBase_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFBLE - Class in com.rscja.deviceapi
  UHF模块低功耗蓝牙操作类
  UHF module operation type
RFIDWithUHFBLE_qcom - Class in com.rscja.team.qcom.deviceapi
  UHF模块低功耗蓝牙操作类
  UHF module operation type
RFIDWithUHFBLE_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
RFIDWithUHFBLEManage - Class in com.rscja.deviceapi
  BLE设备读写器管理类，支持一对多连接
  具体操作步骤:
  1.通过`RFIDWithUHFBLEManage.getInstance()` 函数获取 RFIDWithUHFBLEManage对象
  2.调用`RFIDWithUHFBLEManage.addBleDevice(String address, Context context)`添加BLE读写器设备，每个蓝牙地址作为设备的唯一标识
  3.通过`RFIDWithUHFBLEManage.getBleDeviceByMac(String address)` 函数获取每一台蓝牙设备的操作对象 `com.rscja.deviceapi.BleDevice`。
RFIDWithUHFBLEManage() - Constructor for class com.rscja.deviceapi.RFIDWithUHFBLEManage
RFIDWithUHFBLEN51() - Constructor for class com.rscja.custom.UHFTemperatureTag.RFIDWithUHFBLEN51
RFIDWithUHFBLEN51_qcom - Class in com.rscja.team.qcom.ble
RFIDWithUHFBLEN51_qcom() - Constructor for class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
RFIDWithUHFBLEN52() - Constructor for class com.rscja.custom.UHFTemperatureTag.RFIDWithUHFBLEN52
RFIDWithUHFBLEN52_qcom - Class in com.rscja.team.qcom.ble
RFIDWithUHFBLEN52_qcom() - Constructor for class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
RFIDWithUHFJieCe - Class in com.rscja.custom
RFIDWithUHFJieCe.TemperatureTagInfo - Class in com.rscja.custom
RFIDWithUHFJieCe_qcom - Class in com.rscja.team.qcom.custom
RFIDWithUHFRLM - Class in com.rscja.deviceapi
RFIDWithUHFRLM_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFShuangYingDianZi_qcom - Class in com.rscja.team.qcom.custom
RFIDWithUHFUART - Class in com.rscja.deviceapi
  UHF模块手持机，串口通信操作类
  UHF module handheld, serial communication operation interface
  第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFUART.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFUART.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUART_mtk - Class in com.rscja.team.mtk.deviceapi
RFIDWithUHFUART_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFUARTUAE_qcom - Class in com.rscja.team.qcom.custom
RFIDWithUHFUrxNetwork - Class in com.rscja.deviceapi
  UHF模块URx网口通信操作类
  URx network operation of UHF module
  第一步：先通过`RFIDWithUHFUrxNetwork.setIPAndPort(String ip, int port)`设置要连接的IP地址, 再通过 `RFIDWithUHFUrxNetwork.init(Context context)`连接读写器串口。 Step 1: Connect to the serial port of the reader via`RFIDWithUHFUrxNetwork.setIPAndPort(String ip, int port)`-> `RFIDWithUHFUrxNetwork.init(Context context)`.
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUrxNetwork.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUrxNetwork.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUrxNetwork() - Constructor for class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
RFIDWithUHFUrxNetwork_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFUrxNetwork_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
RFIDWithUHFUrxUart - Class in com.rscja.deviceapi
  URx 模块，串口通信操作类
  URx module , serial communication operation interface
  第一步:通过`RFIDWithUHFUrxUart.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUrxUart.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUrxUart.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUrxUart.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUrxUart2_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFUrxUart_qcom - Class in com.rscja.team.qcom.deviceapi
RFIDWithUHFUrxUsbToUart - Class in com.rscja.deviceapi
  URx 模块，串口通信操作类
  URx module , serial communication operation interface
  第一步:通过`RFIDWithUHFUrxUsbToUart.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUrxUsbToUart.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUrxUsbToUart.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUrxUsbToUart.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUrxUsbToUart_qcom - Class in com.rscja.team.qcom.deviceapi
  UR4 设备USB转串口,目前已经适配 pl2302芯片的usb转接线
RFIDWithUHFUSB - Class in com.rscja.deviceapi
  UHF模块手持机，USB通信操作类
  UHF module handheld, USB operation interface
  第一步:通过`RFIDWithUHFUSB.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUSB.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUSB.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUSB.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUSB_qcom - Class in com.rscja.team.qcom.deviceapi
RK - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
RKURA4C8Device - Class in com.rscja.team.qcom.urax
RKURA4C8Device() - Constructor for class com.rscja.team.qcom.urax.RKURA4C8Device
RKURA4Gpio - Class in com.rscja.team.qcom.urax
RKURA4Gpio() - Constructor for class com.rscja.team.qcom.urax.RKURA4Gpio
RKURAxDevice - Class in com.rscja.team.qcom.urax
RKURAxDevice() - Constructor for class com.rscja.team.qcom.urax.RKURAxDevice
RX_CHAR_UUID - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
RX_SERVICE_UUID - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
RxUsb_qcom - Class in com.rscja.team.qcom.usb
RxUsb_qcom(UsbBase_qcom) - Constructor for class com.rscja.team.qcom.usb.RxUsb_qcom

A B C D E F G H I J K L M N O P Q R S T U V W X Z