## Uses of Interface
com.rscja.deviceapi.interfaces.IUHFLocationCallback

- Packages that use IUHFLocationCallback
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.mtk.deviceapi |
  com.rscja.team.qcom.ble |
  com.rscja.team.qcom.deviceapi |

- - ### Uses of IUHFLocationCallback in com.rscja.deviceapi

    Methods in com.rscja.deviceapi with parameters of type IUHFLocationCallback
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFUSB.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`
    `boolean` | RFIDWithUHFBLE.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)` 开始定位 Start location
    `boolean` | RFIDWithUHFUART.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)` 开始定位 Start location
    `boolean` | BleDevice.`startLocation(java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)` 开始定位

  - ### Uses of IUHFLocationCallback in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces with parameters of type IUHFLocationCallback
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | IHandheldRFID.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`
    `boolean` | IBleDevice.`startLocation(java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`

  - ### Uses of IUHFLocationCallback in com.rscja.team.mtk.deviceapi

    Methods in com.rscja.team.mtk.deviceapi with parameters of type IUHFLocationCallback
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFUART_mtk.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)` 开始定位 Start location

  - ### Uses of IUHFLocationCallback in com.rscja.team.qcom.ble

    Methods in com.rscja.team.qcom.ble with parameters of type IUHFLocationCallback
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFBLEN52_qcom.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`
    `boolean` | RFIDWithUHFBLEN51_qcom.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`
    `boolean` | EmptyUhfBle.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`

  - ### Uses of IUHFLocationCallback in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi with parameters of type IUHFLocationCallback
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFUSB_qcom.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`
    `boolean` | RFIDWithUHFUART_qcom.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)` 开始定位 Start location
    `boolean` | RFIDWithUHFBLE_qcom.`startLocation(android.content.Context context, java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)` 开始定位 Start location
    `boolean` | UhfLocation_qcom.`startLocation(java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`
    `boolean` | BleDevice_qcom.`startLocation(java.lang.String label, int bank, int ptr, IUHFLocationCallback locationCallback)`