A B C D E F G H I J K L M N O P Q R S T U V W X Z

## F

F - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
factoryReset() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  还原出厂设置(Restore factory settings)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  还原出厂设置(Restore factory settings)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  还原出厂设置(Restore factory settings)
factoryReset() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  还原出厂设置(Restore factory settings)
factoryReset() - Method in class com.rscja.deviceapi.UhfBase
  恢复出厂设置(Reset uhf parameters)
FactoryReset() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
factoryReset() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  恢复出厂设置(Reset uhf parameters)
FactoryReset() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
factoryReset() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
  恢复出厂设置(Reset uhf parameters)
factoryReset() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
  还原出厂设置(Restore factory settings)
factoryReset() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
  还原出厂设置(Restore factory settings)
factoryReset() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
  还原出厂设置(Restore factory settings)
filePath - Static variable in class com.rscja.team.mtk.utility.FileUtils
FileUtility - Class in com.rscja.utility
FileUtility() - Constructor for class com.rscja.utility.FileUtility
FileUtils - Class in com.rscja.team.mtk.utility
  Created by Administrator on 2017-5-22.
FileUtils() - Constructor for class com.rscja.team.mtk.utility.FileUtils
filterCharacter(Context, String) - Method in class com.rscja.barcode.BarcodeUtility
  过滤字符串 Filter charactor string
filterCharacter(Context, String) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  过滤字符串 Filter charactor string
filterCharacter(Context, String) - Method in interface com.rscja.scanner.IScanner
  过滤字符串
  Filter string
filterCharacter(Context, String) - Method in class com.rscja.scanner.utility.ScannerUtility
filterCharacter(Context, String) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  过滤字符串 Filter charactor string
filterCharacter(Context, String) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
filterCharacter(Context, String) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  过滤字符串 Filter charactor string
filterCharacter(Context, String) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
finalZ - Variable in class com.rscja.team.qcom.utility.GyroAngle
fingerCLEARTemplate() - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  清空FLASH中指纹模板
fingerCLEARTemplate() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  清空FLASH中指纹模板
fingerCLEARTemplate() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  清空FLASH中指纹模板
fingerCLEARTemplate() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  清空FLASH中指纹模板
fingerCLEARTemplateBuffer() - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  清空指纹特征缓冲区
fingerCLEARTemplateBuffer() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  清空指纹特征缓冲区
fingerCLEARTemplateBuffer() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  清空指纹特征缓冲区
fingerCLEARTemplateBuffer() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  清空指纹特征缓冲区
fingerDELTemplateBufferID(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  删除内存中指定的模板
fingerDELTemplateBufferID(FingerprintWithTLK1NC.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  删除内存中指定的模板
fingerDELTemplateBufferID(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  删除内存中指定的模板
fingerDELTemplateBufferID(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  删除内存中指定的模板
fingerDELTemplatePageID(int) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  删除FLASH中指定的模板
fingerDELTemplatePageID(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  删除FLASH中指定的模板
fingerDELTemplatePageID(int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  删除FLASH中指定的模板
fingerDELTemplatePageID(int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  删除FLASH中指定的模板
fingerDOWNTemplateToBuffer(FingerprintWithTLK1NC.BufferEnum, byte[]) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  下载指纹特征到指定的特征缓冲区中
fingerDOWNTemplateToBuffer(FingerprintWithTLK1NC.BufferEnum, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  下载指纹特征到指定的特征缓冲区中
fingerDOWNTemplateToBuffer(FingerprintWithTLK1NC.BufferEnum, byte[]) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  下载指纹特征到指定的特征缓冲区中
fingerDOWNTemplateToBuffer(FingerprintWithTLK1NC.BufferEnum, byte[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  下载指纹特征到指定的特征缓冲区中
fingerDOWNTemplateToFlashPage(int, byte[]) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  下载指纹特征到指定的Flash Page中
fingerDOWNTemplateToFlashPage(int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  下载指纹特征到指定的Flash Page中
fingerDOWNTemplateToFlashPage(int, byte[]) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  下载指纹特征到指定的Flash Page中
fingerDOWNTemplateToFlashPage(int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  下载指纹特征到指定的Flash Page中
fingerGETImage() - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  从采集器采集指纹图像并保存于 ImageBuffer 中
fingerGETImage() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  从采集器采集指纹图像并保存于 ImageBuffer 中
fingerGETImage() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  从采集器采集指纹图像并保存于 ImageBuffer 中
fingerGETImage() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  从采集器采集指纹图像并保存于 ImageBuffer 中
fingerGETTemplateCount() - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  获取可存储的指纹模板数
fingerGETTemplateCount() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  获取可存储的指纹模板数
fingerGETTemplateCount() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  获取可存储的指纹模板数
fingerGETTemplateCount() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  获取可存储的指纹模板数
fingerGRABHalfImage() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
fingerGRABHalfImage() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
fingerGRABHalfImageProgress() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
fingerGRABHalfImageProgress() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
fingerGRABImage() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
fingerGRABImage() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
fingerPKTemplate(int, FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplate(int, FingerprintWithTLK1NC.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplate(int, FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplate(int, FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplate2(FingerprintWithTLK1NC.BufferEnum, int) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplate2(FingerprintWithTLK1NC.BufferEnum, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplate2(FingerprintWithTLK1NC.BufferEnum, int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplate2(FingerprintWithTLK1NC.BufferEnum, int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  精确比对指定特征缓冲区和指定的Flash Page中特征
fingerPKTemplateBuffer(FingerprintWithTLK1NC.BufferEnum, FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  精确比对指定特征缓冲区中特征
fingerPKTemplateBuffer(FingerprintWithTLK1NC.BufferEnum, FingerprintWithTLK1NC.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  精确比对指定特征缓冲区中特征
fingerPKTemplateBuffer(FingerprintWithTLK1NC.BufferEnum, FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  精确比对指定特征缓冲区中特征
fingerPKTemplateBuffer(FingerprintWithTLK1NC.BufferEnum, FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  精确比对指定特征缓冲区中特征
fingerPKTemplatePage(int, int) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  精确比对指定Flash Page中特征
fingerPKTemplatePage(int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  精确比对指定Flash Page中特征
fingerPKTemplatePage(int, int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  精确比对指定Flash Page中特征
fingerPKTemplatePage(int, int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  精确比对指定Flash Page中特征
Fingerprint - Class in com.rscja.deviceapi
  指纹识别模块操作类,
  Fingerprint identify module operation type
Fingerprint.BufferEnum - Enum in com.rscja.deviceapi
  模块缓冲区枚举
  Module buffer zone example.
Fingerprint_qcom - Class in com.rscja.team.qcom.deviceapi
  指纹识别模块操作类,
  Fingerprint identify module operation type
FingerprintAlreadyEnrolledException - Exception in com.rscja.deviceapi.exception
  指纹已经存在异常类
  fingerprint has exception type
FingerprintAlreadyEnrolledException() - Constructor for exception com.rscja.deviceapi.exception.FingerprintAlreadyEnrolledException
FingerprintInfo() - Constructor for class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
FingerprintInvalidIDException - Exception in com.rscja.deviceapi.exception
  ID已被占用异常类
  ID has been occupied exception type
FingerprintInvalidIDException() - Constructor for exception com.rscja.deviceapi.exception.FingerprintInvalidIDException
FingerprintPictureUtility - Class in com.rscja.utility
FingerprintPictureUtility() - Constructor for class com.rscja.utility.FingerprintPictureUtility
FingerprintSM206B - Class in com.rscja.deviceapi
  SM206B 指纹模块操作接口
  第一步:调用init(Context context) 函数初始化指纹模块
  第二步:调用指纹相关接口,比如：search()，getDeviceVersion()...
  第三步:调用free()释放指纹模块相关资源
  示例代码:
  public void Test() {
  Context context;
  FingerprintSM206B fingerprintSM206B= FingerprintSM206B.getInstance();
  boolean result= fingerprintSM206B.init(context);
  if(!result){
  //init fail
  return;
  }
  fingerprintSM206B.getImage();
  fingerprintSM206B.getFingerTemplate();
  fingerprintSM206B.getDeviceVersion();
  //...........
FingerprintSM206B_qcom - Class in com.rscja.team.qcom.deviceapi
FingerprintSwitchUart() - Method in interface com.rscja.deviceapi.interfaces.IUsbFingerprint
  指纹切换到串口
FingerprintSwitchUart() - Method in class com.rscja.deviceapi.UsbFingerprint
  指纹切换到串口
FingerprintSwitchUart(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
FingerprintSwitchUart() - Method in class com.rscja.team.mtk.deviceapi.UsbFingerprint_mtk
  指纹切换到串口
FingerprintSwitchUart(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
FingerprintSwitchUart() - Method in class com.rscja.team.qcom.deviceapi.UsbFingerprint_qcom
  指纹切换到串口
FingerprintSwitchUsb() - Method in interface com.rscja.deviceapi.interfaces.IUsbFingerprint
  指纹切换到USB
FingerprintSwitchUsb() - Method in class com.rscja.deviceapi.UsbFingerprint
  指纹切换到USB
FingerprintSwitchUsb(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
FingerprintSwitchUsb() - Method in class com.rscja.team.mtk.deviceapi.UsbFingerprint_mtk
  指纹切换到USB
FingerprintSwitchUsb(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
FingerprintSwitchUsb() - Method in class com.rscja.team.qcom.deviceapi.UsbFingerprint_qcom
  指纹切换到USB
FingerprintWithFIPS - Class in com.rscja.deviceapi
  FIPS指纹识别模块操作类,
  FIPS fingerprint indentify module operation type,
FingerprintWithFIPS.DataFormat - Enum in com.rscja.deviceapi
  指纹数据格式
  Fingerprint data format
FingerprintWithFIPS.EnrollCallBack - Interface in com.rscja.deviceapi
  采集指纹回调接口
  call-back contact for acquiring fingerprint
FingerprintWithFIPS.FingerprintInfo - Class in com.rscja.deviceapi
FingerprintWithFIPS.GRABCallBack - Interface in com.rscja.deviceapi
  指纹图像回调接口
  fingerprint image call-back contact
FingerprintWithFIPS.IdentificationCallBack - Interface in com.rscja.deviceapi
  验证指纹的回调接口
  call-back contact of verify fingerprint
FingerprintWithFIPS.PtCaptureCallBack - Interface in com.rscja.deviceapi
  获取指纹模版数据回调接口
  Acquire call-back contact fingerprint template data
FingerprintWithFIPS.TemplateVerifyCallBack - Interface in com.rscja.deviceapi
  指纹模版比对
  fingerprint template comparison
FingerprintWithFIPS_mtk - Class in com.rscja.team.mtk.deviceapi
  FIPS指纹识别模块操作类,
  FIPS fingerprint indentify module operation type,
FingerprintWithFIPS_qcom - Class in com.rscja.team.qcom.deviceapi
  FIPS指纹识别模块操作类,
  FIPS fingerprint indentify module operation type,
FingerprintWithMorpho - Class in com.rscja.deviceapi
FingerprintWithMorpho.EnrollCallBack - Interface in com.rscja.deviceapi
  采集指纹回调接口
  acquire fingerprint call-back contact
FingerprintWithMorpho.GrabCallBack - Interface in com.rscja.deviceapi
FingerprintWithMorpho.IdentificationCallBack - Interface in com.rscja.deviceapi
  验证指纹的回调接口
  call-back contact for fingerprint verification
FingerprintWithMorpho.PtCaptureCallBack - Interface in com.rscja.deviceapi
  设置获取指纹模版回调接口
  setup fingerprint template acquire call-back contact
FingerprintWithMorpho.TemplateVerifyCallBack - Interface in com.rscja.deviceapi
FingerprintWithMorpho_mtk - Class in com.rscja.team.mtk.deviceapi
FingerprintWithMorpho_qcom - Class in com.rscja.team.qcom.deviceapi
FingerprintWithTLK1NC - Class in com.rscja.deviceapi
  迪安杰
FingerprintWithTLK1NC.BufferEnum - Enum in com.rscja.deviceapi
  模块缓冲区枚举
  Module buffer zone example.
FingerprintWithTLK1NC.IUPImageCallback - Interface in com.rscja.deviceapi
  指纹图像回调接口
  fingerprint image call-back contact
FingerprintWithTLK1NC_mtk - Class in com.rscja.team.mtk.deviceapi
  迪安杰
FingerprintWithTLK1NC_qcom - Class in com.rscja.team.qcom.deviceapi
  迪安杰
FingerprintWithZAZ - Class in com.rscja.deviceapi
  指昂
FingerprintWithZAZ.BufferEnum - Enum in com.rscja.deviceapi
  模块缓冲区枚举
  Module buffer zone example.
FingerprintWithZAZ_qcom - Class in com.rscja.team.qcom.deviceapi
  指昂
fingerSearchTemplate(FingerprintWithTLK1NC.BufferEnum, int, int) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  下载一个特征到指定特征缓冲区，然后用此特征搜索指纹库中的模板
fingerSearchTemplate(FingerprintWithTLK1NC.BufferEnum, int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  下载一个特征到指定特征缓冲区，然后用此特征搜索指纹库中的模板
fingerSearchTemplate(FingerprintWithTLK1NC.BufferEnum, int, int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  下载一个特征到指定特征缓冲区，然后用此特征搜索指纹库中的模板
fingerSearchTemplate(FingerprintWithTLK1NC.BufferEnum, int, int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  下载一个特征到指定特征缓冲区，然后用此特征搜索指纹库中的模板
fingerStopGRABImage() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
fingerStopGRABImage() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
fingerStoreCharToBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  生成指纹特征，存储在指定特征缓冲区
fingerStoreCharToBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  生成指纹特征，存储在指定特征缓冲区
fingerStoreCharToBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  生成指纹特征，存储在指定特征缓冲区
fingerStoreCharToBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  生成指纹特征，存储在指定特征缓冲区
fingerStoreCharToFlashPage(int) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  生成指纹特征，存储在Flash Page
fingerStoreCharToFlashPage(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  生成指纹特征，存储在Flash Page
fingerStoreCharToFlashPage(int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  生成指纹特征，存储在Flash Page
fingerStoreCharToFlashPage(int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  生成指纹特征，存储在Flash Page
fingerUPTemplateFromBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  上传指纹特征值，将指定缓冲区中的特征值上传到上位机
fingerUPTemplateFromBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  上传指纹特征值，将指定缓冲区中的特征值上传到上位机
fingerUPTemplateFromBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  上传指纹特征值，将指定缓冲区中的特征值上传到上位机
fingerUPTemplateFromBuffer(FingerprintWithTLK1NC.BufferEnum) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  上传指纹特征值，将指定缓冲区中的特征值上传到上位机
fingerUPTemplateFromFlashPage(int) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  上传指纹特征值，将指定Flash Page中的特征值上传到上位机
fingerUPTemplateFromFlashPage(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  上传指纹特征值，将指定Flash Page中的特征值上传到上位机
fingerUPTemplateFromFlashPage(int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
  上传指纹特征值，将指定Flash Page中的特征值上传到上位机
fingerUPTemplateFromFlashPage(int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  上传指纹特征值，将指定Flash Page中的特征值上传到上位机
fips_encryption_decryption(byte[], int, byte[], int, byte) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
fips_encryption_decryption(byte[], int, byte[], int, byte) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
fips_encryption_decryption_EX(byte[], int, byte[], int, byte, Object, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
fips_encryption_decryption_EX(byte[], int, byte[], int, byte, Object, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
FLOWCONTROL_NONE - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  No flow control.
FLOWCONTROL_RTSCTS_IN - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  RTS/CTS input flow control.
FLOWCONTROL_RTSCTS_OUT - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  RTS/CTS output flow control.
FLOWCONTROL_XONXOFF_IN - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  XON/XOFF input flow control.
FLOWCONTROL_XONXOFF_OUT - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  XON/XOFF output flow control.
FORMAT_ASCII - Static variable in interface com.rscja.scanner.IScanner
  编码格式：ASCII
  decoding format: ASCII
FORMAT_DECIMAL - Static variable in interface com.rscja.scanner.IScanner
  编码格式：十进制
  decoding format: decimalism
FORMAT_DEFAULT - Static variable in interface com.rscja.scanner.IScanner
  编码格式：默认格式
  decoding format: default format
FORMAT_GB18030 - Static variable in interface com.rscja.scanner.IScanner
  编码格式：GB18030
  decoding format: GB18030
FORMAT_GB2312 - Static variable in interface com.rscja.scanner.IScanner
  编码格式：GB2312
  decoding format: GB2312
FORMAT_GBK - Static variable in interface com.rscja.scanner.IScanner
  编码格式：GBK
  decoding format: GBK
FORMAT_HEX - Static variable in interface com.rscja.scanner.IScanner
  编码格式：十六进制
  decoding format: hexvalue
FORMAT_UNICODE - Static variable in interface com.rscja.scanner.IScanner
  编码格式：UNICODE
  decoding format: UNICODE
FORMAT_UTF8 - Static variable in interface com.rscja.scanner.IScanner
  编码格式：UTF8
  decoding format: UTF8
free() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFUARTUAE
  关闭UHF模块
  Switch off UHF module
free() - Method in class com.rscja.custom.UHFCSYXForURx
free() - Method in class com.rscja.deviceapi.BleDevice
free() - Method in class com.rscja.deviceapi.BluetoothReader
free() - Method in class com.rscja.deviceapi.CardWithBYL
  释放模块
free() - Method in class com.rscja.deviceapi.Fingerprint
  释放指纹模块
  Release fingerprint module.
free() - Method in class com.rscja.deviceapi.FingerprintSM206B
  释放指纹模块
free() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  释放指纹模块
  Release fingerprint module
free() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  释放指纹模块
  free fingerprint module
free() - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
free() - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  释放指纹模块
  free fingerprint module
free() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  释放蓝牙相关的资源(free Bluetooth resources)
free() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  释放模块
free() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  释放指纹模块
  Release fingerprint module.
free() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
free() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  释放指纹模块
  Release fingerprint module
free() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  释放指纹模块
  free fingerprint module
free() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
free() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  释放指纹模块
  free fingerprint module
free() - Method in interface com.rscja.deviceapi.interfaces.IModule
  释放模块,模块断电同时关闭串口
  Release module
free() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  关闭打印机模块
  Switch off printer module
free() - Method in interface com.rscja.deviceapi.interfaces.IPSAM
  释放PSAM
  Release PSAM
free() - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
  释放rfid模块
  Release RFID module
free() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  释放RFID低频模块
  Release RFID LF module
free() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  关闭UHF模块
  Switch OFF UHF module
free() - Method in class com.rscja.deviceapi.Module
  释放模块,模块断电同时关闭串口
  Release module
free() - Method in class com.rscja.deviceapi.Printer
  关闭打印机模块
  Switch off printer module
free() - Method in class com.rscja.deviceapi.PSAM
  释放PSAM
  Release PSAM
free() - Method in class com.rscja.deviceapi.RFIDBase
  释放rfid模块
  Release RFID module
free() - Method in class com.rscja.deviceapi.RFIDWithLF
  释放RFID低频模块
  Release RFID LF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
free() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
free() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  关闭UHF模块
  Switch off UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  关闭UHF模块
  Switch OFF UHF module
free() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
free() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  断开usb连接，释放usb资源
  Disconnect USB connection, release USB resources
free() - Method in class com.rscja.deviceapi.UhfBase
free() - Method in class com.rscja.scanner.led.ScanLed
  释放设备资源
  release device source
free() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  释放指纹模块
  Release fingerprint module
free() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  释放指纹模块
  free fingerprint module
free() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
free() - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  释放模块,模块断电同时关闭串口
  Release module
free() - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  关闭打印机模块
  Switch off printer module
free() - Method in class com.rscja.team.mtk.deviceapi.PSAM_mtk
  释放PSAM
  Release PSAM
free() - Method in class com.rscja.team.mtk.deviceapi.RFIDBase_mtk
  释放rfid模块
  Release RFID module
free() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  关闭UHF模块
  Switch off UHF module
free() - Method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  释放设备资源
  release device source
free() - Method in class com.rscja.team.mtk.scanner.led.ScanLed_mtk
  释放设备资源
  release device source
free() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
free() - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
free() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
  关闭UHF模块
  Switch off UHF module
free() - Method in class com.rscja.team.qcom.custom.UHFCSYX_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
  释放模块
free() - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  释放指纹模块
  Release fingerprint module.
free() - Method in class com.rscja.team.qcom.deviceapi.FingerprintSM206B_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  释放指纹模块
  Release fingerprint module
free() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  释放指纹模块
  free fingerprint module
free() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  释放指纹模块
  free fingerprint module
free(HardwareInterface_qcom.FunctionEnum) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  释放模块,模块断电同时关闭串口
  Release module
free() - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  释放模块,模块断电同时关闭串口
  Release module
free() - Method in class com.rscja.team.qcom.deviceapi.PSAM_qcom
  释放PSAM
  Release PSAM
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDBase_qcom
  释放rfid模块
  Release RFID module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  释放RFID低频模块
  Release RFID LF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
  关闭UHF模块
  Switch off UHF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
  断开uhf连接
  Switch OFF UHF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  关闭UHF模块
  Switch OFF UHF module
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
free() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
  断开usb连接，释放usb资源
  Disconnect USB connection, release USB resources
free() - Method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  释放设备资源
  release device source
free(byte) - Method in interface com.rscja.team.qcom.r1.IPSAM
  释放PSAM(Release PSAM)
free(byte) - Method in class com.rscja.team.qcom.r1.psam.PSAM
  释放PSAM(Release PSAM)
free() - Method in class com.rscja.team.qcom.service.BLEService_qcom
fullData - Variable in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom.CMDInfo
fullData - Variable in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase.CMDInfo
fullData - Variable in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase.CMDInfo
FUNCTION_14443A - Static variable in interface com.rscja.scanner.IScanner
  14443A
FUNCTION_15693 - Static variable in interface com.rscja.scanner.IScanner
  15693
FUNCTION_1D - Static variable in interface com.rscja.scanner.IScanner
  1D
FUNCTION_2D - Static variable in interface com.rscja.scanner.IScanner
  2D软解码
  2D soft_decoding
FUNCTION_2D_H - Static variable in interface com.rscja.scanner.IScanner
  2D硬解码
  2D Hard_decoding
FUNCTION_LF_ANIMAL - Static variable in interface com.rscja.scanner.IScanner
  LF-动物标签
  LF_Animal tag
FUNCTION_LF_EM4450 - Static variable in interface com.rscja.scanner.IScanner
  LF-EM4450
FUNCTION_LF_HDX - Static variable in interface com.rscja.scanner.IScanner
  LF-hdx
FUNCTION_LF_HID - Static variable in interface com.rscja.scanner.IScanner
  LF-HID
FUNCTION_LF_HITAG - Static variable in interface com.rscja.scanner.IScanner
  LF-hiTag
FUNCTION_LF_ID - Static variable in interface com.rscja.scanner.IScanner
  LF-id卡
  LF_ID card
FUNCTION_LF_NEEDLE - Static variable in interface com.rscja.scanner.IScanner
  LF二合一模块
  LF dual_protocol module
FUNCTION_UHF - Static variable in interface com.rscja.scanner.IScanner
  UHF

A B C D E F G H I J K L M N O P Q R S T U V W X Z