## Uses of Interface
com.rscja.deviceapi.interfaces.IUHFOfAndroidUart

- Packages that use IUHFOfAndroidUart
  Package | Description
  --- | ---
  com.rscja.custom |
  com.rscja.custom.interfaces |
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.mtk.custom |
  com.rscja.team.mtk.deviceapi |
  com.rscja.team.qcom.custom |
  com.rscja.team.qcom.deviceapi |

- - ### Uses of IUHFOfAndroidUart in com.rscja.custom

    Classes in com.rscja.custom that implement IUHFOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `M775Authenticate` 英频杰特殊标签定制 Special label customization 第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 盘点标签之前先要设置回调函数`M775Authenticate.setInventoryCallback(IUHFInventoryCallback)`,然后调用盘点函数`RFIDWithUHFUART.startInventoryTag()`开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。 For parameter setting, after the connection is successful, call the corresponding function to set parameters and read/write operations.
    `class` | `RFIDWithUHFJieCe`
    `class` | `UHFCSYX` MQTT是长沙盈芯，定制接口
    `class` | `UHFTamperAPI` 阿联酋Acube 定制接口
    `class` | `UHFTemperatureSensors`
    `class` | `UHFTemperatureTagsAPI`
    `class` | `UHFUartFoxconn`
    `class` | `UHFUartTemperatureTag`
    `class` | `UHFXSAPI`

  - ### Uses of IUHFOfAndroidUart in com.rscja.custom.interfaces

    Subinterfaces of IUHFOfAndroidUart in com.rscja.custom.interfaces
    Modifier and Type | Interface and Description
    --- | ---
    `interface` | `IM775Authenticate`
    `interface` | `IRFIDWithUHFJieCe`
    `interface` | `IRFIDWithUHFShuangYingDianZi`
    `interface` | `IRFIDWithUHFUARTUAE`
    `interface` | `IUHFCSYX` MQTT是长沙盈芯，定制接口
    `interface` | `IUHFTamperAPI`
    `interface` | `IUHFUartFoxconn`

  - ### Uses of IUHFOfAndroidUart in com.rscja.deviceapi

    Classes in com.rscja.deviceapi that implement IUHFOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFA4` UHF模块 A4操作类 UHF module operation type 第一步:通过`RFIDWithUHFA4.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFA4.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFA4.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFA4.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFA4.stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
    `class` | `RFIDWithUHFA8` UHF模块 A8操作类 UHF module operation type 第一步:通过`RFIDWithUHFA8.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFA8.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFA8.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFA8.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFA8.stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
    `class` | `RFIDWithUHFAxBase`
    `class` | `RFIDWithUHFRLM`
    `class` | `RFIDWithUHFUART` UHF模块手持机，串口通信操作类 UHF module handheld, serial communication operation interface 第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFUART.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFUART.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.

  - ### Uses of IUHFOfAndroidUart in com.rscja.deviceapi.interfaces

    Subinterfaces of IUHFOfAndroidUart in com.rscja.deviceapi.interfaces
    Modifier and Type | Interface and Description
    --- | ---
    `interface` | `IRFIDWithUHFA4Uart`
    `interface` | `IRFIDWithUHFA8Uart`
    `interface` | `IRFIDWithUHFRLM`

  - ### Uses of IUHFOfAndroidUart in com.rscja.team.mtk.custom

    Classes in com.rscja.team.mtk.custom that implement IUHFOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `M775Authenticate_mtk`
    `class` | `UHFTemperatureTagsAPI_mtk`
    `class` | `UHFUartFoxconn_mtk`

  - ### Uses of IUHFOfAndroidUart in com.rscja.team.mtk.deviceapi

    Classes in com.rscja.team.mtk.deviceapi that implement IUHFOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFUART_mtk`

  - ### Uses of IUHFOfAndroidUart in com.rscja.team.qcom.custom

    Classes in com.rscja.team.qcom.custom that implement IUHFOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `M775Authenticate_qcom`
    `class` | `RFIDWithUHFJieCe_qcom`
    `class` | `RFIDWithUHFShuangYingDianZi_qcom`
    `class` | `RFIDWithUHFUARTUAE_qcom`
    `class` | `UHFCSYX_qcom`
    `class` | `UHFTamperAPI_qcom`
    `class` | `UHFTemperatureTagsAPI_qcom`
    `class` | `UHFUartFoxconn_qcom`

  - ### Uses of IUHFOfAndroidUart in com.rscja.team.qcom.deviceapi

    Classes in com.rscja.team.qcom.deviceapi that implement IUHFOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFA4_qcom` UHF模块 A4操作类 UHF module operation type
    `class` | `RFIDWithUHFA8_qcom` UHF模块 A8操作类 UHF module operation type
    `class` | `RFIDWithUHFAxBase_qcom`
    `class` | `RFIDWithUHFRLM_qcom`
    `class` | `RFIDWithUHFUART_qcom`