## Uses of Interface
com.rscja.deviceapi.interfaces.ConnectionStatusCallback

- Packages that use ConnectionStatusCallback
  Package | Description
  --- | ---
  com.rscja.custom |
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.mtk.deviceapi |
  com.rscja.team.qcom.ble |
  com.rscja.team.qcom.deviceapi |
  com.rscja.team.qcom.service |
  com.rscja.team.qcom.usb |

- - ### Uses of ConnectionStatusCallback in com.rscja.custom

    Classes in com.rscja.custom that implement ConnectionStatusCallback
    Modifier and Type | Class and Description
    --- | ---
    `class` | `UHFTemperatureTag.RFIDWithUHFBLEN51`
    `class` | `UHFTemperatureTag.RFIDWithUHFBLEN52`

  - ### Uses of ConnectionStatusCallback in com.rscja.deviceapi

    Methods in com.rscja.deviceapi with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | BleDevice.`connect(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 连接蓝牙(Connect Bluetooth)
    `void` | BluetoothReader.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFBLE.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFA8NetWork.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置监听连接状态(Set the listening connection status)
    `void` | RFIDWithUHFUSB.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUrxUart.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置UHF连接状态回调 Setup UHF continuous stauts call-back
    `void` | RFIDWithUHFUrxUsbToUart.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | BleDevice.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置UHF连接状态回调 Setup UHF continuous stauts call-back
    `void` | RFIDWithUHFUrxNetwork.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | BluetoothReader.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFA4NetWork.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置监听连接状态(Set the listening connection status)
    `void` | RFIDWithUHFBLE.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUART.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFA4RS232.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> statusCallback)` 设置监听连接状态(Set the listening connection status)
    `void` | RFIDWithUHFA8RS232.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> statusCallback)` 设置监听连接状态(Set the listening connection status)

  - ### Uses of ConnectionStatusCallback in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | IBleDevice.`connect(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | IBluetoothReader.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 连接蓝牙(Connect Bluetooth)
    `void` | IUHF.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置UHF连接状态回调 Setup UHF continuous stauts call-back
    `void` | IBluetoothReader.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置蓝牙连接状态的回调(Setup Bluetooth connection status call back)
    `void` | IBleDevice.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`

  - ### Uses of ConnectionStatusCallback in com.rscja.team.mtk.deviceapi

    Methods in com.rscja.team.mtk.deviceapi with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | RFIDWithUHFUART_mtk.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`

  - ### Uses of ConnectionStatusCallback in com.rscja.team.qcom.ble

    Classes in com.rscja.team.qcom.ble that implement ConnectionStatusCallback
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFBLEN51_qcom`
    `class` | `RFIDWithUHFBLEN52_qcom`

    Methods in com.rscja.team.qcom.ble with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | EmptyUhfBle.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | EmptyUhfBle.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`

  - ### Uses of ConnectionStatusCallback in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | BleDevice_qcom.`connect(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFBLE_qcom.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | BluetoothReader_qcom.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUSB_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUrxUsbToUart_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUrxUart_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置UHF连接状态回调 Setup UHF continuous stauts call-back
    `void` | RFIDWithUHFUrxUart2_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUrxNetwork_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUART_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFBLE_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | BluetoothReader_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | BleDevice_qcom.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`

  - ### Uses of ConnectionStatusCallback in com.rscja.team.qcom.service

    Methods in com.rscja.team.qcom.service with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | BLEService_qcom.`connect(java.lang.String address, ConnectionStatusCallback btStatusCallback)`
    `void` | BLEService_qcom.`setStatusCallback(ConnectionStatusCallback btStatusCallback)`

  - ### Uses of ConnectionStatusCallback in com.rscja.team.qcom.usb

    Methods in com.rscja.team.qcom.usb with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | UsbBase_qcom.`setConnectionStatusCallback(ConnectionStatusCallback callback)`