## Uses of Class
com.rscja.deviceapi.interfaces.ConnectionStatus

- Packages that use ConnectionStatus
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.mtk.deviceapi |
  com.rscja.team.qcom.ble |
  com.rscja.team.qcom.deviceapi |
  com.rscja.team.qcom.service |
  com.rscja.team.qcom.socket |
  com.rscja.team.qcom.usb |
  com.rscja.team.qcom.usb.pl2302 |

- - ### Uses of ConnectionStatus in com.rscja.deviceapi

    Methods in com.rscja.deviceapi that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | R1HFAndPsamManage.`getConnectionStatus()`
    `ConnectionStatus` | RFIDWithUHFA8NetWork.`getConnectStatus()` 获取连接状态(Acquire UHF connection status)
    `ConnectionStatus` | RFIDWithUHFUSB.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFUrxUart.`getConnectStatus()` 获取UHF连接状态 Acquire UHF connection status
    `ConnectionStatus` | RFIDWithUHFUrxUsbToUart.`getConnectStatus()`
    `ConnectionStatus` | BleDevice.`getConnectStatus()` 获取UHF连接状态 Acquire UHF connection status
    `ConnectionStatus` | RFIDWithUHFUrxNetwork.`getConnectStatus()`
    `ConnectionStatus` | BluetoothReader.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFA4NetWork.`getConnectStatus()` 获取连接状态(Acquire UHF connection status)
    `abstract ConnectionStatus` | UhfBase.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFUART.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFA4RS232.`getConnectStatus()` 获取连接状态(Acquire UHF connection status)
    `ConnectionStatus` | RFIDWithUHFA8RS232.`getConnectStatus()` 获取连接状态(Acquire UHF connection status)

  - ### Uses of ConnectionStatus in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | IUHF.`getConnectStatus()` 获取UHF连接状态 Acquire UHF connection status
    `ConnectionStatus` | IBluetoothReader.`getConnectStatus()` 获取蓝牙连接状态(Acquire Bluetooth connection status)
    `ConnectionStatus` | IBleDevice.`getConnectStatus()`
    `static ConnectionStatus` | ConnectionStatus.`valueOf(int value)`
    `static ConnectionStatus` | ConnectionStatus.`valueOf(java.lang.String name)` Returns the enum constant of this type with the specified name.
    `static ConnectionStatus[]` | ConnectionStatus.`values()` Returns an array containing the constants of this enum type, in the order they are declared.

    Methods in com.rscja.deviceapi.interfaces with parameters of type ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `void` | ConnectionStatusCallback.`getStatus(ConnectionStatus status, T device)`
    `void` | IConnectionStatusChangedListener.`onStatusChanged(ConnectionStatus status)`

  - ### Uses of ConnectionStatus in com.rscja.team.mtk.deviceapi

    Methods in com.rscja.team.mtk.deviceapi that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | RFIDWithUHFUART_mtk.`getConnectStatus()`

  - ### Uses of ConnectionStatus in com.rscja.team.qcom.ble

    Methods in com.rscja.team.qcom.ble that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | EmptyUhfBle.`getConnectStatus()`

    Methods in com.rscja.team.qcom.ble with parameters of type ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `void` | RFIDWithUHFBLEN52_qcom.`getStatus(ConnectionStatus status, java.lang.Object device)`
    `void` | RFIDWithUHFBLEN51_qcom.`getStatus(ConnectionStatus status, java.lang.Object device)`

  - ### Uses of ConnectionStatus in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | RFIDWithUHFUSB_qcom.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFUrxUsbToUart_qcom.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFUrxUart_qcom.`getConnectStatus()` 获取UHF连接状态 Acquire UHF connection status
    `ConnectionStatus` | RFIDWithUHFUrxUart2_qcom.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFUrxNetwork_qcom.`getConnectStatus()`
    `ConnectionStatus` | RFIDWithUHFUART_qcom.`getConnectStatus()`
    `ConnectionStatus` | BluetoothReader_qcom.`getConnectStatus()`
    `ConnectionStatus` | BleDevice_qcom.`getConnectStatus()`

  - ### Uses of ConnectionStatus in com.rscja.team.qcom.service

    Methods in com.rscja.team.qcom.service that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | BLEService_qcom.`getBTConnectStatus()`

  - ### Uses of ConnectionStatus in com.rscja.team.qcom.socket

    Methods in com.rscja.team.qcom.socket that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | SocketManageUR4.`getConnectStatus()`
    `ConnectionStatus` | SocketManageA4.`getConnectStatus()`

    Methods in com.rscja.team.qcom.socket with parameters of type ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `void` | SocketManageUR4.`update(ConnectionStatus arg)`
    `void` | SocketManageA4.`update(ConnectionStatus status)`

  - ### Uses of ConnectionStatus in com.rscja.team.qcom.usb

    Methods in com.rscja.team.qcom.usb that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | UsbBase_qcom.`getConnectionStatus()`

  - ### Uses of ConnectionStatus in com.rscja.team.qcom.usb.pl2302

    Methods in com.rscja.team.qcom.usb.pl2302 that return ConnectionStatus
    Modifier and Type | Method and Description
    --- | ---
    `ConnectionStatus` | UsbPL2302.`getConnectionStatus()`