## Uses of Interface
com.rscja.deviceapi.interfaces.IURAxOfAndroidUart

- Packages that use IURAxOfAndroidUart
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.qcom.custom |
  com.rscja.team.qcom.deviceapi |

- - ### Uses of IURAxOfAndroidUart in com.rscja.deviceapi

    Classes in com.rscja.deviceapi that implement IURAxOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFA4` UHF模块 A4操作类 UHF module operation type 第一步:通过`RFIDWithUHFA4.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFA4.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFA4.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFA4.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFA4.stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
    `class` | `RFIDWithUHFA8` UHF模块 A8操作类 UHF module operation type 第一步:通过`RFIDWithUHFA8.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFA8.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点标签先调用`RFIDWithUHFA8.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`设置标签回调接口，有标签数据就会回调这个接口。 然后在调用`RFIDWithUHFA8.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFA8.stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
    `class` | `RFIDWithUHFAxBase`

  - ### Uses of IURAxOfAndroidUart in com.rscja.deviceapi.interfaces

    Subinterfaces of IURAxOfAndroidUart in com.rscja.deviceapi.interfaces
    Modifier and Type | Interface and Description
    --- | ---
    `interface` | `IRFIDWithUHFA4Uart`
    `interface` | `IRFIDWithUHFA8Uart`

  - ### Uses of IURAxOfAndroidUart in com.rscja.team.qcom.custom

    Classes in com.rscja.team.qcom.custom that implement IURAxOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `UHFTemperatureTagsAPI_qcom`

  - ### Uses of IURAxOfAndroidUart in com.rscja.team.qcom.deviceapi

    Classes in com.rscja.team.qcom.deviceapi that implement IURAxOfAndroidUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFA4_qcom` UHF模块 A4操作类 UHF module operation type
    `class` | `RFIDWithUHFA8_qcom` UHF模块 A8操作类 UHF module operation type
    `class` | `RFIDWithUHFAxBase_qcom`