A B C D E F G H I J K L M N O P Q R S T U V W X Z

## S

S - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
Save24bitFingerprintPicture(String, int, int, byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
saveXmlList(List<String[]>) - Static method in class com.rscja.team.mtk.utility.FileUtils
scan() - Method in class com.rscja.deviceapi.Barcode1D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in class com.rscja.deviceapi.Barcode2D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scan() - Method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.deviceapi.Barcode1D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.deviceapi.Barcode2D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.deviceapi.BleDevice
  扫描条码
  Scan barcode
scanBarcode() - Method in class com.rscja.deviceapi.BluetoothReader
scanBarcode() - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
scanBarcode() - Method in interface com.rscja.deviceapi.interfaces.IReader
  扫描条码
  Scan barcode
scanBarcode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
scanBarcode() - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
scanBarcode() - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  触发一次条码扫描
  Enable barcode scanning for 1 time.
scanBarcode() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
scanBarcode() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
scanBarcode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
scanBarcodeToBytes() - Method in class com.rscja.deviceapi.BleDevice
  扫描条码
  Scan barcode
scanBarcodeToBytes() - Method in class com.rscja.deviceapi.BluetoothReader
scanBarcodeToBytes() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
scanBarcodeToBytes() - Method in interface com.rscja.deviceapi.interfaces.IReader
  扫描条码
  Scan barcode
scanBarcodeToBytes() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
scanBarcodeToBytes() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
scanBarcodeToBytes() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
scanBarcodeToBytes() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
scanBarcodeToBytes() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
ScanBTCallback - Interface in com.rscja.deviceapi.interfaces
ScanerLed_Free(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ScanerLed_Free(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ScanerLed_Init(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ScanerLed_Init(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ScanerLed_Off(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ScanerLed_Off(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ScanerLed_On(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ScanerLed_On(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
ScanerLedLight - Class in com.rscja.deviceapi
  扫描LED灯控制类（仅C6000有效）
  Scanning LED light control type ( valid for C6000 only)
ScanerLedLight() - Constructor for class com.rscja.deviceapi.ScanerLedLight
ScanerLedLight_mtk - Class in com.rscja.team.mtk.deviceapi
  扫描LED灯控制类（仅C6000有效）
  Scanning LED light control type ( valid for C6000 only)
ScanerLedLight_mtk() - Constructor for class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
ScanerLedLight_qcom - Class in com.rscja.team.qcom.deviceapi
  扫描LED灯控制类（仅C6000有效）
  Scanning LED light control type ( valid for C6000 only)
ScanerLedLight_qcom() - Constructor for class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
ScanLed - Class in com.rscja.scanner.led
ScanLed() - Constructor for class com.rscja.scanner.led.ScanLed
ScanLed_mtk - Class in com.rscja.team.mtk.scanner.led
ScanLed_mtk() - Constructor for class com.rscja.team.mtk.scanner.led.ScanLed_mtk
ScanLedManage - Class in com.rscja.scanner.led
ScanLedManage_mtk - Class in com.rscja.team.mtk.scanner.led
ScanLedManage_qcom - Class in com.rscja.team.qcom.scanner.led
SCANNER_BARCODE_1D - Static variable in class com.rscja.barcode.BarcodeUtility
  1D是否已经开启
SCANNER_BARCODE_2D - Static variable in class com.rscja.barcode.BarcodeUtility
  2D是否已经开启
SCANNER_BARCODENOTREPEAT - Static variable in class com.rscja.barcode.BarcodeUtility
  条码是否重复显示
SCANNER_BROADCAST_ACTION - Static variable in class com.rscja.barcode.BarcodeUtility
  接收扫描数据的广播ACTION
SCANNER_BROADCAST_EXTRA - Static variable in class com.rscja.barcode.BarcodeUtility
  接收扫描数据的广播的extra数据
SCANNER_CONTINUOUS - Static variable in class com.rscja.barcode.BarcodeUtility
  是否是连续扫描 Whether enable continuous scan
SCANNER_CONTINUOUS_INTREVALTIME - Static variable in class com.rscja.barcode.BarcodeUtility
  连续扫描时间间隔
SCANNER_CONTINUOUSMODE - Static variable in class com.rscja.barcode.BarcodeUtility
  是否启用了连续扫描模式
SCANNER_CONTINUOUSTIMEOUT - Static variable in class com.rscja.barcode.BarcodeUtility
  连续扫描超时时间 continuous scanning overtime duration
SCANNER_ENDINDEX - Static variable in class com.rscja.barcode.BarcodeUtility
  后面去掉多少个字符
SCANNER_ENTER - Static variable in class com.rscja.barcode.BarcodeUtility
  是否启用回车
SCANNER_FAILUREBROADCAST - Static variable in class com.rscja.barcode.BarcodeUtility
  扫描失败是否发送广播 Send broadcast when scanning failure.
SCANNER_FAILURESOUND - Static variable in class com.rscja.barcode.BarcodeUtility
  扫描失败是否播放声音 whether playing notification when scanning failure.
SCANNER_FILTERCHARS - Static variable in class com.rscja.barcode.BarcodeUtility
  条码数据需要过滤的字符串
SCANNER_FORMAT_BARCODE - Static variable in class com.rscja.barcode.BarcodeUtility
  条码格式 0: Default 1: ASCII 2:GB2312 3:UTF8 4:Unicode 10:GBK, 11:GB18030 Barcode format 0: Default 1: ASCII 2:GB2312 3:UTF8 4:Unicode 10:GBK, 11:GB18030
SCANNER_ILLUMINATIONPOWERLEVEL - Static variable in class com.rscja.barcode.BarcodeUtility
  4710 扫描头亮度等级
SCANNER_KEYBORADHELPER_OPEN - Static variable in class com.rscja.barcode.BarcodeUtility
  键盘助手总开关是否已经打开
SCANNER_OUTPUTMODE - Static variable in class com.rscja.barcode.BarcodeUtility
  数据接收方式 0:键盘模拟 1:剪切板 2:系统广播 ouput mode 0: virtual key 1: clipboard 2: broadcast
SCANNER_PREFIX - Static variable in class com.rscja.barcode.BarcodeUtility
  条码前缀 barcode prefix.
SCANNER_RELEASESCAN - Static variable in class com.rscja.barcode.BarcodeUtility
  松开扫描按键是否停止扫描 loose scanning button to stop scanning or not
SCANNER_SCANKEYCODE_1 - Static variable in class com.rscja.barcode.BarcodeUtility
  扫描按键值 scan key code.
SCANNER_SCANKEYCODE_3 - Static variable in class com.rscja.barcode.BarcodeUtility
  扫描按键值 scan key code.
SCANNER_SOUND - Static variable in class com.rscja.barcode.BarcodeUtility
  扫描成功是否播放声音
SCANNER_STARTINDEX - Static variable in class com.rscja.barcode.BarcodeUtility
  前面去掉多少个字符
SCANNER_SUFFIX - Static variable in class com.rscja.barcode.BarcodeUtility
  条码后缀 barcode suffix.
SCANNER_TAB - Static variable in class com.rscja.barcode.BarcodeUtility
  是否启用tab
SCANNER_TIMEOUT - Static variable in class com.rscja.barcode.BarcodeUtility
  扫描超时 scanning time out.
SCANNER_VIBRATE - Static variable in class com.rscja.barcode.BarcodeUtility
  是否启用震动 whether vibrating when scanning success
ScannerCameraIdFile - Static variable in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
  Deprecated.
ScannerParameterEntity - Class in com.rscja.deviceapi.entity
ScannerParameterEntity() - Constructor for class com.rscja.deviceapi.entity.ScannerParameterEntity
ScannerParameterEntity.Builder - Class in com.rscja.deviceapi.entity
ScannerParameterUtility_qcom - Class in com.rscja.team.qcom.scanner.utility
ScannerParameterUtility_qcom() - Constructor for class com.rscja.team.qcom.scanner.utility.ScannerParameterUtility_qcom
ScannerStateFile - Static variable in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
  Deprecated.
ScannerUtility - Class in com.rscja.scanner.utility
  键盘助手工具类，用于控制键盘助手
  keyboardemulator tool-kits, control keyboardemulator
ScannerUtility_mtk - Class in com.rscja.team.mtk.scanner.utility
  键盘助手工具类，用于控制键盘助手
  keyboardemulator tool-kits, control keyboardemulator
ScannerUtility_qcom - Class in com.rscja.team.qcom.scanner.utility
  键盘助手工具类，用于控制键盘助手
  keyboardemulator tool-kits, control keyboardemulator
search(Fingerprint.BufferEnum, int, int) - Method in class com.rscja.deviceapi.Fingerprint
  检索指纹库
  Searching fingerprint database
search(FingerprintWithZAZ.BufferEnum, int, int, int[], int[], int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
search(Fingerprint.BufferEnum, int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  检索指纹库
  Searching fingerprint database
search(FingerprintWithZAZ.BufferEnum, int, int, int[], int[], int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
search(Fingerprint.BufferEnum, int, int) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  检索指纹库
  Searching fingerprint database
search(FingerprintWithZAZ.BufferEnum, int, int, int[], int[], int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
send(byte[]) - Method in class com.rscja.deviceapi.Infrared
  发送数据
  send Data
send(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothData
send(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  发送数据
  send Data
send(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IModule
  发送数据
  Send data
send(byte[]) - Method in class com.rscja.deviceapi.Module
  发送数据
  Send data
send(byte[]) - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  发送数据
  send Data
send(byte[]) - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  发送数据
  Send data
send(HardwareInterface_qcom.FunctionEnum, byte[]) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  发送数据
  Send data
send(int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
send(byte[]) - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  发送数据
  Send data
send(byte[]) - Method in class com.rscja.team.qcom.socket.SocketManageA4
send(byte[]) - Method in class com.rscja.team.qcom.socket.SocketTcpIpBase
send(byte[]) - Method in class com.rscja.team.qcom.socket.SocketUdpClient
sendAndReceive(byte[], int) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothData
sendAndReceive(byte[], byte[]) - Method in interface com.rscja.deviceapi.interfaces.IModule
  收发数据
sendAndReceive(byte[], byte[]) - Method in class com.rscja.deviceapi.Module
  收发数据
sendAndReceive(byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  收发数据
sendAndReceive(int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  收发数据
sendAndReceive(HardwareInterface_qcom.FunctionEnum, byte[]) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  收发数据
sendAndReceive(byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  收发数据
sendAndReceive(byte[]) - Method in class com.rscja.team.qcom.socket.SocketManageA4
sendAndReceive(byte[], int) - Method in class com.rscja.team.qcom.socket.SocketManageA4
sendAndReceive(byte[], int, int) - Method in class com.rscja.team.qcom.socket.SocketManageA4
sendAndReceive(byte[]) - Method in class com.rscja.team.qcom.socket.SocketManageUR4
sendAndReceive(byte[], int) - Method in class com.rscja.team.qcom.socket.SocketManageUR4
sendAndReceive(byte[]) - Method in class com.rscja.team.qcom.usb.R1HFUSB
sendAndReceive(byte[], int) - Method in class com.rscja.team.qcom.usb.R1HFUSB
sendAndReceive(byte[], boolean) - Method in class com.rscja.team.qcom.usb.RxUsb_qcom
sendAndReceive(byte[], boolean, int) - Method in class com.rscja.team.qcom.usb.RxUsb_qcom
sendAndReceive(byte[]) - Method in class com.rscja.team.qcom.usb.UrxUsb_qcom
sendAndReceive(byte[], int) - Method in class com.rscja.team.qcom.usb.UrxUsb_qcom
sendAndReceiveData(byte[], byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  收发数据
  sent/received data
sendAndReceiveData(byte[], byte[]) - Method in class com.rscja.deviceapi.Printer
  收发数据
  sent/received data
sendAndReceiveData(byte[], byte[]) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  收发数据
  sent/received data
sendBusCMD(char[], char[], int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  /** 墨西哥公交命令
  Mexico bus commande
sendBusCMD(char[], char[], int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  /** 墨西哥公交命令
  Mexico bus commande
sendBusCMD(char[], char[], int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A_mtk
  /** 墨西哥公交命令
  Mexico bus commande
sendBusCMD(char[], char[], int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A_qcom
  /** 墨西哥公交命令
  Mexico bus commande
sendBytes(byte[]) - Method in class com.rscja.team.qcom.serialportapi.SerialportAPI
sendCommand(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IHF14443B
  发送命令(send command)
sendCommand(String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A4CPU
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443B
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443A4CPU_mtk
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithISO14443B_mtk
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443A4CPU_qcom
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithISO14443B_qcom
  CPU卡 T=CL发送COS指令
  CPU card T=CL send COS command
sendCommand(byte[]) - Method in class com.rscja.team.qcom.r1.hf.HF14443B
  发送命令(send command)
sendContentToCursor(String) - Method in interface com.rscja.system.ISystemInterfaces
  将数据发送到光标位置
sendData(byte[]) - Method in class com.rscja.deviceapi.BluetoothReader
sendData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  发送指令(send data)
sendData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  发送数据到串口
  send data to serial port
sendData(byte[]) - Method in class com.rscja.deviceapi.Printer
  发送数据到串口
  send data to serial port
sendData(byte[]) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  发送数据到串口
  send data to serial port
sendData(byte[]) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
sendData(byte[]) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
sendData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
sendData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
sendData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
SendData(byte[], int) - Method in class com.rscja.team.qcom.serialportapi.SerialPort
sendData(byte[]) - Method in class com.rscja.team.qcom.usb.pl2302.UsbPL2302
sendData(byte[]) - Method in class com.rscja.team.qcom.usb.RxUsb_qcom
sendData(byte[]) - Method in class com.rscja.team.qcom.usb.UrxUsb_qcom
sendData(byte[]) - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
sendDataNotSyn(byte[]) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
sendOnThread(byte[]) - Method in class com.rscja.team.qcom.socket.SocketManageUR4
sendOnThread(byte[]) - Method in class com.rscja.team.qcom.socket.SocketTcpIpBase
sendOnThread(byte[]) - Method in class com.rscja.team.qcom.socket.SocketUdpClient
SerailClose(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SerailClose(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
SerailOpen(String, String, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SerailOpen(String, String, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
SerialPort - Class in com.rscja.team.qcom.serialportapi
SerialPort(File, int, int) - Constructor for class com.rscja.team.qcom.serialportapi.SerialPort
SerialportAPI - Class in com.rscja.team.qcom.serialportapi
setA4GPIO01SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
setA4GPIO02SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
setA4GPIO03SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
setA4GPIO04SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
setA4GPIOWgData0SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
setA4GPIOWgData1SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA4_qcom
setAddress(String) - Method in class com.rscja.deviceapi.BleDevice.BleDeviceInfo
setAfi(byte) - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity.Builder
setAFI(String) - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  设置AFI值
  setup AFI value
setAimId(String) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setAmbientTemperature(float) - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
setAngle(int) - Method in class com.rscja.deviceapi.entity.RadarLocationEntity.Builder
setAngle(int) - Method in class com.rscja.deviceapi.entity.RadarLocationEntity
  设置标签的方位角 (Set the azimuth of the label)
setAnimalFlag(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的AnimalFlag
  setup AnimalFlag of animal tag
setAnt(int) - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
setAnt(String) - Method in class com.rscja.custom.UHFSFForUrxNetwork.AntInfo
setAnt(int) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setAnt(int) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setAnt(AntennaEnum) - Method in class com.rscja.deviceapi.entity.AntennaPowerEntity
setAnt(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setANT(List<AntennaState>) - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
  设置天线
setANT(List<AntennaState>) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  设置天线
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  设置天线号
  Setup antenna number
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置天线启用状态(Set the antenna enable state)
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置天线启用状态(Set the antenna enable state)
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFA8
  设置天线号
  Setup antenna number
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置天线启用状态(Set the antenna enable state)
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置天线启用状态(Set the antenna enable state)
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
  设置天线号
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置天线
setANT(List<AntennaState>) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setANT(List<AntennaState>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  设置天线号
  Setup antenna number
setANT(List<AntennaState>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
  设置天线号
  Setup antenna number
setANT(List<AntennaState>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
  设置天线启用状态(Set the antenna enable state)
setANT(List<AntennaState>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setANT(List<AntennaState>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setANT(List<AntennaState>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置天线
setANT(List<AntennaState>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setAntBlinkSendData(byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setAntennaPower(AntennaEnum, int) - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
  设置单个天线的功率
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置天线功率 (Set the antenna power)
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置天线功率 (Set the antenna power)
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置天线功率 (Set the antenna power)
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置天线功率 (Set the antenna power)
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
setAntennaPower(AntennaEnum, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setAntSendData(char, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
setAntSendData(char, byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
setAntSendData(char, byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setAntWorkTimeSendData(byte, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
setAntWorkTimeSendData(byte, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
setAntWorkTimeSendData(byte, int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setBarcodeBytesData(byte[]) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setBarcodeBytesData(byte[]) - Method in class com.rscja.deviceapi.entity.BarcodeResult
setBarcodeCodeID(String) - Method in class com.rscja.deviceapi.entity.BarcodeResult
setBarcodeContinuousMode(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置扫描头连续扫描模式 (备注：键盘助手v2.3.5 之后的版本才支持)
  Setup UHF mode (Comment: Supports after keyboardemualator v2.3.5 has been released)
setBarcodeContinuousMode(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setBarcodeContinuousMode(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setBarcodeContinuousMode(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setBarcodeContinuousScan(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setBarcodeContinuousScanIntervalTime(int) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setBarcodeContinuousScanTimeOut(int) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setBarcodeData(String) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setBarcodeDecodeCallback(BluetoothReader.DecodeCallback) - Method in class com.rscja.team.qcom.uhfhandler.UHFRxBLEDataHandle
setBarcodeEncodingFormat(Context, int) - Method in class com.rscja.barcode.BarcodeUtility
  设置条码编码格式 Setup barcode coding format
setBarcodeEncodingFormat(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置条码编码格式 Setup barcode coding format
setBarcodeEncodingFormat(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置条码编码格式
  Setup barcode decoding format
setBarcodeEncodingFormat(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setBarcodeEncodingFormat(Context, int) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置条码编码格式 Setup barcode coding format
setBarcodeEncodingFormat(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setBarcodeEncodingFormat(Context, int) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置条码编码格式 Setup barcode coding format
setBarcodeEncodingFormat(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setBarcodeFormat(int) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setBarcodeHeight(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置一维条码的高度
  Setup 1D barcode height
setBarcodeHeight(int) - Method in class com.rscja.deviceapi.Printer
  设置一维条码的高度
  Setup 1D barcode height
setBarcodeHeight(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置一维条码的高度
  Setup 1D barcode height
setBarcodeHRI(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置一维条码可读字符（HRI）打印位置
  setup 1D barcode readable character (HRI) print position
setBarcodeHRI(int) - Method in class com.rscja.deviceapi.Printer
  设置一维条码可读字符（HRI）打印位置
  setup 1D barcode readable character (HRI) print position
setBarcodeHRI(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置一维条码可读字符（HRI）打印位置
  *setup 1D barcode readable character (HRI) print position
setBarcodeName(String) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setBarcodeSSIID(int) - Method in class com.rscja.deviceapi.entity.BarcodeResult
setBarcodeSSIID(boolean) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setBarcodeSymbology(int) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setBarcodeType(boolean) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setBarcodeTypeInSSIID(boolean) - Method in class com.rscja.deviceapi.BluetoothReader
setBarcodeTypeInSSIID(boolean) - Method in interface com.rscja.deviceapi.interfaces.IReader
setBarcodeTypeInSSIID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setBarcodeTypeInSSIID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setBarcodeTypeInSSIID(boolean) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setBarcodeTypeInSSIID(boolean) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setBarcodeTypeInSSIID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setBarcodeWidth(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置一维条码的宽度
  Setup 1D barcode width
setBarcodeWidth(int) - Method in class com.rscja.deviceapi.Printer
  设置一维条码的宽度
  Setup 1D barcode width
setBarcodeWidth(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置一维条码的宽度
  Setup 1D barcode width
setBaudrate(int) - Method in class com.rscja.deviceapi.Barcode1D
setBaudrate(int) - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
setBaudrate(int) - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
setBaudrate(int) - Method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  设置波特率
  Setup baudrate
setBaudrate(int) - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
setBaudrate(int) - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  设置波特率
  Setup baudrate
setBeep(boolean) - Method in class com.rscja.deviceapi.BleDevice
  设置蜂鸣器开关
  Setup buzzer ON/OFF
setBeep(boolean) - Method in class com.rscja.deviceapi.BluetoothReader
setBeep(boolean) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setBeep(boolean) - Method in interface com.rscja.deviceapi.interfaces.IReader
  设置蜂鸣器开关
  Setup buzzer ON/OFF
setBeep(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setBeep(boolean) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setBeep(boolean) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setBeep(boolean) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setBeep(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setBeepTimeOfDurationSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setBeepTimeOfDurationSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setBlackWhiteListState(int) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setBlackWhiteListState(int) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setBluetoothDevice(BluetoothDevice) - Method in class com.rscja.deviceapi.BleDevice.BleDeviceInfo
setBluetoothReader(IBluetoothData) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
setBluetoothReader(IBluetoothData) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
setBtName(String) - Method in class com.rscja.team.qcom.service.BLEService_qcom
setBuzzerOff() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setBuzzerOff() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  关闭蜂鸣器鸣叫，此函数与盘点无关
setBuzzerOff() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  关闭蜂鸣器鸣叫，此函数与盘点无关
setBuzzerOff() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  关闭蜂鸣器鸣叫，此函数与盘点无关
setBuzzerOff() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  关闭蜂鸣器鸣叫，此函数与盘点无关
setBuzzerOffOfAndroidSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setBuzzerOn(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
  单位:毫秒,time:100-65535
setBuzzerOn(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置蜂鸣器鸣叫，此函数与盘点无关，不管是否盘点到标签都会鸣叫
setBuzzerOn(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置蜂鸣器鸣叫，此函数与盘点无关，不管是否盘点到标签都会鸣叫
setBuzzerOn(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置蜂鸣器鸣叫，此函数与盘点无关，不管是否盘点到标签都会鸣叫
setBuzzerOn(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置蜂鸣器鸣叫，此函数与盘点无关，不管是否盘点到标签都会鸣叫
setBuzzerOnOfAndroidSendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setCalibrationData(String) - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
setCalibrationData(String) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setCalibrationData(String) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setCameraState(boolean) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setCameraState(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setCheckConnectState(SocketManageUR4.CheckConnectState) - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
setCheckConnectState(SocketManageUR4.CheckConnectState) - Method in class com.rscja.team.qcom.socket.SocketManageUR4
setCheckGPIO(boolean) - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
setCheckGPIO(boolean) - Method in class com.rscja.team.qcom.socket.SocketManageA4
setChipInfo(UHFTAGInfo.ChipInfo) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setChipType(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo.Builder
SetConfig(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SetConfig(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.BleDevice
  设置UHF连接状态回调
  Setup UHF continuous stauts call-back
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.BluetoothReader
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  设置蓝牙连接状态的回调(Setup Bluetooth connection status call back)
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置UHF连接状态回调
  Setup UHF continuous stauts call-back
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置监听连接状态(Set the listening connection status)
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置监听连接状态(Set the listening connection status)
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置监听连接状态(Set the listening connection status)
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置监听连接状态(Set the listening connection status)
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置UHF连接状态回调
  Setup UHF continuous stauts call-back
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置UHF连接状态回调
  Setup UHF continuous stauts call-back
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setConnectionStatusCallback(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setConnectionStatusCallback(ConnectionStatusCallback) - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
setConnectionStatusChangedListener(IConnectionStatusChangedListener) - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
setConnectionStatusChangedListener(IConnectionStatusChangedListener) - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
setConnectionStatusChangedListener(IConnectionStatusChangedListener) - Method in class com.rscja.team.qcom.socket.SocketManageA4
setConnectionStatusChangedListener(IConnectionStatusChangedListener) - Method in class com.rscja.team.qcom.socket.SocketManageUR4
setContainAnt(boolean) - Method in class com.rscja.deviceapi.entity.TagInfoRule
  设置标签是否包含天线信息
setContinuousScan(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  设置条码连续扫描
  Setup barcode continuous scanning
setContinuousScan(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
setContinuousScan(Context, boolean) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setContinuousScan(Context, boolean) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setContinuousScanIntervalTime(Context, int) - Method in class com.rscja.barcode.BarcodeUtility
  设置连续扫描间隔时间 Setup continuous scanning duration
setContinuousScanIntervalTime(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置连续扫描间隔时间 Setup continuous scanning duration
setContinuousScanIntervalTime(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置条码连续扫描间隔时间
  Setup barcode continuous scanning intervals
setContinuousScanIntervalTime(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setContinuousScanIntervalTime(Context, int) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置连续扫描间隔时间 Setup continuous scanning duration
setContinuousScanIntervalTime(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setContinuousScanIntervalTime(Context, int) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置连续扫描间隔时间 Setup continuous scanning duration
setContinuousScanIntervalTime(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setContinuousScanIntervalTimeRFID(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置UHF连续扫描间隔时间
  Setup UHF continuous scanning intervals
setContinuousScanIntervalTimeRFID(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setContinuousScanIntervalTimeRFID(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setContinuousScanIntervalTimeRFID(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setContinuousScanRFID(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  设置UHF连续扫描
  Setup UHF continuous scann
setContinuousScanRFID(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
setContinuousScanRFID(Context, boolean) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setContinuousScanRFID(Context, boolean) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setContinuousScanTimeOut(Context, int) - Method in class com.rscja.barcode.BarcodeUtility
  设置连续扫描超时时间 Setup continuous scanning overtime duration
setContinuousScanTimeOut(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置连续扫描超时时间 Setup continuous scanning overtime duration
setContinuousScanTimeOut(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置条码连续扫描超时时间
  Setup barcode continuous scanning time-out interval
setContinuousScanTimeOut(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setContinuousScanTimeOut(Context, int) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置连续扫描超时时间 Setup continuous scanning overtime duration
setContinuousScanTimeOut(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setContinuousScanTimeOut(Context, int) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置连续扫描超时时间 Setup continuous scanning overtime duration
setContinuousScanTimeOut(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setContinuousScanTimeOutRFID(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置UHF连续扫描超时时间
  Setup UHF continuous scanning time-out interval
setContinuousScanTimeOutRFID(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setContinuousScanTimeOutRFID(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setContinuousScanTimeOutRFID(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setControlWork(int) - Method in class com.rscja.deviceapi.entity.GPIOInfo
setCount(int) - Method in class com.rscja.custom.UHFSFForUrxNetwork.AntInfo
setCount(int) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setCountryID(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的国家代码
  setup national code of animal tag
setCurrentNumber(int) - Method in class com.rscja.custom.UHFTemperatureTagsAPI.MultipleTemperatureInfo
setCW(int) - Method in class com.rscja.deviceapi.BleDevice
  设置连续波
  Setup CW
setCW(int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setCW(int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置连续波
  Setup CW
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置连续波(continuous waves)
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置连续波(continuous waves)
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置连续波(continuous waves)
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置连续波(continuous waves)
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置连续波
  Setup CW
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setCW(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setCW(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setCW(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置连续波
  Setup CW
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setCW(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setCWSendData(char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setCWSendData(char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setData(String) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置数据，仅对数据文件类型有效
  setup data, it is valid for value file type only
setData(byte[]) - Method in class com.rscja.deviceapi.entity.GPIOInfo
setData(String) - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  设置标签数据
  setup tag data
setData(byte[]) - Method in class com.rscja.team.qcom.http.NetResult_qcom
setDataBlock(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的DataBlock
  setup DataBlock of animal tag
setDataCallBack(BLEService_qcom.IDataCallBack) - Method in class com.rscja.team.qcom.service.BLEService_qcom
setDataCallback(UsbBase_qcom.DataCallback) - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
setDebug(boolean) - Static method in class com.rscja.team.mtk.utility.LogUtility_mtk
setDebug(boolean) - Static method in class com.rscja.team.qcom.utility.LogUtility_qcom
setDebug(boolean) - Static method in class com.rscja.utility.StringUtility
setDecodeCallback(BarcodeDecoder.DecodeCallback) - Method in class com.rscja.barcode.BarcodeDecoder
  设置回调对象接收条码数据,主线程回调
  Setup call-back target to acquire barcode data.
setDecodeCallback(BarcodeDecoder.DecodeCallback) - Method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
setDecodeCallback(BarcodeDecoder_mtk.DecodeCallback) - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  设置回调对象接收条码数据,主线程回调
  Setup call-back target to acquire barcode data.
setDecodeCallback(BarcodeDecoder.DecodeCallback) - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
setDecodeTime(int) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setDesfid(byte) - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity.Builder
setDESFID(String) - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  设置DESFID值
  setup DESFID value
setDestIP(ReaderIPEntity) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  设置目标IP
setDestIP(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setDestIP(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置目标IP
setDestIP(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setDestIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setDestIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setDestIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置目标IP
setDestIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setDeviceName(String) - Method in class com.rscja.deviceapi.Fingerprint
  设置设备名称
  Setup device name
setDeviceName(String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  设置设备名称
  Setup device name
setDeviceName(String) - Method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  设置设备名
  Setup device name
setDeviceName(String) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  设置设备名称
  Setup device name
setDeviceName(String) - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  设置设备名
  Setup device name
setDns1(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setDns2(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setDTR(boolean) - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Sets the DTR (Data Terminal Ready) bit on the underlying UART, if supported.
setDTR(boolean) - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
setDynamicDistance(int) - Method in interface com.rscja.deviceapi.interfaces.IHandheldRFID
  Radar positioning dynamically adjusts distance.
setDynamicDistance(int) - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
  Radar positioning dynamically adjusts distance.
setDynamicDistance(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  Radar positioning dynamically adjusts distance.
setDynamicDistance(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  Radar positioning dynamically adjusts distance.
setDynamicDistance(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  Radar positioning dynamically adjusts distance.
setDynamicDistance(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setDynamicDistance(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setDynamicDistance(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setDynamicDistance(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setDynamicDistance(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setEnable(boolean) - Method in class com.rscja.deviceapi.entity.AntennaState
setEnable(boolean) - Static method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
setEnable(boolean) - Static method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
setEnable4G(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置4G 禁用、启用
setEnable4G(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnable4G(boolean) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setEnable4G(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setEnableBackKey(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  返回按键 禁用、启用
setEnableBackKey(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnableBackKey(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnableBackKey(boolean) - Method in class com.rscja.team.qcom.system.SysInterfacesOfC66P_qcom
setEnableBarcode2D(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setEnableBlueth(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置Blueth 禁用、启用
setEnableBlueth(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnableBlueth(boolean) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setEnableBlueth(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setEnableCamera(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置Camera 禁用、启用
setEnableHomeKey(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置Home按键禁用、启用
setEnableHomeKey(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnableHomeKey(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnableHomeKey(boolean) - Method in class com.rscja.team.qcom.system.SysInterfacesOfC66P_qcom
setEnableKeyMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setEnableMenuKey(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置Menu按键 禁用、启用
setEnableMenuKey(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnableMenuKey(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnableMenuKey(boolean) - Method in class com.rscja.team.qcom.system.SysInterfacesOfC66P_qcom
setEnableNavigationBar(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置虚拟导航栏禁用、启用
setEnableNavigationBar(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnableNavigationBar(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setEnableOtg(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置OTG 禁用、启用
setEnableOtg(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnablePanelBar(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置下拉面板禁用、启用
setEnablePanelBar(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnablePanelBar(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnablePanelBar(boolean) - Method in class com.rscja.team.qcom.system.SysInterfacesOfC66P_qcom
setEnableRecentKey(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  最近APP使用记录按键 禁用、启用
setEnableRecentKey(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnableRecentKey(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnableRecentKey(boolean) - Method in class com.rscja.team.qcom.system.SysInterfacesOfC66P_qcom
setEnableScanner(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setEnableScapKey(Context, boolean) - Method in class com.rscja.team.mtk.system.SystemSettingsDBData_mtk
setEnableScreensho(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置屏幕截图 禁用、启用
setEnableScreensho(boolean) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setEnableScreenshot(boolean) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setEnableScreenshot(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setEnableSystemSettingButton(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置音量加减界面的设置按钮的禁用、启用
setEnableSystemSettingButton(boolean) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setEnableSystemSettingButton(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setEnableTurnkey(boolean) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setEnableWifi(boolean) - Method in interface com.rscja.system.ISystemInterfaces
  设置wifi 禁用、启用,需要申请android.permission.CHANGE_WIFI_STATE权限
setEnableWifi(boolean) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setEnableWifi(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setEnrollCallBack(FingerprintWithFIPS.EnrollCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置采集指纹回调接口
  Setup call-back contact for acquiring fingerprint
setEnrollCallBack(FingerprintWithFIPS.EnrollCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  设置采集指纹回调接口
  Setup call-back contact for acquiring fingerprint
setEnrollCallBack(FingerprintWithFIPS.EnrollCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  设置采集指纹回调接口
  Setup call-back contact for acquiring fingerprint
setEnrollCallBack(FingerprintWithFIPS.EnrollCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  设置采集指纹回调接口
  Setup call-back contact for acquiring fingerprint
setEnter(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setEpc(String) - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
setEpc(String) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setEpc(String) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setEPC(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setEPCAndTamperAlarm() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFUARTUAE
setEPCAndTamperAlarm() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
setEPCAndTamperAlarmMode() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFUARTUAE
setEPCAndTamperAlarmMode() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
setEPCAndTamperMode() - Method in interface com.rscja.custom.interfaces.IUHFTamperAPI
setEPCAndTamperMode() - Method in class com.rscja.custom.UHFTamperAPI
setEPCAndTamperMode() - Method in class com.rscja.team.qcom.custom.UHFTamperAPI_qcom
setEPCAndTemperatureMode() - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
setEPCAndTemperatureMode() - Method in class com.rscja.custom.UHFTemperatureTagsAPI
setEPCAndTemperatureMode() - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
  设置盘点标签为EPC+温度模式
setEPCAndTemperatureMode() - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
  设置盘点标签为EPC+温度模式
setEPCAndTemperatureMode() - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
setEPCAndTemperatureModeRequest(char, int, int, int) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
setEPCAndTemperatureModeRequest(char, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
setEPCAndTemperatureModeResponse(byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
setEPCAndTemperatureModeResponse(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
setEPCAndTIDMode() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFShuangYingDianZi
setEPCAndTIDMode() - Method in class com.rscja.custom.UHFTemperatureSensors
setEPCAndTIDMode() - Method in class com.rscja.custom.UHFXSAPI
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.BleDevice
  设置循环盘点同时读取 EPC、TID 模式
  Setup auto scan to acquire EPC, TID mode
setEPCAndTIDMode() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setEPCAndTIDMode() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置循环盘点同时读取 EPC、TID 模式
  Setup auto scan to acquire EPC, TID mode
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置盘点模式为EPC+TID，返回标签的EPC+TID数据 (Set the inventory mode to EPC+TID, and return the EPC+TID data of the label)
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置盘点模式为EPC+TID，返回标签的EPC+TID数据 (Set the inventory mode to EPC+TID, and return the EPC+TID data of the label)
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置盘点模式为EPC+TID，返回标签的EPC+TID数据 (Set the inventory mode to EPC+TID, and return the EPC+TID data of the label)
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置盘点模式为EPC+TID，返回标签的EPC+TID数据 (Set the inventory mode to EPC+TID, and return the EPC+TID data of the label)
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置循环盘点同时读取 EPC、TID 模式
  Setup auto scan to acquire EPC, TID mode
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setEPCAndTIDMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setEPCAndTIDMode() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置循环盘点同时读取 EPC、TID 模式
  Setup auto scan to acquire EPC, TID mode
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setEPCAndTIDMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setEPCAndTIDModeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setEPCAndTIDModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setEPCAndTidReservedModeEx(String, int, int, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFShuangYingDianZi
  设置循环盘点同时读取 TID + EPC区 + Reserve区
  Setup auto scan to acquire EPC, TID, Reserved mode
setEPCAndTidReservedModeEx(int, int, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFShuangYingDianZi
setEPCAndTidReservedModeEx(String, int, int, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
  设置循环盘点同时读取 TID + EPC区 + Reserve区
  Setup auto scan to acquire EPC, TID, Reserved mode
setEPCAndTidReservedModeEx(int, int, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.custom.UHFTemperatureSensors
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.custom.UHFXSAPI
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.BleDevice
  设置循环盘点同时读取 EPC、TID、USER 模式
  Setup auto scan to acquire EPC, TID, User mode
setEPCAndTIDUserMode(int, int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setEPCAndTIDUserMode(int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置循环盘点同时读取 EPC、TID、USER 模式
  Setup auto scan to acquire EPC, TID, User mode
setEPCAndTIDUserMode(InventoryModeEntity) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置循环盘点同时读取 EPC、TID、USER 模式
  Setup auto scan to acquire EPC, TID, User mode
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置盘点模式为EPC+TID+USER，返回标签的EPC+TID+USER数据 (Set the inventory mode to EPC+TID+USER, and return the EPC+TID+USER data of the label)
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置盘点模式为EPC+TID+USER，返回标签的EPC+TID+USER数据 (Set the inventory mode to EPC+TID+USER, and return the EPC+TID+USER data of the label)
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置盘点模式为EPC+TID+USER，返回标签的EPC+TID+USER数据 (Set the inventory mode to EPC+TID+USER, and return the EPC+TID+USER data of the label)
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置盘点模式为EPC+TID+USER，返回标签的EPC+TID+USER数据 (Set the inventory mode to EPC+TID+USER, and return the EPC+TID+USER data of the label)
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  设置循环盘点同时读取 EPC、TID、USER 模式
  Setup auto scan to acquire EPC, TID, User mode
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置循环盘点同时读取 EPC、TID、USER 模式
  Setup auto scan to acquire EPC, TID, User mode
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.deviceapi.UhfBase
  设置循环盘点同时读取 EPC、TID、USER 模式
  Setup auto scan to acquire EPC, TID, User mode
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setEPCAndTIDUserMode(InventoryModeEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置循环盘点同时读取 EPC、TID、USER 模式
  Setup auto scan to acquire EPC, TID, User mode
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setEPCAndTIDUserMode(int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setEPCAndTIDUserModeEx(int, int, int, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFShuangYingDianZi
setEPCAndTIDUserModeEx(int, int, int, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
setEPCAndTIDUserModeEx(int, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setEPCAndTIDUserModeSendData(int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setEPCAndTIDUserModeSendData(int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setEPCAndTIDUserModeSendData(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setEPCAndUserReservedModeEx(int, int, int, int, int) - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFShuangYingDianZi
setEPCAndUserReservedModeEx(int, int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setEPCAndUserReservedModeEx(int, int, int, int, int) - Method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
setEPCAndUserReservedModeEx(int, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setEpcBytes(byte[]) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setEPCMode() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFShuangYingDianZi
setEPCMode() - Method in interface com.rscja.custom.interfaces.IRFIDWithUHFUARTUAE
  设置读取 EPC模式设置
setEPCMode() - Method in class com.rscja.custom.UHFXSAPI
setEPCMode() - Method in class com.rscja.deviceapi.BleDevice
  设置循环盘点只获取EPC的数据
  Setup auto scan to acquire EPC only
setEPCMode() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setEPCMode() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置循环盘点只获取EPC的数据
  Setup auto scan to acquire EPC only
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置盘点模式为EPC，只返回标签的EPC数据 (Set the inventory mode to EPC, and only return the EPC data of the label)
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置盘点模式为EPC，只返回标签的EPC数据 (Set the inventory mode to EPC, and only return the EPC data of the label)
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置盘点模式为EPC，只返回标签的EPC数据 (Set the inventory mode to EPC, and only return the EPC data of the label)
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置盘点模式为EPC，只返回标签的EPC数据 (Set the inventory mode to EPC, and only return the EPC data of the label)
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置循环盘点只获取EPC的数据
  Setup auto scan to acquire EPC only
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setEPCMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setEPCMode() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setEPCMode() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setEPCMode() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFShuangYingDianZi_qcom
setEPCMode() - Method in class com.rscja.team.qcom.custom.RFIDWithUHFUARTUAE_qcom
  设置读取 EPC模式设置
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置循环盘点只获取EPC的数据
  Setup auto scan to acquire EPC only
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setEPCMode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setEPCModeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setEPCModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setEPCSensorsMode() - Method in class com.rscja.custom.UHFTemperatureSensors
setErrCode(int) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setEthernetConfigInfo(ReaderIPEntity) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setEthernetConfigInfo(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置以太网IP地址
setEthernetConfigInfo(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置以太网IP地址
setEthernetConfigInfo(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置以太网IP地址
setEthernetConfigInfo(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置以太网IP地址
setEthernetConfigInfoSendData(ReaderIPEntity) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setEthernetDynamicSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setEthernetIpDynamicAssign() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setEthernetIpDynamicAssign() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置以太网获取动态IP
setEthernetIpDynamicAssign() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置以太网获取动态IP
setEthernetIpDynamicAssign() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置以太网获取动态IP
setEthernetIpDynamicAssign() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置以太网获取动态IP
setExtraData(String, String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setFactory(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo.Builder
setFailureSound(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setFastID(boolean) - Method in class com.rscja.deviceapi.BleDevice
  开关FastID功能
  ON/OFF FastID function
setFastID(boolean) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setFastID(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  开关FastID功能
  ON/OFF FastID function
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  开关FastID功能 (Switch FastID function)
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  开关FastID功能 (Switch FastID function)
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  开关FastID功能 (Switch FastID function)
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  开关FastID功能 (Switch FastID function)
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  开关FastID功能
  ON/OFF FastID function
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setFastID(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setFastID(boolean) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setFastID(boolean) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  开关FastID功能
  ON/OFF FastID function
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setFastID(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setFastIdSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setFastIdSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setFastInventoryMode(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  setFastInventory
setFastInventoryMode(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  setFastInventory
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  setFastInventory
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  setFastInventory
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  setFastInventory
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  setFastInventory
setFastInventoryMode(boolean) - Method in class com.rscja.deviceapi.UhfBase
setFastInventoryMode(boolean) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setFastInventoryMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setFastInventoryMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setFastInventoryMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setFastInventoryMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
  setFastInventory
setFastInventoryMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
  setFastInventory
setFeedRow(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印并进纸 n行
  print and paper infeed n
setFeedRow(int) - Method in class com.rscja.deviceapi.Printer
  打印并进纸 n行
  print and paper infeed n
setFeedRow(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  打印并进纸 n行
  print and paper infeed n
setFileSize(int) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置文件大小，仅对数据文件类型有效
  setup file size, it is valid for data file type only
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.BleDevice
  过滤循环盘点的标签，在`BleDevice.startInventoryTag()`循环盘点标签之前，可以设置要过滤的数据。
  Filter tag in auto scan mode, before scanning tags `BleDevice.startInventoryTag()`, setup data that needs to be filtered.
setFilter(int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setFilter(int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  过滤循环盘点的标签，在`IUHF.startInventoryTag()`循环盘点标签之前，可以设置要过滤的数据。
  Filter tag in auto scan mode, before scanning tags `IUHF.startInventoryTag()`, setup data that needs to be filtered.
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置循环盘点符合过滤条件的标签，不符合过滤条件的标签将不会上传。注意：必须在循环盘点标签之前设置
  Set up a round-robin inventory of tags that meet the filter conditions, and tags that do not meet the filter conditions will not be uploaded.
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置循环盘点符合过滤条件的标签，不符合过滤条件的标签将不会上传。注意：必须在循环盘点标签之前设置
  Set up a round-robin inventory of tags that meet the filter conditions, and tags that do not meet the filter conditions will not be uploaded.
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置循环盘点符合过滤条件的标签，不符合过滤条件的标签将不会上传。注意：必须在循环盘点标签之前设置
  Set up a round-robin inventory of tags that meet the filter conditions, and tags that do not meet the filter conditions will not be uploaded.
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置循环盘点符合过滤条件的标签，不符合过滤条件的标签将不会上传。注意：必须在循环盘点标签之前设置
  Set up a round-robin inventory of tags that meet the filter conditions, and tags that do not meet the filter conditions will not be uploaded.
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  过滤循环盘点的标签，在`RFIDWithUHFUrxUart.startInventoryTag()`循环盘点标签之前，可以设置要过滤的数据。
  Filter tag in auto scan mode, before scanning tags `RFIDWithUHFUrxUart.startInventoryTag()`, setup data that needs to be filtered.
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setFilter(int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setFilter(int, int, int, String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  过滤循环盘点的标签，在`RFIDWithUHFUrxUart_qcom.startInventoryTag()`循环盘点标签之前，可以设置要过滤的数据。
  Filter tag in auto scan mode, before scanning tags `RFIDWithUHFUrxUart_qcom.startInventoryTag()`, setup data that needs to be filtered.
  设置过滤条件之后，盘点标签时将符合过滤条件的标签上传到缓存区`RFIDWithUHFUrxUart_qcom.readTagFromBuffer()`。
  After setup, upload filtered tags to buffer `RFIDWithUHFUrxUart_qcom.readTagFromBuffer()`.
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setFilter(int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setFilterChars(String) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setFilterSendData(char, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setFilterSendData(char, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setFreHop(float) - Method in class com.rscja.deviceapi.BleDevice
  设置模块频点
  Setup frequency Hop
setFreHop(float) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setFreHop(float) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置模块频点
  Setup frequency Hop
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置模块频点(Setup frequency Hop)
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置模块频点(Setup frequency Hop)
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置模块频点(Setup frequency Hop)
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置模块频点(Setup frequency Hop)
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置模块频点
  Setup frequency Hop
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setFreHop(float) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setFreHop(float) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setFreHop(float) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置模块频点
  Setup frequency Hop
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setFreHop(float) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setFrequencyMode(int) - Method in class com.rscja.deviceapi.BleDevice
  设置模块的工作模式
  Setup work mode of module
setFrequencyMode(int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setFrequencyMode(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
setFrequencyMode(int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置模块的工作模式
  Setup work mode of module
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置模块的工作频率(Set the operating frequency of the module)
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置模块的工作频率(Set the operating frequency of the module)
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置模块的工作频率(Set the operating frequency of the module)
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置模块的工作频率(Set the operating frequency of the module)
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setFrequencyMode(byte) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setFrequencyMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setFrequencyMode(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setFrequencyMode(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setFrequencyMode(byte) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setFrequencyMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setFrequencyModeSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setFrequencyModeSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setFrequencyPoint(float) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setFullData(byte[]) - Method in class com.rscja.deviceapi.entity.GPIOInfo
setGateway(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.BleDevice
  设置 Gen2参数
  Setup Gen2 parameter
setGen2(Gen2Entity) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setGen2(Gen2Entity) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置GEN2参数值 (Set GEN2 parameter value)
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置GEN2参数值 (Set GEN2 parameter value)
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置GEN2参数值 (Set GEN2 parameter value)
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置GEN2参数值 (Set GEN2 parameter value)
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置GEN2参数值 (Set GEN2 parameter value)
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置 Gen2参数
  Setup Gen2 parameter
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setGen2(Gen2Entity) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
SetGen2(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
setGen2(Gen2Entity) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
SetGen2(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setGen2(int, int, int, int, int, int, int, int, int, int, int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置 Gen2参数
  Setup Gen2 parameter
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setGen2(Gen2Entity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setGen2SendData(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setGen2SendData(char, char, char, char, char, char, char, char, char, char, char, char, char, char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setGpiName(String) - Method in class com.rscja.deviceapi.entity.GPIStateEntity
setGPIO03SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA8_qcom
setGPIO04SendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrA8_qcom
setGpiState(int) - Method in class com.rscja.deviceapi.entity.GPIStateEntity
setGPIStateCallback(IGPIStateCallback) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setGPIStateCallback(IGPIStateCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置GPIO状态回调接口
setGPIStateCallback(IGPIStateCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置GPIO状态回调接口
setGPIStateCallback(IGPIStateCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置GPIO状态回调接口
setGPIStateCallback(IGPIStateCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置GPIO状态回调接口
setGPIStateReverse(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setGPIStateReverse(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
setGPIStateReverse(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
setGPIStateReverse(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
setGPIStateReverse(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
setGPIStateReverse(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4NetWork_qcom
setGPIStateReverse(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4RS232_qcom
setGPIStateReverse(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8NetWork_qcom
setGPIStateReverse(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8RS232_qcom
setGpoName(String) - Method in class com.rscja.deviceapi.entity.GPOEntity
setGpoState(int) - Method in class com.rscja.deviceapi.entity.GPOEntity
setGrabCallBack(FingerprintWithFIPS.GRABCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置获取图片回调接口
  Setup call-back contact for acquiring picture
setGrabCallBack(FingerprintWithMorpho.GrabCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
setGrabCallBack(FingerprintWithFIPS.GRABCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  设置获取图片回调接口
  Setup call-back contact for acquiring picture
setGrabCallBack(FingerprintWithMorpho.GrabCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
setGrabCallBack(FingerprintWithFIPS.GRABCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  设置获取图片回调接口
  Setup call-back contact for acquiring picture
setGrabCallBack(FingerprintWithMorpho.GrabCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
setGrabCallBack(FingerprintWithFIPS.GRABCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  设置获取图片回调接口
  Setup call-back contact for acquiring picture
setGrabCallBack(FingerprintWithMorpho.GrabCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
setGroupSeparator(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  是否去掉分组符
  Delete D GS
setGroupSeparator(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
setGroupSeparator(Context, boolean) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setGroupSeparator(Context, boolean) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setHexChallenge(String) - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
setHexTagResponse(String) - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
setHexTagsShortenedTID(String) - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
setId(String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
setID(String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置指纹模块ID
  Setup fingerprint module ID
setID(String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  设置指纹模块ID
  Setup fingerprint module ID
setID(String) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  设置指纹模块ID
  Setup fingerprint module ID
setID(String) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  设置指纹模块ID
  Setup fingerprint module ID
setIdData(String) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置64bit的识别号数据，十六进制表示
  setup 64bit identification number, hexdecimal
setIdentificationCallBack(FingerprintWithFIPS.IdentificationCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置指纹验证回调接口
  Setup fingerprint verification
setIdentificationCallBack(FingerprintWithMorpho.IdentificationCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置指纹验证回调接口
  setup fingerprint verification call-back contact
setIdentificationCallBack(FingerprintWithFIPS.IdentificationCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  设置指纹验证回调接口
  Setup fingerprint verification
setIdentificationCallBack(FingerprintWithMorpho.IdentificationCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  设置指纹验证回调接口
  setup fingerprint verification call-back contact
setIdentificationCallBack(FingerprintWithFIPS.IdentificationCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  设置指纹验证回调接口
  Setup fingerprint verification
setIdentificationCallBack(FingerprintWithMorpho.IdentificationCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  设置指纹验证回调接口
  setup fingerprint verification call-back contact
setIdentificationCallBack(FingerprintWithFIPS.IdentificationCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  设置指纹验证回调接口
  Setup fingerprint verification
setIdentificationCallBack(FingerprintWithMorpho.IdentificationCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  设置指纹验证回调接口
  setup fingerprint verification call-back contact
setIndex(int) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setIndexData(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setInterceptTrimLeft(int) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setInterceptTrimRight(int) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setInventoryBank(UHFXSAPI.Bank, int, int) - Method in class com.rscja.custom.UHFXSAPI
setInventoryCallback(M775Authenticate.IUHFInventoryCallback) - Method in interface com.rscja.custom.interfaces.IM775Authenticate
setInventoryCallback(UHFCSYX.IUHFInventoryCallback) - Method in interface com.rscja.custom.interfaces.IUHFCSYX
setInventoryCallback(UHFTemperatureTagsAPI.IUHFInventoryTempCallback) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
setInventoryCallback(M775Authenticate.IUHFInventoryCallback) - Method in class com.rscja.custom.M775Authenticate
setInventoryCallback(UHFCSYX.IUHFInventoryCallback) - Method in class com.rscja.custom.UHFCSYX
setInventoryCallback(UHFCSYX.IUHFInventoryCallback) - Method in class com.rscja.custom.UHFCSYX_A4NetWork
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.custom.UHFCSYX_A4NetWork
setInventoryCallback(UHFCSYX.IUHFInventoryCallback) - Method in class com.rscja.custom.UHFCSYXForURx
setInventoryCallback(UHFTemperatureSensors.IUHFInventoryTemperatureTagCallback) - Method in class com.rscja.custom.UHFTemperatureSensors
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.custom.UHFTemperatureSensors
setInventoryCallback(UHFTemperatureTagsAPI.IUHFInventoryTempCallback) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.custom.UHFXSAPI
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.BleDevice
  设置盘点回调接口，接收循环盘点到的标签数据
  Set the inventory callback interface to receive the label data from the cyclic inventory
  备注：需要在开始循环盘点`BleDevice.startInventoryTag()`之前调用此方法。
  Note: This method needs to be called before starting the loop inventory `BleDevice.startInventoryTag()`.
setInventoryCallback(IUHFInventoryCallback) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setInventoryCallback(IUHFInventoryCallback) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置盘点回调接口，接收循环盘点到的标签数据
  Set the inventory callback interface to receive the label data from the cyclic inventory
  备注：需要在开始循环盘点`IUHF.startInventoryTag()`之前调用此方法。
  Note: This method needs to be called before starting the loop inventory `IUHF.startInventoryTag()`.
setInventoryCallback(IUHFInventoryCallback) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA4
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置盘点回调接口，接收循环盘点到的标签数据
  Set the inventory callback interface to receive the label data from the cyclic inventory
  备注：需要在开始循环盘点`RFIDWithUHFA4NetWork.startInventoryTag()`之前调用此方法。
  Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA4NetWork.startInventoryTag()`.
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置盘点回调接口，接收循环盘点到的标签数据
  Set the inventory callback interface to receive the label data from the cyclic inventory
  备注：需要在开始循环盘点`RFIDWithUHFA4RS232.startInventoryTag()`之前调用此方法。
  Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA4RS232.startInventoryTag()`.
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA8
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置盘点回调接口，接收循环盘点到的标签数据
  Set the inventory callback interface to receive the label data from the cyclic inventory
  备注：需要在开始循环盘点`RFIDWithUHFA8NetWork.startInventoryTag()`之前调用此方法。
  Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA8NetWork.startInventoryTag()`.
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置盘点回调接口，接收循环盘点到的标签数据
  Set the inventory callback interface to receive the label data from the cyclic inventory
  备注：需要在开始循环盘点`RFIDWithUHFA8RS232.startInventoryTag()`之前调用此方法。
  Note: This method needs to be called before starting the loop inventory `RFIDWithUHFA8RS232.startInventoryTag()`.
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  设置盘点回调接口，接收循环盘点到的标签数据
  Set the inventory callback interface to receive the label data from the cyclic inventory
  备注：需要在开始循环盘点`RFIDWithUHFUART.startInventoryTag()`之前调用此方法。
  Note: This method needs to be called before starting the loop inventory `RFIDWithUHFUART.startInventoryTag()`.
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setInventoryCallback(M775Authenticate.IUHFInventoryCallback) - Method in class com.rscja.team.mtk.custom.M775Authenticate_mtk
setInventoryCallback(UHFTemperatureTagsAPI.IUHFInventoryTempCallback) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
  盘点温度标签回调
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
setInventoryCallback(M775Authenticate.IUHFInventoryCallback) - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
setInventoryCallback(UHFCSYX.IUHFInventoryCallback) - Method in class com.rscja.team.qcom.custom.UHFCSYX_qcom
setInventoryCallback(UHFTemperatureTagsAPI.IUHFInventoryTempCallback) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
  盘点温度标签回调
setInventoryCallback(UHFTemperatureTagsAPI.IUHFInventoryTempCallback) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setInventoryCallback(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
SetInventoryFixed(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SetInventoryFixed(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
setInventoryMessageMode() - Method in interface com.rscja.custom.interfaces.IM775Authenticate
  设置读取Message模式(Set Read Message Mode)
setInventoryMessageMode() - Method in interface com.rscja.custom.interfaces.IUHFCSYX
setInventoryMessageMode() - Method in class com.rscja.custom.M775Authenticate
  设置读取Message模式(Set Read Message Mode)
setInventoryMessageMode() - Method in class com.rscja.custom.UHFCSYX
setInventoryMessageMode() - Method in class com.rscja.custom.UHFCSYX_A4NetWork
setInventoryMessageMode() - Method in class com.rscja.custom.UHFCSYXForURx
setInventoryMessageMode() - Method in class com.rscja.team.mtk.custom.M775Authenticate_mtk
setInventoryMessageMode() - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
setInventoryMessageMode() - Method in class com.rscja.team.qcom.custom.UHFCSYX_qcom
setInventoryMessageModeSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setInventoryModeEntity(InventoryModeEntity) - Method in class com.rscja.deviceapi.entity.TagInfoRule
  设置盘点模式
setInventoryModeEntity(InventoryModeEntity) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
setInventoryParameter(InventoryParameter) - Method in class com.rscja.deviceapi.entity.TagInfoRule
  设置盘点标签的参数信息
SetInventorySper(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SetInventorySper() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SetInventorySper(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
SetInventorySper() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
setInventoryTemperatureTagCallback(UHFTemperatureTag.InventoryTemperatureTagCallback) - Method in class com.rscja.custom.UHFTemperatureTag
setInventoryTemperatureTagCallback(UHFUartTemperatureTag.InventoryTemperatureTagCallback) - Method in class com.rscja.custom.UHFUartTemperatureTag
setIOControlSendData(byte, byte, byte) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
setIOControlSendData(byte, byte, byte) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
setIp(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setIP(String) - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  设置端口
setIPAndPort(String, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4NetWork
setIPAndPort(String, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8NetWork
setIPAndPort(String, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUrxNetwork
setIPAndPort(String, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置要连接的IP和端口 (Set the IP address and port to be connected)
setIPAndPort(String, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置要连接的IP和端口 (Set the IP address and port to be connected)
setIPAndPort(String, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  设置要连接的UR4 IP和端口
setIPAndPort(String, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
  设置要连接的UR4 IP和端口
setIpv6Dns1(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setIpv6Dns2(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setIpv6Ip1(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setIpv6Ip2(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setIpv6Ip3(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setIsAutoReceive(boolean) - Method in class com.rscja.team.qcom.usb.pl2302.UsbPL2302
setJumpFrequencySendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setJumpFrequencySendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.deviceapi.BleDevice
  设置扫描按键回调
  Setup SCAN button call back
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.deviceapi.BluetoothReader
setKeyEventCallback(KeyEventCallback) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setKeyEventCallback(KeyEventCallback) - Method in interface com.rscja.deviceapi.interfaces.IReader
  设置扫描按键回调
  Setup SCAN button call back
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.uhfhandler.UHFRxBLEDataHandle
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.uhfhandler.UHFRxUsbDataHandle
setkeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.uhfparse.UHFBLEProtocolParse
setKeyEventCallback(KeyEventCallback) - Method in class com.rscja.team.qcom.usb.RxUsb_qcom
setLBTMode(boolean) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setLBTMode(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setLinkFrequency(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  Link Frequency 设置(Link Frequency setting)
setLog(boolean) - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
setManuFacture(String) - Method in class com.rscja.deviceapi.Fingerprint
  设置厂商名称
  Setup manufacture name
setManuFacture(String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  设置厂商名称
  Setup manufacture name
setManuFacture(String) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  设置厂商名称
  Setup manufacture name
setMaxQ(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
setMaxValue(int) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置最小值，仅对值文件类型有效
  setup minimum value, it is valid for value file type only
setMessageHex(String) - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
setMessages(String) - Method in class com.rscja.team.qcom.http.NetResult_qcom
setMinQ(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
setMinValue(int) - Method in class com.rscja.deviceapi.entity.DESFireFile
  设置最小值，仅对值文件类型有效
  setup minimum value, it is valid for value file type only
setMode(int) - Method in class com.rscja.deviceapi.entity.InventoryModeEntity.Builder
setMorphoLoadKs(byte[]) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置加密数据秘钥
  Setup encypted data key
setMorphoLoadKs(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  设置加密数据秘钥
  Setup encypted data key
setMorphoLoadKs(byte[]) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  设置加密数据秘钥
  Setup encypted data key
setMorphoLoadKs(byte[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  设置加密数据秘钥
  Setup encypted data key
setMorphoSecurityLevel(int) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
setMorphoSecurityLevel(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
setMorphoSecurityLevel(int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
setMorphoSecurityLevel(int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
setName(String) - Method in class com.rscja.deviceapi.BleDevice.BleDeviceInfo
setNationalID(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的NationalID信息
  setup NationalID infor of animal tag
setNeedFrequencyPoint(boolean) - Method in class com.rscja.deviceapi.entity.InventoryParameter.ResultData
setNeedPhase(boolean) - Method in class com.rscja.deviceapi.entity.InventoryParameter.ResultData
setNetworkType(int) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setOnDataChangeListener(BluetoothReader.OnDataChangeListener) - Method in class com.rscja.deviceapi.BluetoothReader
  设置接收蓝牙原始数据的回调函数
  setup call back function for receiving BT initial data.
setOnDataChangeListener(BluetoothReader.OnDataChangeListener) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
setOnDataChangeListener(BluetoothReader.OnDataChangeListener) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setOnDataChangeListener(BluetoothReader.OnDataChangeListener) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
  设置接收蓝牙原始数据的回调函数
  setup call back function for receiving BT initial data.
setOnLowBatteryListener(Context, LowBatteryEntity, OnLowBatteryListener) - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
setOnLowBatteryListener(Context, LowBatteryEntity, OnLowBatteryListener) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setOnLowBatteryListener(Context, LowBatteryEntity, OnLowBatteryListener) - Method in class com.rscja.deviceapi.UhfBase
setOnLowBatteryListener(Context, LowBatteryEntity, OnLowBatteryListener) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setOnUhfWorkStateListener(Context, OnUhfWorkStateListener) - Method in interface com.rscja.scanner.IScanner
setOnUhfWorkStateListener(Context, OnUhfWorkStateListener) - Method in class com.rscja.scanner.utility.ScannerUtility
  设置UHF工作状态发送改变的回调接口 Register a callback to be invoked when this UHF working state changes.
setOnUhfWorkStateListener(Context, OnUhfWorkStateListener) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
  设置UHF工作状态发送改变的回调接口 Register a callback to be invoked when this UHF working state changes.
setOnUhfWorkStateListener(Context, OnUhfWorkStateListener) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
  设置UHF工作状态发送改变的回调接口 Register a callback to be invoked when this UHF working state changes.
setOriginalUID(char[]) - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  设置标签原始的UID
  setup original UID of tag
setOTGState(boolean) - Method in class com.rscja.team.mtk.system.SystemPropValues_mtk
setOTGState(boolean) - Method in class com.rscja.team.qcom.system.SystemPropValues_qcom
setOutputMode(Context, int) - Method in class com.rscja.barcode.BarcodeUtility
  设置输出模式 Setup ouput mode
setOutputMode(int) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setOutputMode(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置输出模式 Setup ouput mode
setOutputMode(Context, int) - Method in interface com.rscja.scanner.IScanner
  输出模式
  Output mode
setOutputMode(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setOutputMode(Context, int) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置输出模式 Setup ouput mode
setOutputMode(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setOutputMode(Context, int) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置输出模式 Setup ouput mode
setOutputMode(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setParam(int, int, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  根据指定的参数类型，设置设备参数
setParam(int, int, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  根据指定的参数类型，设置设备参数
setParam(int, int, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  根据指定的参数类型，设置设备参数
setParam_zebra(Context, int, int) - Method in class com.rscja.barcode.BarcodeUtility
  设置斑马扫描头参数,扫描头上电之后设置一次即可,扫描头断电之后失效。(备注：键盘助手v2.2.0.3 之后的版本才支持)
setParam_zebra(Context, int, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置斑马扫描头参数,扫描头上电之后设置一次即可,扫描头断电之后失效。(备注：键盘助手v2.2.0.3 之后的版本才支持)
setParam_zebra(Context, int, int) - Method in interface com.rscja.scanner.IScanner
  设置斑马扫描头参数,扫描头上电之后设置一次即可,扫描头断电之后失效。(备注：键盘助手v2.2.0.3 之后的版本才支持)
  Setup zebra scanner parameters, after scanner has powered on to setup for once,
setParam_zebra(Context, int, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setParam_zebra(Context, int, int) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置斑马扫描头参数,扫描头上电之后设置一次即可,扫描头断电之后失效。(备注：键盘助手v2.2.0.3 之后的版本才支持)
setParam_zebra(Context, int, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setParam_zebra(Context, int, int) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置斑马扫描头参数,扫描头上电之后设置一次即可,扫描头断电之后失效。(备注：键盘助手v2.2.0.3 之后的版本才支持)
setParam_zebra(Context, int, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setParameter(int, int) - Method in class com.rscja.barcode.BarcodeDecoder
  设置扫描头参数(Setup scanning module parameter)
setParameter(byte[], byte[]) - Method in class com.rscja.deviceapi.BluetoothReader
setParameter(byte[], byte[]) - Method in interface com.rscja.deviceapi.interfaces.IReader
setParameter(byte[], byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setParameter(int, int) - Method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
  设置扫描头参数
  Setup scanning module parameter
setParameter(int, int) - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  设置扫描头参数(Setup scanning module parameter)
setParameter(int, int) - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
  设置扫描头参数
  Setup scanning module parameter
setParameter(byte[], byte[]) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setParameter(byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setParameter(byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setParameters() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
setParameters(int, int, int, int) - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Sets various serial port parameters.
setParameters() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
setParameters(int, int, int, int) - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
setParameterSendData(byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setParse(boolean) - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
setParse(boolean) - Method in class com.rscja.team.qcom.socket.SocketManageA4
setPassword(String) - Method in class com.rscja.deviceapi.entity.WifiConfig
setPc(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setPhase(int) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setPort(int) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setPort(int) - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  设置端口
setPortSendData(int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setPower(int) - Method in class com.rscja.deviceapi.BleDevice
  设置模块的功率
  Setup output power
setPower(int) - Method in class com.rscja.deviceapi.entity.AntennaPowerEntity
setPower(int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setPower(int) - Method in interface com.rscja.deviceapi.interfaces.ISingleAntenna
  设置模块的功率
  Setup output power
setPower(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setPower(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setPower(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setPower(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setPower(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setPower(int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setPower(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setPower(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setPower(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setPower(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setPowerOnBySystem(Context) - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
  设置uhf由系统内部上电,不使用DeviceAPI的代码上电!
setPowerOnBySystem(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  设置uhf由系统内部上电,不使用DeviceAPI的代码上电!
setPowerOnBySystem(Context) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  设置uhf由系统内部上电,不使用DeviceAPI的代码上电!
setPowerOnBySystem(Context) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
  设置uhf由系统内部上电,不使用DeviceAPI的代码上电!
setPowerOnDynamicSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setPowerOnDynamicSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setPowerSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取设置功率的发送数据
setPowerSendData(int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setPowerSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setPowerSendData(int, int) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setPrefix(Context, String) - Method in class com.rscja.barcode.BarcodeUtility
  设置前缀 Setup prefix
setPrefix(byte[]) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setPrefix(String) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setPrefix(Context, String) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置前缀 Setup prefix
setPrefix(Context, String) - Method in interface com.rscja.scanner.IScanner
  设置前缀
  Setup prefix
setPrefix(Context, String) - Method in class com.rscja.scanner.utility.ScannerUtility
setPrefix(Context, String) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置前缀 Setup prefix
setPrefix(Context, String) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setPrefix(Context, String) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置前缀 Setup prefix
setPrefix(Context, String) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setPressure(int) - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
setPreviewDisplay(Surface) - Method in interface com.rscja.deviceapi.interfaces.IBarcodePhoto
setPrintCharacterStyle(boolean, boolean, boolean, boolean, boolean, boolean, boolean) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置字体样式
  set font style
setPrintCharacterStyle(boolean, boolean, boolean, boolean, boolean, boolean, boolean) - Method in class com.rscja.deviceapi.Printer
  设置字体样式
  set font style
setPrintCharacterStyle(boolean, boolean, boolean, boolean, boolean, boolean, boolean) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置字体样式
  set font style
setPrintCodePage(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
setPrintCodePage(int) - Method in class com.rscja.deviceapi.Printer
setPrintCodePage(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
setPrinterStatusCallBack(Printer.PrinterStatusCallBack) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置接收打印机状态的回调
  set call back of printer received status
setPrinterStatusCallBack(Printer.PrinterStatusCallBack) - Method in class com.rscja.deviceapi.Printer
  设置接收打印机状态的回调
  set call back of printer received status
setPrinterStatusCallBack(Printer.PrinterStatusCallBack) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置接收打印机状态的回调
  set call back of printer received status
setPrinterStatusCallBackEnable(boolean) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置是否接收打印机状态回调消息
  Setup receive printer status return message or not
setPrinterStatusCallBackEnable(boolean) - Method in class com.rscja.deviceapi.Printer
  设置是否接收打印机状态回调消息
  Setup receive printer status return message or not
setPrinterStatusCallBackEnable(boolean) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置是否接收打印机状态回调消息
  Setup receive printer status return message or not
setPrinterType(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
setPrinterType(int) - Method in class com.rscja.deviceapi.Printer
setPrinterType(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
setPrintGrayLevel(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置打印 灰度
  setup print grey level
setPrintGrayLevel(int) - Method in class com.rscja.deviceapi.Printer
  设置打印 灰度
  setup print grey level
setPrintGrayLevel(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置打印 灰度
  setup print grey level
setPrintLeftMargin(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置左边距
  Setup left margin
setPrintLeftMargin(int) - Method in class com.rscja.deviceapi.Printer
  设置左边距
  Setup left margin
setPrintLeftMargin(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置左边距
  * Setup left margin
setPrintRightMargin(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置左边距
  Setup right margin
setPrintRightMargin(int) - Method in class com.rscja.deviceapi.Printer
  设置左边距
  Setup right margin
setPrintRightMargin(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置左边距
  * Setup right margin
setPrintRowSpacing(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置行间距(若设定的行间距小于一行中的最大字符高度，那么该行行间距等于最大字符高度)
  Setup line spacing (if the set value is less than max.charater height, then the line spacing equals to max.character height)
setPrintRowSpacing(int) - Method in class com.rscja.deviceapi.Printer
  设置行间距(若设定的行间距小于一行中的最大字符高度，那么该行行间距等于最大字符高度)
  Setup line spacing (if the set value is less than max.charater height, then the line spacing equals to max.character height)
setPrintRowSpacing(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置行间距(若设定的行间距小于一行中的最大字符高度，那么该行行间距等于最大字符高度)
  Setup line spacing (if the set value is less than max.charater height, then the line spacing equals to max.character height)
setPrintSpeed(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  设置打印速度
  setup print velocity
setPrintSpeed(int) - Method in class com.rscja.deviceapi.Printer
  设置打印速度
  setup print velocity
setPrintSpeed(int) - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  设置打印速度
  setup print velocity
setProtocol(int) - Method in class com.rscja.deviceapi.BleDevice
  设置协议
  Setup protocol
setProtocol(int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setProtocol(int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置协议
  Setup protocol
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置协议(Set protocol)
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置协议(Set protocol)
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置协议(Set protocol)
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置协议(Set protocol)
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置协议
  Setup protocol
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setProtocol(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setProtocol(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setProtocol(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置协议
  Setup protocol
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setProtocol(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setProtocolSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取设置协议的发送数据
setProtocolSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setProxy(int) - Method in class com.rscja.deviceapi.entity.WifiConfig
setPtCaptureCallBack(FingerprintWithFIPS.PtCaptureCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithFIPS.PtCaptureCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithFIPS.PtCaptureCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithFIPS.PtCaptureCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  设置获取指纹模版回调接口
  Setup call-back contact for acquiring fingerprint template
setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置采集指纹回调接口
  setup fingerprint acquire call-back contact
setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  设置采集指纹回调接口
  setup fingerprint acquire call-back contact
setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  设置采集指纹回调接口
  setup fingerprint acquire call-back contact
setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  设置采集指纹回调接口
  setup fingerprint acquire call-back contact
setPWD(String) - Method in class com.rscja.deviceapi.Fingerprint
  设置密码
  Setup password
setPWD(String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  设置密码
  Setup password
setPWD(String) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  设置密码
  Setup password
setQ(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置Q值(Q value)
SetQTPara(char) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SetQTPara(char) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
setQueryDR(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置query命令的DR参数(DR parameter of the query command)
setQueryM(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置query命令的M参数(M parameter of the query command )
setQuerySel(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置query命令的sel参数(sel parameter of the query command)
setQuerySession(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置query命令的session参数(session parameter of the query command)
setQueryTarget(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置 query命令的Target参数(Target parameter of the query command)
setQueryTRext(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置query命令的TRext参数(TRext parameter of the query command )
setR6WorkmodeSendData(char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setR6WorkmodeSendData(char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setRawData(String) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置原始数据
  setup original data
setReaderAwaitSleepTime(int) - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  设置读写器等待休眠的时间。在读写器断开连接的状态下，即将进入休眠的时间。
setReaderAwaitSleepTime(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setReaderAwaitSleepTime(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setReaderAwaitSleepTime(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setReaderAwaitSleepTime(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setReaderAwaitSleepTime(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setReaderAwaitSleepTimeSendData(char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setReaderAwaitSleepTimeSendData(char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setReaderDestIpSendData(ReaderIPEntity) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
setReaderDestIpSendData(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
setReaderIpSendData(ReaderIPEntity) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
setReaderIpSendData(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
setReg(int, int) - Method in class com.rscja.deviceapi.Fingerprint
  设置寄存器值，修改模块参数
  Setup the value in RAM, modify the parameter in module.
setReg(int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  设置寄存器值，修改模块参数
  Setup the value in RAM, modify the parameter in module.
setReg(int, int) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  设置寄存器值，修改模块参数
  Setup the value in RAM, modify the parameter in module.
setRelayStatus(byte) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  设置继电器状态
setRelayStatus(byte) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setRelayStatus(byte) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置继电器状态
setRelayStatus(byte) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setRelayStatus(byte) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setRelayStatus(byte) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setRelayStatus(byte) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置继电器状态
setRelayStatus(byte) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setReleaseScan(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  松开扫描按键是否停止扫描 loose scanning button to stop scanning or not
setReleaseScan(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  松开扫描按键是否停止扫描 loose scanning button to stop scanning or not
setReleaseScan(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  松开扫描按键是否停止扫描
  Stop scan after release scan button
setReleaseScan(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
setReleaseScan(Context, boolean) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  松开扫描按键是否停止扫描 loose scanning button to stop scanning or not
setReleaseScan(Context, boolean) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setReleaseScan(Context, boolean) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  松开扫描按键是否停止扫描 loose scanning button to stop scanning or not
setReleaseScan(Context, boolean) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setReleaseScanKeyOnStartScan(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setReleaseScanKeyOnStopScan(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setRemain(int) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setRemoteBluetoothName(String) - Method in class com.rscja.deviceapi.BleDevice
  修改蓝牙名称(Change Bluetooth device Name)
setRemoteBluetoothName(String) - Method in class com.rscja.deviceapi.BluetoothReader
setRemoteBluetoothName(String) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setRemoteBluetoothName(String) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  修改蓝牙名称(Change Bluetooth device Name)
setRemoteBluetoothName(String) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setRemoteBluetoothName(String) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setRemoteBluetoothName(String) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
setReserved(long) - Method in class com.rscja.deviceapi.entity.AnimalEntity
  设置动物标签的Reserved信息
  setup Reserved infor of animal tag
setReserved(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setReservedLength(int) - Method in class com.rscja.deviceapi.entity.InventoryModeEntity.Builder
setReservedOffset(int) - Method in class com.rscja.deviceapi.entity.InventoryModeEntity.Builder
setResponseHex(String) - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
setResultCode(int) - Method in class com.rscja.deviceapi.entity.BarcodeEntity
setResultData(InventoryParameter.ResultData) - Method in class com.rscja.deviceapi.entity.InventoryParameter
setRFIDEncodingFormat(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置RFID编码格式
  Setup RFID decoding format
setRFIDEncodingFormat(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setRFIDEncodingFormat(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setRFIDEncodingFormat(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setRFLink(int) - Method in class com.rscja.deviceapi.BleDevice
  设置链路参数
  Setup RFlink
setRFLink(int) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setRFLink(int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  设置链路参数
  Setup RFlink
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置链路参数(Set link parameters)
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置链路参数(Set link parameters)
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置链路参数(Set link parameters)
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置链路参数(Set link parameters)
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置链路参数
  Setup RFlink
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setRFLink(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setRFLink(int) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setRFLink(int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置链路参数
  Setup RFlink
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setRFLink(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setRFLinkSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setRFLinkSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setRssi(String) - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
setRssi(String) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setRssi(String) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setRssi(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setRssiCode(String) - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
setRssiCode(String) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setRssiCode(String) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setRTS(boolean) - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Sets the RTS (Request To Send) bit on the underlying UART, if supported.
setRTS(boolean) - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
setScanFailureBroadcast(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  扫描失败是否发送广播 Send broadcast when scanning failure.
setScanFailureBroadcast(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setScanFailureBroadcast(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  扫描失败是否发送广播 Send broadcast when scanning failure.
setScanFailureBroadcast(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  扫描失败是否发送广播,接收广播的action和扫描成功的action是同一个
  Send broadcast when scan failure
setScanFailureBroadcast(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
setScanFailureBroadcast(Context, boolean) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  扫描失败是否发送广播 Send broadcast when scanning failure.
setScanFailureBroadcast(Context, boolean) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setScanFailureBroadcast(Context, boolean) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  扫描失败是否发送广播 Send broadcast when scanning failure.
setScanFailureBroadcast(Context, boolean) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setScanKey(Context, int, int[]) - Method in interface com.rscja.scanner.IScanner
  设置扫描或者读卡的按键值
  Setup keycode for barcode scan or card reading
setScanKey(Context, int, int[]) - Method in class com.rscja.scanner.utility.ScannerUtility
setScanKey(Context, int, int[]) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setScanKey(Context, int, int[]) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setScanner70() - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setScanner70() - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setScanOutTime(Context, int) - Method in class com.rscja.barcode.BarcodeUtility
  设置超时时间 Setup overtime duration
setScanOutTime(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置超时时间 Setup overtime duration
setScanOutTime(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置扫码超时时间
  Setup scan time-out duration
setScanOutTime(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setScanOutTime(Context, int) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置超时时间 Setup overtime duration
setScanOutTime(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setScanOutTime(Context, int) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置超时时间 Setup overtime duration
setScanOutTime(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setScanResultBroadcast(Context, String, String) - Method in class com.rscja.barcode.BarcodeUtility
  设置接收扫描数据的广播 Setup broad cast of received scanning data
setScanResultBroadcast(Context, String, String) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置接收扫描数据的广播 Setup broad cast of received scanning data
setScanResultBroadcast(Context, String, String) - Method in interface com.rscja.scanner.IScanner
  设置条码扫描结果接收的广播
  Setup barcode scanning result
setScanResultBroadcast(Context, String, String) - Method in class com.rscja.scanner.utility.ScannerUtility
setScanResultBroadcast(Context, String, String) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置接收扫描数据的广播 Setup broad cast of received scanning data
setScanResultBroadcast(Context, String, String) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setScanResultBroadcast(Context, String, String) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置接收扫描数据的广播 Setup broad cast of received scanning data
setScanResultBroadcast(Context, String, String) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setScanResultBroadcastAction(String) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setScanResultBroadcastKey(String) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setScanResultBroadcastRFID(Context, String, String) - Method in interface com.rscja.scanner.IScanner
  设置RFID扫描结果接收广播
  Setup RFID scanning result receive broadcast
setScanResultBroadcastRFID(Context, String, String) - Method in class com.rscja.scanner.utility.ScannerUtility
setScanResultBroadcastRFID(Context, String, String) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setScanResultBroadcastRFID(Context, String, String) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setSecurityType(int) - Method in class com.rscja.deviceapi.entity.WifiConfig
setSelectAction(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置select 命令的Action参数 (Action parameter of the select command)
setSelectTarget(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置select命令的Target参数 (Target parameter of the select command)
setSelectTruncate(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
  设置select命令的Truncate参数(Truncate parameter of the select command)
setSensorCode(String) - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
setSensorCode(String) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setSensorCode(String) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setShortenedTidHex(String) - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
setSignalValue(int) - Method in class com.rscja.deviceapi.entity.TagLocationInfo
setSsid(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setSsid(String) - Method in class com.rscja.deviceapi.entity.WifiConfig
setStartQ(int) - Method in class com.rscja.deviceapi.entity.Gen2Entity
setStaticIp(boolean) - Method in class com.rscja.deviceapi.entity.WifiConfig
setStaticIpConfig(ReaderIPEntity) - Method in class com.rscja.deviceapi.entity.WifiConfig
setStatusCallback(ConnectionStatusCallback) - Method in class com.rscja.team.qcom.service.BLEService_qcom
setSubnetMask(String) - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
setSucces(boolean) - Method in class com.rscja.team.qcom.http.NetResult_qcom
setSuccessSound(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setSuffix(Context, String) - Method in class com.rscja.barcode.BarcodeUtility
  设置后缀 Setup suffix
setSuffix(String) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setSuffix(Context, String) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  设置后缀 Setup suffix
setSuffix(Context, String) - Method in interface com.rscja.scanner.IScanner
  设置后缀
  Setup suffix
setSuffix(Context, String) - Method in class com.rscja.scanner.utility.ScannerUtility
setSuffix(Context, String) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  设置后缀 Setup suffix
setSuffix(Context, String) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setSuffix(Context, String) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  设置后缀 Setup suffix
setSuffix(Context, String) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setSupportRssi(boolean) - Method in class com.rscja.deviceapi.BleDevice
setSupportRssi(boolean) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setSupportRssi(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setSupportRssi(boolean) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setSupportRssi(boolean) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setSupportRssi(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setSupportRssi(boolean) - Method in class com.rscja.team.qcom.uhfparse.UHFBLEProtocolParse
setSystemTime(long) - Method in interface com.rscja.system.ISystemInterfaces
  设置系统时间
setSystemTime(long) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
setTab(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setTag(String) - Method in class com.rscja.deviceapi.entity.RadarLocationEntity.Builder
setTagFocus(boolean) - Method in class com.rscja.deviceapi.BleDevice
  开关TagFocus功能
  ON/OFF TagFocus
setTagFocus(boolean) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
setTagFocus(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  开关TagFocus功能
  ON/OFF TagFocus
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  开关TagFocus功能(Switch TagFocus function)
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  开关TagFocus功能(Switch TagFocus function)
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  开关TagFocus功能(Switch TagFocus function)
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  开关TagFocus功能(Switch TagFocus function)
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  开关TagFocus功能
  ON/OFF TagFocus
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setTagFocus(boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
setTagFocus(boolean) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
setTagFocus(boolean) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  开关TagFocus功能
  ON/OFF TagFocus
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setTagFocus(boolean) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
setTagfocusSendData(char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
setTagfocusSendData(char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setTagLocationInfo(TagLocationInfo) - Method in class com.rscja.deviceapi.entity.TagLocationEntity
setTamper(String) - Method in class com.rscja.custom.UHFTamperAPI.TamperInfo
setTcpServicePort(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setTcpServicePort(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置UHF TCP服务端口
setTcpServicePort(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置UHF TCP服务端口
setTcpServicePort(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置UHF TCP服务端口
setTcpServicePort(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置UHF TCP服务端口
setTempCount(int) - Method in class com.rscja.custom.UHFTemperatureTagsAPI.TempertureInfo
setTempeCode(String) - Method in class com.rscja.custom.RFIDWithUHFJieCe.TemperatureTagInfo
setTempeCode(String) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setTempeCode(String) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setTemperature(float) - Method in class com.rscja.custom.UHFTemperatureTag.TemperatureTagInfo
setTemperature(float) - Method in class com.rscja.custom.UHFTemperatureTagsAPI.TempertureInfo
setTemperature(float) - Method in class com.rscja.custom.UHFUartTemperatureTag.TemperatureTagInfo
setTemperatureByContactResistance(float) - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
setTemperture(float[]) - Method in class com.rscja.custom.UHFTemperatureTagsAPI.MultipleTemperatureInfo
setTemplateVerifyCallBack(FingerprintWithFIPS.TemplateVerifyCallBack) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithMorpho.TemplateVerifyCallBack) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithFIPS.TemplateVerifyCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithMorpho.TemplateVerifyCallBack) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithFIPS.TemplateVerifyCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithMorpho.TemplateVerifyCallBack) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithFIPS.TemplateVerifyCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTemplateVerifyCallBack(FingerprintWithMorpho.TemplateVerifyCallBack) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  设置模版比对回调接口
  Setup call-back contact for template comparison
setTempValid(boolean) - Method in class com.rscja.custom.UHFTemperatureTagsAPI.TempertureInfo
SetTestMode() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SetTestMode() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
setTid(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setTidBytes(byte[]) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setTimeOut(int) - Method in class com.rscja.barcode.BarcodeDecoder
  设置超时时间
  setup time-out duration
setTimeOut(int) - Method in class com.rscja.deviceapi.Barcode1D
  设置超时时间
  set time out.
setTimeOut(int) - Method in class com.rscja.deviceapi.Barcode2D
  设置超时时间
  set time out.
setTimeOut(int) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  设置指纹模块超时时间
setTimeOut(int) - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  设置超时时间
  set time out.
setTimeOut(int) - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  设置超时时间
  set time out.
setTimeOut(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  设置指纹模块超时时间
setTimeOut(int) - Method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
setTimeOut(int) - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  设置超时时间
  setup time-out duration
setTimeOut(int) - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  设置超时时间
  set time out.
setTimeOut(int) - Method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  设置超时时间
  set time out.
setTimeOut(int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  设置指纹模块超时时间
setTimeOut(int) - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
setTimeOut(int) - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  设置超时时间
  set time out.
setTimeOut(int) - Method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  设置超时时间
  set time out.
setTimeOut(int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  设置指纹模块超时时间
setTimestamp(long) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setTotal(int) - Method in class com.rscja.custom.UHFTemperatureTagsAPI.MultipleTemperatureInfo
setTriggerWorkModePara(int, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  设置触发工作模式参数
setTriggerWorkModePara(int, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setTriggerWorkModePara(int, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置触发工作模式参数
setTriggerWorkModePara(int, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setTriggerWorkModePara(int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setTriggerWorkModePara(int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setTriggerWorkModePara(int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置触发工作模式参数
setTriggerWorkModePara(int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setTriggerWorkModeParaSendData(int, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
setTriggerWorkModeParaSendData(int, int, int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
setType(HF15693RequestEntity.TagType) - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity.Builder
setUart(String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4RS232
setUart(String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8RS232
setUart(String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUrxUart
setUart(String) - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
  设置uhf串口，使用此函数需要谨慎，否则uhf会无法工作。
setUart(String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
setUart(String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
setUart(String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  设置uhf串口，使用此函数需要谨慎，否则uhf会无法工作。
setUart(String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置uhf串口，使用此函数需要谨慎，否则uhf会无法工作。
setUart(String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  设置uhf串口，使用此函数需要谨慎，否则uhf会无法工作。
setUart(String) - Method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  设置串口路径
  Setup serial port directory.
setUart(String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
  设置uhf串口，使用此函数需要谨慎，否则uhf会无法工作。
setUart(String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setUart(String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置uhf串口，使用此函数需要谨慎，否则uhf会无法工作。
setUart(String) - Method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  设置串口路径
  Setup serial port directory.
setUart(String, int) - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
setUhfBank(int) - Method in class com.rscja.deviceapi.entity.RadarLocationEntity.Builder
setUHFMode(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置uhf模式 (备注：键盘助手v2.3.5 之后的版本才支持)
  Setup UHF mode (Comment: Supports after keyboardemualator v2.3.5 has been released)
setUHFMode(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setUHFMode(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setUHFMode(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setUHFPower(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置uhf功率
  Setup UHF output power
setUHFPower(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
setUHFPower(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
setUHFPower(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
setUhfReaderIP(ReaderIPEntity) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  设置UHF读写器IP
setUhfReaderIP(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setUhfReaderIP(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置UHF读写器IP
setUhfReaderIP(ReaderIPEntity) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setUhfReaderIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setUhfReaderIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setUhfReaderIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置UHF读写器IP
setUhfReaderIP(ReaderIPEntity) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setUhftagInfo(UHFTAGInfo) - Method in class com.rscja.custom.M775Authenticate.AuthenticateInfo
setUhftagInfo(UHFTAGInfo) - Method in class com.rscja.custom.UHFCSYX.TagAuthenticationResponseInfo
setUhftagInfo(List<UHFTAGInfo>) - Method in class com.rscja.custom.UHFSFForUrxNetwork.AntInfo
setUhftagInfo(UHFTAGInfo) - Method in class com.rscja.custom.UHFTamperAPI.TamperInfo
setUhftagInfo(UHFTAGInfo) - Method in class com.rscja.custom.UHFTemperatureSensors.TemperatureTag
setUhftagInfo(UHFTAGInfo) - Method in class com.rscja.custom.UHFTemperatureTagsAPI.TempertureInfo
setUhftagInfo(UHFTAGInfo) - Method in class com.rscja.deviceapi.entity.TagLocationEntity
setUid(byte[]) - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity.Builder
setUpgradeProgress(IUpgradeProgress) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setUpgradeProgress(IUpgradeProgress) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置监听升级进度
setUpgradeProgress(IUpgradeProgress) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置监听升级进度
setUpgradeProgress(IUpgradeProgress) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置监听升级进度
setUpgradeProgress(IUpgradeProgress) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置监听升级进度
setUpgradeTcpServiceData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setUpgradeTcpServiceData(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  升级UHF Tcp服务器程序第二步,设置要升级的APK数据
setUpgradeTcpServiceData(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  升级UHF Tcp服务器程序第二步,设置要升级的APK数据
setUpgradeTcpServiceData(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  升级UHF Tcp服务器程序第二步,设置要升级的APK数据
setUpgradeTcpServiceData(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  升级UHF Tcp服务器程序第二步,设置要升级的APK数据
setUser(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setUserBytes(byte[]) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
setUserLength(int) - Method in class com.rscja.deviceapi.entity.InventoryModeEntity.Builder
setUserOffset(int) - Method in class com.rscja.deviceapi.entity.InventoryModeEntity.Builder
setUserSettingSendData(byte, byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
setValid(boolean) - Method in class com.rscja.deviceapi.entity.TagLocationInfo
setValue(int) - Method in class com.rscja.deviceapi.entity.RadarLocationEntity.Builder
setValue(int) - Method in class com.rscja.deviceapi.entity.RadarLocationEntity
  设置标签的信号值 (Set the signal value of the label)
setVersions(String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
setVibrate(boolean) - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
setVirtualScanButton(Context, int) - Method in interface com.rscja.scanner.IScanner
  设置虚拟扫描按钮
setVirtualScanButton(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
  设置虚拟扫描按钮
setVirtualScanButton(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
  设置虚拟扫描按钮
setVirtualScanButton(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
  设置虚拟扫描按钮
setVoltage(int) - Method in class com.rscja.deviceapi.entity.BatteryEntity
setWifiConfigInfo(WifiConfig) - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
setWifiConfigInfo(WifiConfig) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  设置wifi配置信息
setWifiConfigInfo(WifiConfig) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  设置wifi配置信息
setWifiConfigInfo(WifiConfig) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  设置wifi配置信息
setWifiConfigInfo(WifiConfig) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  设置wifi配置信息
setWifiConfigInfoSendData(WifiConfig) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
setWorkMode(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  设置工作模式
setWorkMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
setWorkMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  设置工作模式
setWorkMode(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
setWorkMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
setWorkMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
setWorkMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  设置工作模式
setWorkMode(int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
setWorkModeSendData(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
setWorkModeSendData(int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseUrxByJava_qcom
setWriteLog(boolean) - Static method in class com.rscja.team.mtk.utility.LogUtility_mtk
setWriteLog(boolean, String, String) - Static method in class com.rscja.team.mtk.utility.LogUtility_mtk
setWriteLog(boolean) - Static method in class com.rscja.team.qcom.utility.LogUtility_qcom
setWriteLog(boolean, String, String) - Static method in class com.rscja.team.qcom.utility.LogUtility_qcom
silentInstall(String) - Method in interface com.rscja.system.ISystemInterfaces
  静默安装apk
silentInstall(String) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
silentUninstall(String) - Method in interface com.rscja.system.ISystemInterfaces
  静默卸载apk
silentUninstall(String) - Method in class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
SimpleRFIDEntity - Class in com.rscja.deviceapi.entity
  RFID简单数据实体
  RFID simple data entity
SimpleRFIDEntity(String, String) - Constructor for class com.rscja.deviceapi.entity.SimpleRFIDEntity
  构造函数
  create formula
SimpleRFIDEntity(String, String, byte[]) - Constructor for class com.rscja.deviceapi.entity.SimpleRFIDEntity
  构造函数
  create formula
sledCtrl(boolean) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  控制采集器背光灯的开/关
sledCtrl(boolean) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  控制采集器背光灯的开/关
sledCtrl(boolean) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  控制采集器背光灯的开/关
SocketManageA4 - Class in com.rscja.team.qcom.socket
SocketManageA4() - Constructor for class com.rscja.team.qcom.socket.SocketManageA4
SocketManageUR4 - Class in com.rscja.team.qcom.socket
SocketManageUR4() - Constructor for class com.rscja.team.qcom.socket.SocketManageUR4
SocketManageUR4.CheckConnectState - Interface in com.rscja.team.qcom.socket
SocketTcpIpBase - Class in com.rscja.team.qcom.socket
SocketTcpIpBase() - Constructor for class com.rscja.team.qcom.socket.SocketTcpIpBase
SocketUdpClient - Class in com.rscja.team.qcom.socket
SocketUdpClient() - Constructor for class com.rscja.team.qcom.socket.SocketUdpClient
SocketUdpClientUR4 - Class in com.rscja.team.qcom.socket
SocketUdpClientUR4() - Constructor for class com.rscja.team.qcom.socket.SocketUdpClientUR4
spClose() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  关闭串口
spClose() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  关闭串口
SpiFree(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SpiFree(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
SpiInit(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SpiInit(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
SpiRead(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SpiRead(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
SpiWrite(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
SpiWrite(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
spOpen(String, int, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
  打开串口
spOpen(String, int, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
  打开串口
start(IUHFInventoryCallback) - Method in interface com.rscja.deviceapi.interfaces.IUHFUrxAutoInventoryTag
start(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.deviceapi.UHFUrxNetWorkAutoInventoryTag_qcom
startBTScan(ScanBTCallback) - Method in class com.rscja.team.qcom.service.BLEService_qcom
startEnroll() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始采集指纹,注意:请调用
  start acquire fingerprint, attention: call out
  `FingerprintWithFIPS.setEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setEnrollCallBack(EnrollCallBack callBack)`setup receviced call-back data
startEnroll(int, String) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `FingerprintWithMorpho.setPtEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setPtEnrollCallBack(EnrollCallBack callBack)` setup receive call-back data
startEnroll(int, String, String, String) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `FingerprintWithMorpho.setPtEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setPtEnrollCallBack(EnrollCallBack callBack)` setup receive call-back data
startEnroll() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  开始采集指纹,注意:请调用
  start acquire fingerprint, attention: call out
  `IFingerprintWithFIPS.setEnrollCallBack(FingerprintWithFIPS.EnrollCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithFIPS.setEnrollCallBack(FingerprintWithFIPS.EnrollCallBack callBack)`setup receviced call-back data
startEnroll(int, String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `IFingerprintWithMorpho.setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithMorpho.setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack callBack)` setup receive call-back data
startEnroll(int, String, String, String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `IFingerprintWithMorpho.setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithMorpho.setPtEnrollCallBack(FingerprintWithMorpho.EnrollCallBack callBack)` setup receive call-back data
startEnroll() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  开始采集指纹,注意:请调用
  start acquire fingerprint, attention: call out
  `#setEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `#setEnrollCallBack(EnrollCallBack callBack)`setup receviced call-back data
startEnroll(int, String) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `#setPtEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `#setPtEnrollCallBack(EnrollCallBack callBack)` setup receive call-back data
startEnroll(int, String, String, String) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `#setPtEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `#setPtEnrollCallBack(EnrollCallBack callBack)` setup receive call-back data
startEnroll() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  开始采集指纹,注意:请调用
  start acquire fingerprint, attention: call out
  `#setEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `#setEnrollCallBack(EnrollCallBack callBack)`setup receviced call-back data
startEnroll(int, String) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `#setPtEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `#setPtEnrollCallBack(EnrollCallBack callBack)` setup receive call-back data
startEnroll(int, String, String, String) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  开始采集指纹,注意:请调用
  Start acquire fingerprint, attention: call out
  `#setPtEnrollCallBack(EnrollCallBack callBack)` 方法设置接收回调数据
  `#setPtEnrollCallBack(EnrollCallBack callBack)` setup receive call-back data
startGRAB() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始获取图片,注意:请调用
  start acquire picture, attention: call out
  `FingerprintWithFIPS.setGrabCallBack(GRABCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setGrabCallBack(GRABCallBack callBack)`method to setup received call-back data.
startGrab(String, String) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
startGRAB() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  开始获取图片,注意:请调用
  start acquire picture, attention: call out
  `IFingerprintWithFIPS.setGrabCallBack(FingerprintWithFIPS.GRABCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithFIPS.setGrabCallBack(FingerprintWithFIPS.GRABCallBack callBack)`method to setup received call-back data.
startGrab(String, String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
startGRAB() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  开始获取图片,注意:请调用
  start acquire picture, attention: call out
  `#setGrabCallBack(GRABCallBack callBack)` 方法设置接收回调数据
  `#setGrabCallBack(GRABCallBack callBack)`method to setup received call-back data.
startGrab(String, String) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
startGRAB() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  开始获取图片,注意:请调用
  start acquire picture, attention: call out
  `#setGrabCallBack(GRABCallBack callBack)` 方法设置接收回调数据
  `#setGrabCallBack(GRABCallBack callBack)`method to setup received call-back data.
startGrab(String, String) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
startIdentification() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始验证指纹,注意:请调用
  start verify finerprint, attention: call out
  `FingerprintWithFIPS.setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setIdentificationCallBack(IdentificationCallBack callBack)` setup receviced call-back data
startIdentification() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始验证指纹,注意:请调用
  Start verify fingerprint, attention: call-out
  `FingerprintWithMorpho.setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setIdentificationCallBack(IdentificationCallBack callBack)` setup receive call-back data
startIdentification() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  开始验证指纹,注意:请调用
  start verify finerprint, attention: call out
  `IFingerprintWithFIPS.setIdentificationCallBack(FingerprintWithFIPS.IdentificationCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithFIPS.setIdentificationCallBack(FingerprintWithFIPS.IdentificationCallBack callBack)` setup receviced call-back data
startIdentification() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  开始验证指纹,注意:请调用
  Start verify fingerprint, attention: call-out
  `IFingerprintWithMorpho.setIdentificationCallBack(FingerprintWithMorpho.IdentificationCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithMorpho.setIdentificationCallBack(FingerprintWithMorpho.IdentificationCallBack callBack)` setup receive call-back data
startIdentification() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  开始验证指纹,注意:请调用
  start verify finerprint, attention: call out
  `#setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `#setIdentificationCallBack(IdentificationCallBack callBack)` setup receviced call-back data
startIdentification() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  开始验证指纹,注意:请调用
  Start verify fingerprint, attention: call-out
  `#setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `#setIdentificationCallBack(IdentificationCallBack callBack)` setup receive call-back data
startIdentification() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  开始验证指纹,注意:请调用
  start verify finerprint, attention: call out
  `#setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `#setIdentificationCallBack(IdentificationCallBack callBack)` setup receviced call-back data
startIdentification() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  开始验证指纹,注意:请调用
  Start verify fingerprint, attention: call-out
  `#setIdentificationCallBack(IdentificationCallBack callBack)` 方法设置接收回调数据
  `#setIdentificationCallBack(IdentificationCallBack callBack)` setup receive call-back data
startInventoryTag() - Method in class com.rscja.custom.UHFCSYX_A4NetWork
startInventoryTag() - Method in class com.rscja.custom.UHFCSYXForURx
startInventoryTag() - Method in class com.rscja.custom.UHFTemperatureSensors
startInventoryTag() - Method in class com.rscja.custom.UHFTemperatureTag.RFIDWithUHFBLEN51
startInventoryTag() - Method in class com.rscja.custom.UHFTemperatureTag.RFIDWithUHFBLEN52
startInventoryTag() - Method in class com.rscja.deviceapi.BleDevice
  启动识别Tag循环
  Enable Tag auto reading
startInventoryTag() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
startInventoryTag(int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
startInventoryTag() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  开始循环识别标签。
startInventoryTag(InventoryParameter) - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
  开始循环识别标签。
startInventoryTag(InventoryParameter) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  开始循环识别标签。
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  开始循环识别标签
  Begin looping through the identification labels.
  通过 `RFIDWithUHFA4NetWork.setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 这个回调接口获取标签数据，需要在开始盘点之前调用setInventoryCallback方法。
  Get the label data through the callback interface `RFIDWithUHFA4NetWork.setInventoryCallback(IUHFInventoryCallback inventoryCallback)`, you need to call the setInventoryCallback method before starting the inventory.
  备注：开启循环识别标签后模块只能响应`RFIDWithUHFA4NetWork.stopInventory()`函数 。
  Note: The module can only respond to the `RFIDWithUHFA4NetWork.stopInventory()` function after the loop identification tag is turned on.
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  开始循环识别标签。
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
  开始循环识别标签。
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  开始循环识别标签。
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  开始循环识别标签。
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
startInventoryTag(InventoryParameter) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
startInventoryTag(int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
startInventoryTag(InventoryParameter) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
startInventoryTag(InventoryParameter) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  开始循环识别标签。
startInventoryTag(InventoryParameter) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  开始循环识别标签。
startInventoryTag(InventoryParameter) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
startInventoryTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
startInventoryTag() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startInventoryTag() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.custom.UHFCSYX_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
startInventoryTag(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFRLM_qcom
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  启动识别Tag循环，只是开启识别Tag循环，之后将识别到的标签号上传到缓冲区， `RFIDWithUHFUrxUart_qcom.readTagFromBuffer()`
  Enable Tag auto reading and upload tag number to buffer, `RFIDWithUHFUrxUart_qcom.readTagFromBuffer()`
  用于从缓冲区读取一个标签号数据，开启循环识别之后，模块只能响应`RFIDWithUHFUrxUart_qcom.stopInventory()`函数 。
  Read tag data from buffer, after switch on auto reading, module will give feedback to `RFIDWithUHFUrxUart_qcom.stopInventory()` only.
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
startInventoryTag(InventoryParameter) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
startInventoryTag() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
startInventoryTemperatureTag(int) - Method in class com.rscja.custom.UHFUartTemperatureTag
startInventoryThread() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
startLocation(String, int, int, IUHFLocationCallback) - Method in class com.rscja.deviceapi.BleDevice
  开始定位
startLocation(String, int, int, IUHFLocationCallback) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in interface com.rscja.deviceapi.interfaces.IHandheldRFID
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  开始定位
  Start location
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  开始定位
  Start location
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  开始定位
  Start location
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
startLocation(String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
  开始定位
  Start location
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
  开始定位
  Start location
startLocation(Context, String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
startLocation(String, int, int, IUHFLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.UhfLocation_qcom
startLocation(String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.UhfRadarLocation_qcom
startLogging(float, float, int, int) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
startLogging(int, int, int, String, float, float, int, int) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
startLogging(float, float, int, int) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
startLogging(int, int, int, String, float, float, int, int) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
startLogging(float, float, int, int) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
startLogging(int, int, int, String, float, float, int, int) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
  开始测量温度
startLogging(float, float, int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
startLogging(int, int, int, String, float, float, int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
  开始测量温度
startLogging(float, float, int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
startLogging(int, int, int, String, float, float, int, int) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
startLoggingRequest(int, int, int, byte[], float, float, int, int) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
startLoggingRequest(int, int, int, byte[], float, float, int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
startLoggingResponse(byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
startLoggingResponse(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
startMultiTagsLocate(List<UHFTAGInfo>, ITagLocationCallback<TagLocationEntity>) - Method in interface com.rscja.deviceapi.interfaces.ITagLocate
startMultiTagsLocate(List<UHFTAGInfo>, ITagLocationCallback<TagLocationEntity>) - Method in class com.rscja.team.qcom.deviceapi.TagLocate_qcom
  多标签定位
startPreview() - Method in interface com.rscja.deviceapi.interfaces.IBarcodePhoto
startPtCapture() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call up
  `FingerprintWithFIPS.setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setPtCaptureCallBack(PtCaptureCallBack callBack)` method to setup received call-back data.
startPtCapture(boolean) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startPtCapture() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call up
  `IFingerprintWithFIPS.setPtCaptureCallBack(FingerprintWithFIPS.PtCaptureCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithFIPS.setPtCaptureCallBack(FingerprintWithFIPS.PtCaptureCallBack callBack)` method to setup received call-back data.
startPtCapture(boolean) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `IFingerprintWithMorpho.setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithMorpho.setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack callBack)` setup receive call-back data
startPtCapture() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call up
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` method to setup received call-back data.
startPtCapture(boolean) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startPtCapture() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call up
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` method to setup received call-back data.
startPtCapture(boolean) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startPtCapturePKComp(boolean) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startPtCapturePKComp(boolean) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `IFingerprintWithMorpho.setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithMorpho.setPtCaptureCallBack(FingerprintWithMorpho.PtCaptureCallBack callBack)` setup receive call-back data
startPtCapturePKComp(boolean) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startPtCapturePKComp(boolean) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  开始获取指纹模版,注意:请调用
  Start acquire fingerprint template, attention: call out
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` 方法设置接收回调数据
  `#setPtCaptureCallBack(PtCaptureCallBack callBack)` setup receive call-back data
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in interface com.rscja.deviceapi.interfaces.IHandheldRFID
  开始定位
  Start location
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
  开始定位
  Start location
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  开始定位
  Start location
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
startRadarLocation(Context, String, int, int, IUHFRadarLocationCallback) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
startReceiveUhfTagInfo(IUHFInventoryCallback) - Method in class com.rscja.team.qcom.socket.SocketUdpClientUR4
startScan() - Method in class com.rscja.barcode.BarcodeDecoder
  触发二维条码扫描
  Trigger 2D barcode scanning function
startScan(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.barcode.BarcodeUtility
  开始扫描 Start scanning
startScan(Context, BarcodeUtility.ModuleType) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  开始扫描 Start scanning
startScan(Context, int) - Method in interface com.rscja.scanner.IScanner
  开始扫描或者读卡
  start scanning or card-reading
startScan(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
startScan() - Method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
startScan() - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  触发二维条码扫描
  Trigger 2D barcode scanning function
startScan(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  开始扫描 Start scanning
startScan(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
startScan() - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
startScan(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  开始扫描 Start scanning
startScan(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
startScanBarcode() - Method in class com.rscja.deviceapi.BluetoothReader
startScanBarcode() - Method in interface com.rscja.deviceapi.interfaces.IReader
startScanBarcode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
startScanBarcode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
startScanBarcode() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startScanBarcode() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
startScanBarcode() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
startScanBarcodeInBlinkMode(BluetoothReader.DecodeCallback) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startScanBarcodeInBlinkMode(BluetoothReader.DecodeCallback) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
startScanBarcodeInTriggleMode(BluetoothReader.DecodeCallback) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startScanBarcodeInTriggleMode(BluetoothReader.DecodeCallback) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
startScanBTDevices(ScanBTCallback) - Method in class com.rscja.deviceapi.BluetoothReader
startScanBTDevices(ScanBTCallback) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  扫描蓝牙设备(scanning Bluetooth devices)
startScanBTDevices(ScanBTCallback, Context) - Method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
  搜索蓝牙
startScanBTDevices(ScanBTCallback) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
startScanBTDevices(ScanBTCallback) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
startTemplateVerify(char[]) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `FingerprintWithFIPS.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithFIPS.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(byte[], int) - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `FingerprintWithMorpho.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `FingerprintWithMorpho.setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(char[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `IFingerprintWithFIPS.setTemplateVerifyCallBack(FingerprintWithFIPS.TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithFIPS.setTemplateVerifyCallBack(FingerprintWithFIPS.TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(byte[], int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `IFingerprintWithMorpho.setTemplateVerifyCallBack(FingerprintWithMorpho.TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `IFingerprintWithMorpho.setTemplateVerifyCallBack(FingerprintWithMorpho.TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(char[]) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(byte[], int) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(char[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startTemplateVerify(byte[], int) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  开始模版验证,注意:请调用
  start template verification, attention: call out
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)` 方法设置接收回调数据
  `#setTemplateVerifyCallBack(TemplateVerifyCallBack callBack)`method to setup received call-back data.
startUpgradeTcpService() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
  升级TCP服务
startUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  升级UHF Tcp服务器程序第三步,发送数据到服务器
startUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  升级UHF Tcp服务器程序第三步,发送数据到服务器
startUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  升级UHF Tcp服务器程序第三步,发送数据到服务器
startUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  升级UHF Tcp服务器程序第三步,发送数据到服务器
startUpgradeTcpServiceSendData(long, byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
startUpgradeUhfSendData(long, byte[]) - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
startUPImage(FingerprintWithTLK1NC.IUPImageCallback) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
  // * @param timeOut timeOut (unit:millisecond)
startUPImage(FingerprintWithTLK1NC.IUPImageCallback) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
  // * @param timeOut timeOut (unit:millisecond)
startUPImage(FingerprintWithTLK1NC.IUPImageCallback) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
startUPImage(FingerprintWithTLK1NC.IUPImageCallback) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
  // * @param timeOut timeOut (unit:millisecond)
startVideo(IBarcodeVideoCallback) - Method in interface com.rscja.deviceapi.interfaces.IBarcodePhoto
STATUS_FAILURE - Variable in class com.rscja.deviceapi.FingerprintWithTLK1NC
STATUS_FAILURE - Variable in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
STATUS_FAILURE - Variable in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
STATUS_SUCCESS - Variable in class com.rscja.deviceapi.FingerprintWithTLK1NC
STATUS_SUCCESS - Variable in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
STATUS_SUCCESS - Variable in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
STATUS_TIMEOUT - Variable in class com.rscja.deviceapi.FingerprintWithTLK1NC
STATUS_TIMEOUT - Variable in class com.rscja.team.mtk.deviceapi.FingerprintWithTLK1NC_mtk
STATUS_TIMEOUT - Variable in class com.rscja.team.qcom.deviceapi.FingerprintWithTLK1NC_qcom
stop() - Method in interface com.rscja.deviceapi.interfaces.IUHFUrxAutoInventoryTag
stop() - Method in class com.rscja.team.qcom.deviceapi.UHFUrxNetWorkAutoInventoryTag_qcom
stop2DSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
STOPBITS_1 - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  1 stop bit.
STOPBITS_1_5 - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  1.5 stop bits.
STOPBITS_2 - Static variable in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  2 stop bits.
stopDown() - Method in class com.rscja.team.qcom.http.HttpUtils_qcom
stopEnroll() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止采集指纹
  Stop acquiring fingerprint
stopEnroll() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  Deprecated.
stopEnroll() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  停止采集指纹
  Stop acquiring fingerprint
stopEnroll() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  Deprecated.
stopEnroll() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  停止采集指纹
  Stop acquiring fingerprint
stopEnroll() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  Deprecated.
stopEnroll() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  停止采集指纹
  Stop acquiring fingerprint
stopEnroll() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  Deprecated.
stopGRAB() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止获取图片
  stop acquiring picture
stopGRAB() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  停止获取图片
  stop acquiring picture
stopGRAB() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  停止获取图片
  stop acquiring picture
stopGRAB() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  停止获取图片
  stop acquiring picture
stopIdentification() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止指纹验证
  Stop fingerprint verification
stopIdentification() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  Deprecated.
stopIdentification() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  停止指纹验证
  Stop fingerprint verification
stopIdentification() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  Deprecated.
stopIdentification() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  停止指纹验证
  Stop fingerprint verification
stopIdentification() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  Deprecated.
stopIdentification() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  停止指纹验证
  Stop fingerprint verification
stopIdentification() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  Deprecated.
stopInventory() - Method in class com.rscja.custom.UHFCSYX_A4NetWork
stopInventory() - Method in class com.rscja.custom.UHFCSYXForURx
stopInventory() - Method in class com.rscja.custom.UHFTemperatureSensors
stopInventory() - Method in class com.rscja.custom.UHFTemperatureTag
stopInventory() - Method in class com.rscja.custom.UHFUartTemperatureTag
stopInventory() - Method in class com.rscja.deviceapi.BleDevice
  停止循环识别
  Stop auto reading
stopInventory() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
stopInventory() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  停止循环识别，在调用此函数之后应当退出循环获取缓冲区的标签信息的子线程
  Stop auto reading, after call this function to exit sub threads of tag data of buffer.
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  停止循环盘点标签(Stop cycle count labels)
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  停止循环盘点标签(Stop cycle count labels)
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  停止循环盘点标签(Stop cycle count labels)
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  停止循环盘点标签(Stop cycle count labels)
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  停止循环识别，在调用此函数之后应当退出循环获取缓冲区的标签信息的子线程
  Stop auto reading, after call this function to exit sub threads of tag data of buffer.
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
stopInventory() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
stopInventory() - Method in class com.rscja.deviceapi.UhfBase
stopInventory() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
stopInventory() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
stopInventory() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN51_qcom
stopInventory() - Method in class com.rscja.team.qcom.ble.RFIDWithUHFBLEN52_qcom
stopInventory() - Method in class com.rscja.team.qcom.custom.M775Authenticate_qcom
stopInventory() - Method in class com.rscja.team.qcom.custom.UHFCSYX_qcom
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  停止循环识别，在调用此函数之后应当退出循环获取缓冲区的标签信息的子线程
  Stop auto reading, after call this function to exit sub threads of tag data of buffer.
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
stopInventory() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
stopLocation() - Method in class com.rscja.deviceapi.BleDevice
  停止定位
stopLocation() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
stopLocation() - Method in interface com.rscja.deviceapi.interfaces.IHandheldRFID
stopLocation() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  停止定位 Stop location
stopLocation() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  停止定位 Stop location
stopLocation() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
stopLocation() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
  停止定位 Stop location
stopLocation() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
stopLocation() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
stopLocation() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
  停止定位 Stop location
stopLocation() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
  停止定位 Stop location
stopLocation() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
stopLocation() - Method in class com.rscja.team.qcom.deviceapi.UhfLocation_qcom
stopLocation() - Method in class com.rscja.team.qcom.deviceapi.UhfRadarLocation_qcom
stopLogging(String) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
stopLogging(int, int, int, String, String) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
stopLogging(String) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
stopLogging(int, int, int, String, String) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
stopLogging(String) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
stopLogging(int, int, int, String, String) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
  停止测量温度
stopLogging(String) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
stopLogging(int, int, int, String, String) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
  停止测量温度
stopLogging(String) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
stopLogging(int, int, int, String, String) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
stopLoggingRequest(int, int, int, byte[], byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
stopLoggingRequest(int, int, int, byte[], byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
stopLoggingResponse(byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
stopLoggingResponse(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
stopMultiTagsLocate() - Method in interface com.rscja.deviceapi.interfaces.ITagLocate
stopMultiTagsLocate() - Method in class com.rscja.team.qcom.deviceapi.TagLocate_qcom
  停止多标签定位
stopPreview() - Method in interface com.rscja.deviceapi.interfaces.IBarcodePhoto
stopPtCapture() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止获取指纹模版
  Stop acquiring fingerprint template
stopPtCapture() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  Deprecated.
stopPtCapture() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  停止获取指纹模版
  Stop acquiring fingerprint template
stopPtCapture() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  Deprecated.
stopPtCapture() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  停止获取指纹模版
  Stop acquiring fingerprint template
stopPtCapture() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithMorpho_mtk
  Deprecated.
stopPtCapture() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  停止获取指纹模版
  Stop acquiring fingerprint template
stopPtCapture() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithMorpho_qcom
  Deprecated.
stopRadarLocation() - Method in interface com.rscja.deviceapi.interfaces.IHandheldRFID
stopRadarLocation() - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
  设置R6工作模式
stopRadarLocation() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  关闭定位
  Start location
stopRadarLocation() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
stopRadarLocation() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
stopRadarLocation() - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
stopRadarLocation() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
stopRadarLocation() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
stopRadarLocation() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
stopRadarLocation() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
stopReceiveThread() - Method in class com.rscja.team.qcom.socket.SocketUdpClientUR4
stopScan() - Method in class com.rscja.barcode.BarcodeDecoder
  终止扫描
  Scanning terminated
stopScan(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.barcode.BarcodeUtility
  停止扫描 Stop scanning
stopScan() - Method in class com.rscja.deviceapi.Barcode1D
  终止扫描
  Scanning terminated
stopScan() - Method in class com.rscja.deviceapi.Barcode2D
  终止扫描
  Scanning terminated
stopScan() - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  终止扫描
  Scanning terminated
stopScan() - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  终止扫描
  Scanning terminated
stopScan(Context, BarcodeUtility.ModuleType) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  停止扫描 Stop scanning
stopScan(Context, int) - Method in interface com.rscja.scanner.IScanner
  停止扫描
  Stop scanning
stopScan(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
stopScan() - Method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
stopScan() - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  终止扫描
  Scanning terminated
stopScan(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  停止扫描 Stop scanning
stopScan() - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  终止扫描
  Scanning terminated
stopScan() - Method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  终止扫描
  Scanning terminated
stopScan(Context, int) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
stopScan() - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
stopScan(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  停止扫描 Stop scanning
stopScan() - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  终止扫描
  Scanning terminated
stopScan() - Method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  终止扫描
  Scanning terminated
stopScan(Context, int) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
stopScanBarcode() - Method in class com.rscja.deviceapi.BluetoothReader
stopScanBarcode() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
stopScanBarcode() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
stopScanBarcode() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
stopScanBTDevices() - Method in class com.rscja.deviceapi.BluetoothReader
stopScanBTDevices() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  停止扫描蓝牙设备(Stop scanning Bluetooth devices)
stopScanBTDevices() - Method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
  停止搜索蓝牙
stopScanBTDevices() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
stopScanBTDevices() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
stoptBTScan() - Method in class com.rscja.team.qcom.service.BLEService_qcom
stopTemplateVerify() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  停止模版比对
  Stop template comparison
stopTemplateVerify() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  停止模版比对
  Stop template comparison
stopTemplateVerify() - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  停止模版比对
  Stop template comparison
stopTemplateVerify() - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  停止模版比对
  Stop template comparison
storChar(Fingerprint.BufferEnum, int) - Method in class com.rscja.deviceapi.Fingerprint
  存储模板文件。将模板缓冲区buffer中的模板文件存到 PageID号所对应的指纹库位置
  save templatefile.
storChar(Fingerprint.BufferEnum, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  存储模板文件。将模板缓冲区buffer中的模板文件存到 PageID号所对应的指纹库位置
  save templatefile.
storChar(Fingerprint.BufferEnum, int) - Method in class com.rscja.team.qcom.deviceapi.Fingerprint_qcom
  存储模板文件。将模板缓冲区buffer中的模板文件存到 PageID号所对应的指纹库位置
  save templatefile.
storeChar(int, FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  将保存于指定 Ram Buffer 中的模板保存于指定编号的模块指纹库中
storeChar(int, FingerprintWithZAZ.BufferEnum, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  将保存于指定 Ram Buffer 中的模板保存于指定编号的模块指纹库中
storeChar(int, FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithZAZ_qcom
  将保存于指定 Ram Buffer 中的模板保存于指定编号的模块指纹库中
storeFinger(byte[]) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  将指纹模板导入到指纹模块中
storeFinger(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  将指纹模板导入到指纹模块中
storeFinger(byte[]) - Method in class com.rscja.team.mtk.deviceapi.FingerprintWithFIPS_mtk
  将指纹模板导入到指纹模块中
storeFinger(byte[]) - Method in class com.rscja.team.qcom.deviceapi.FingerprintWithFIPS_qcom
  将指纹模板导入到指纹模块中
STR_AIM_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_AUSPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_AZTEC - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_BOOKLAND - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_BPO - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CANPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CHINAPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODABAR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODABLOCK - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODABLOCK_A - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE11 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE32 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE39 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE39_FULL_ASCII - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE49 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE93 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CODE_16K - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_COUPON_CODE - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_CUSTOM_GS1_DATAMATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_DATAMATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_DISCRETE_2_OF_5 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_DUTCHPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_EAN13 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_EAN8 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_EAN_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_GM - Static variable in class com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
STR_GRIDMATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_GS1_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_GS1_DATA_MATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_GS1_DataBar - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_GS1_DataBar_Expanded - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_GS1_DataBar_Limited - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_GS1_QR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_HANXIN - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_IATA - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_INDUSTRIAL_2_5 - Static variable in class com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
STR_INFOMAIL - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_INTERLEAVED_2_OF_5 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_ISBT_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_ISBT_128 - Static variable in class com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
STR_ISSN - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_JAPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_KOREAPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_MACRO_PDF - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_MACRO_QR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_MATRIX25 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_MAXICODE - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_MICRO_QR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_MICROPDF - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_MSI - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_NEC_2_OF_5 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_OCR - Static variable in class com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
STR_PDF417 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_PLANET - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_POSTAL_4I - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_QR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_STANDARD_2_5 - Static variable in class com.rscja.team.mtk.barcode.BarcodeSymbolUtility_mtk
STR_TELEPEN - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_TLCODE39 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_TRIOPTIC - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_UPC_D - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_UPC_E1 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_UPCA - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_UPCE0 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_US_POSTALS1 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
STR_USPS4CB - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
string2Int(String, int) - Static method in class com.rscja.utility.StringUtility
  字符串转整数
StringUtility - Class in com.rscja.utility
  字符工具类
StringUtility() - Constructor for class com.rscja.utility.StringUtility
successNotify() - Method in interface com.rscja.deviceapi.interfaces.IURAxOfAndroidUart
  成功的通知提示(指示灯闪烁同时发出提示音)
  Success Notification Sound (Play notification tune when light flashing)
successNotify() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  成功的通知提示(指示灯闪烁同时发出提示音)
  Success Notification Sound (Play notification tune when light flashing)
successNotify() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
successNotify() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
  成功的通知提示(指示灯闪烁同时发出提示音)
  Success Notification Sound (Play notification tune when light flashing)
successNotify() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  成功的通知提示(指示灯闪烁同时发出提示音)
  Success Notification Sound (Play notification tune when light flashing)
successNotify() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
successNotify() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
  成功的通知提示(指示灯闪烁同时发出提示音)
  Success Notification Sound (Play notification tune when light flashing)
switchBaudrate(int, int, int, int) - Method in class com.rscja.deviceapi.Infrared
  切换波特率
switchBaudrate(int, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  切换波特率
switchBaudrate(int, int, int, int) - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  切换波特率
SysInterfacesOfC66P_qcom - Class in com.rscja.team.qcom.system
SysInterfacesOfC66P_qcom(Context) - Constructor for class com.rscja.team.qcom.system.SysInterfacesOfC66P_qcom
SysInterfacesOfC7XA11_mtk - Class in com.rscja.team.mtk.system
SysInterfacesOfC7XA11_mtk(Context) - Constructor for class com.rscja.team.mtk.system.SysInterfacesOfC7XA11_mtk
SystemInterfacesFactory - Class in com.rscja.system
  系统接口工厂类
SystemInterfacesFactory_mtk - Class in com.rscja.team.mtk.system
SystemInterfacesFactory_qcom - Class in com.rscja.team.qcom.system
  系统接口工厂类
SystemPropValues_mtk - Class in com.rscja.team.mtk.system
SystemPropValues_qcom - Class in com.rscja.team.qcom.system
SystemSettingsDBData_mtk - Class in com.rscja.team.mtk.system
SystemSettingsDBData_mtk() - Constructor for class com.rscja.team.mtk.system.SystemSettingsDBData_mtk

A B C D E F G H I J K L M N O P Q R S T U V W X Z