## Uses of Class
com.rscja.deviceapi.entity.AntennaState

- Packages that use AntennaState
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.qcom.deviceapi |

- - ### Uses of AntennaState in com.rscja.deviceapi

    Methods in com.rscja.deviceapi that return types with arguments of type AntennaState
    Modifier and Type | Method and Description
    --- | ---
    `java.util.List<AntennaState>` | RFIDWithUHFA8NetWork.`getANT()` 获取天线启用状态(Get the antenna enable status)
    `java.util.List<AntennaState>` | RFIDWithUHFA8.`getANT()` 获取当前设置的天线 Acquire current antenna
    `java.util.List<AntennaState>` | RFIDWithUHFUrxUart.`getANT()` 获取天线
    `java.util.List<AntennaState>` | RFIDWithUHFUrxUsbToUart.`getANT()`
    `java.util.List<AntennaState>` | RFIDWithUHFUrxNetwork.`getANT()`
    `java.util.List<AntennaState>` | RFIDWithUHFA4.`getANT()` 获取当前设置的天线 Acquire current antenna
    `java.util.List<AntennaState>` | RFIDWithUHFA4NetWork.`getANT()` 获取天线启用状态(Get the antenna enable status)
    `java.util.List<AntennaState>` | RFIDWithUHFAxBase.`getANT()` 获取当前设置的天线
    `java.util.List<AntennaState>` | RFIDWithUHFA4RS232.`getANT()` 获取天线启用状态(Get the antenna enable status)
    `java.util.List<AntennaState>` | RFIDWithUHFA8RS232.`getANT()` 获取天线启用状态(Get the antenna enable status)

    Method parameters in com.rscja.deviceapi with type arguments of type AntennaState
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFA8NetWork.`setANT(java.util.List<AntennaState> antStatus)` 设置天线启用状态(Set the antenna enable state)
    `boolean` | RFIDWithUHFA8.`setANT(java.util.List<AntennaState> antStatus)` 设置天线号 Setup antenna number
    `boolean` | RFIDWithUHFUrxUart.`setANT(java.util.List<AntennaState> antStatus)` 设置天线
    `boolean` | RFIDWithUHFUrxUsbToUart.`setANT(java.util.List<AntennaState> antStatus)`
    `boolean` | RFIDWithUHFUrxNetwork.`setANT(java.util.List<AntennaState> antStatus)`
    `boolean` | RFIDWithUHFA4.`setANT(java.util.List<AntennaState> antStatus)` 设置天线号 Setup antenna number
    `boolean` | RFIDWithUHFA4NetWork.`setANT(java.util.List<AntennaState> antStatus)` 设置天线启用状态(Set the antenna enable state)
    `boolean` | RFIDWithUHFAxBase.`setANT(java.util.List<AntennaState> antStatus)` 设置天线号
    `boolean` | RFIDWithUHFA4RS232.`setANT(java.util.List<AntennaState> antStatus)` 设置天线启用状态(Set the antenna enable state)
    `boolean` | RFIDWithUHFA8RS232.`setANT(java.util.List<AntennaState> antStatus)` 设置天线启用状态(Set the antenna enable state)

  - ### Uses of AntennaState in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces that return types with arguments of type AntennaState
    Modifier and Type | Method and Description
    --- | ---
    `java.util.List<AntennaState>` | IUHFURx.`getANT()` 获取天线
    `java.util.List<AntennaState>` | IMultipleAntenna.`getANT()` 获取当前设置的天线

    Method parameters in com.rscja.deviceapi.interfaces with type arguments of type AntennaState
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | IUHFURx.`setANT(java.util.List<AntennaState> antStatus)` 设置天线
    `boolean` | IMultipleAntenna.`setANT(java.util.List<AntennaState> antStatus)` 设置天线

  - ### Uses of AntennaState in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi that return types with arguments of type AntennaState
    Modifier and Type | Method and Description
    --- | ---
    `java.util.List<AntennaState>` | RFIDWithUHFUrxUsbToUart_qcom.`getANT()`
    `java.util.List<AntennaState>` | RFIDWithUHFUrxUart_qcom.`getANT()` 获取天线
    `java.util.List<AntennaState>` | RFIDWithUHFUrxUart2_qcom.`getANT()`
    `java.util.List<AntennaState>` | RFIDWithUHFUrxNetwork_qcom.`getANT()`
    `java.util.List<AntennaState>` | RFIDWithUHFAxBase_qcom.`getANT()` 获取当前设置的天线
    `java.util.List<AntennaState>` | RFIDWithUHFA8_qcom.`getANT()` 获取当前设置的天线 Acquire current antenna
    `java.util.List<AntennaState>` | RFIDWithUHFA4_qcom.`getANT()` 获取当前设置的天线 Acquire current antenna

    Method parameters in com.rscja.team.qcom.deviceapi with type arguments of type AntennaState
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | RFIDWithUHFUrxUsbToUart_qcom.`setANT(java.util.List<AntennaState> antStatus)`
    `boolean` | RFIDWithUHFUrxUart_qcom.`setANT(java.util.List<AntennaState> antStatus)` 设置天线
    `boolean` | RFIDWithUHFUrxUart2_qcom.`setANT(java.util.List<AntennaState> antStatus)`
    `boolean` | RFIDWithUHFUrxNetwork_qcom.`setANT(java.util.List<AntennaState> antStatus)`
    `boolean` | RFIDWithUHFAxBase_qcom.`setANT(java.util.List<AntennaState> antStatus)` 设置天线启用状态(Set the antenna enable state)
    `boolean` | RFIDWithUHFA8_qcom.`setANT(java.util.List<AntennaState> antStatus)` 设置天线号 Setup antenna number
    `boolean` | RFIDWithUHFA4_qcom.`setANT(java.util.List<AntennaState> antStatus)` 设置天线号 Setup antenna number