A B C D E F G H I J K L M N O P Q R S T U V W X Z

## B

B - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
Bank_EPC - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  EPC存储区(EPC area)
Bank_RESERVED - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  RESERVED存储区（RESERVED area）
Bank_TID - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  TID存储区(TID area)
Bank_USER - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
  USER存储区(USER area)
Barcode1D - Class in com.rscja.deviceapi
  一维条码操作类
  1D barcode operation class
Barcode1D_mtk - Class in com.rscja.team.mtk.deviceapi
  一维条码操作类
  1D barcode operation class
Barcode1D_qcom - Class in com.rscja.team.qcom.deviceapi
  一维条码操作类
  1D barcode operation class
Barcode1D_qcom.UHFProtocolParseBase - Class in com.rscja.team.qcom.deviceapi
Barcode2D - Class in com.rscja.deviceapi
  二维条码操作类
  2D barcode operation class.
Barcode2D_mtk - Class in com.rscja.team.mtk.deviceapi
  二维条码操作类
  2D barcode operation class.
Barcode2D_qcom - Class in com.rscja.team.qcom.deviceapi
  二维条码操作类
  2D barcode operation class.
Barcode2DFactory_mtk - Class in com.rscja.team.mtk.barcode.barcode2d
Barcode2DFactory_qcom - Class in com.rscja.team.qcom.barcode.barcode2d
  2D 条码工厂类
Barcode2DSHardwareInfo - Class in com.rscja.barcode
Barcode2DSHardwareInfo() - Constructor for class com.rscja.barcode.Barcode2DSHardwareInfo
Barcode2DSHardwareInfo_mtk - Class in com.rscja.team.mtk.barcode
Barcode2DSHardwareInfo_mtk() - Constructor for class com.rscja.team.mtk.barcode.Barcode2DSHardwareInfo_mtk
Barcode2DSHardwareInfo_qcom - Class in com.rscja.team.qcom.barcode
Barcode2DSHardwareInfo_qcom() - Constructor for class com.rscja.team.qcom.barcode.Barcode2DSHardwareInfo_qcom
Barcode2DSoftCommon(Context) - Method in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
Barcode2DSoftCommon_mtk - Class in com.rscja.team.mtk.barcode
Barcode2DSoftCommon_mtk() - Constructor for class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
Barcode_1D_Close(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_1D_Close(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_1D_Open(String, String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_1D_Open(String, String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_1D_Scan(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_1D_Scan(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_1D_SetTimeOut(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_1D_SetTimeOut(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_1D_StopScan(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_1D_StopScan(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_2D_Close(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_2D_Close(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_2D_Open(String, String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_2D_Open(String, String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_2D_Scan(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_2D_Scan(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_2D_SetTimeOut(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_2D_SetTimeOut(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Barcode_2D_StopScan(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Barcode_2D_StopScan(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
BARCODE_BYTE_DATA - Static variable in class com.rscja.barcode.ConstantUtil
BARCODE_CODE - Static variable in class com.rscja.barcode.ConstantUtil
BARCODE_DECODE_TIME - Static variable in class com.rscja.barcode.ConstantUtil
BARCODE_HEX_DATA - Static variable in class com.rscja.barcode.ConstantUtil
BARCODE_NAME - Static variable in class com.rscja.barcode.ConstantUtil
BARCODE_RESULT_CODE - Static variable in class com.rscja.barcode.ConstantUtil
BARCODE_STRING_DATA - Static variable in class com.rscja.barcode.ConstantUtil
BarcodeDecoder - Class in com.rscja.barcode
BarcodeDecoder() - Constructor for class com.rscja.barcode.BarcodeDecoder
BarcodeDecoder.DecodeCallback - Interface in com.rscja.barcode
BarcodeDecoder.IBarcodeImageCallback - Interface in com.rscja.barcode
BarcodeDecoder_mtk - Class in com.rscja.team.mtk.barcode
BarcodeDecoder_mtk() - Constructor for class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
BarcodeDecoder_mtk.DecodeCallback - Interface in com.rscja.team.mtk.barcode
BarcodeEntity - Class in com.rscja.deviceapi.entity
BarcodeEntity() - Constructor for class com.rscja.deviceapi.entity.BarcodeEntity
BarcodeEntity(int, int) - Constructor for class com.rscja.deviceapi.entity.BarcodeEntity
BarcodeFactory - Class in com.rscja.barcode
  条码工厂类
BarcodeFactory_mtk - Class in com.rscja.team.mtk.barcode
  条码工厂类
BarcodeFactory_qcom - Class in com.rscja.team.qcom.barcode
  条码工厂类
BarcodeResult - Class in com.rscja.deviceapi.entity
barcodeScanTimeOutSend() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
BarcodeSymbolUtility - Class in com.rscja.barcode
  条码符号工具类
BarcodeSymbolUtility_mtk - Class in com.rscja.team.mtk.barcode
  条码符号工具类
BarcodeSymbolUtility_qcom - Class in com.rscja.team.qcom.barcode
  条码符号工具类
BarcodeUtility - Class in com.rscja.barcode
  条码操作类 barcode operate class 注意： Attention: 1、使用前请确认您的机器已安装键盘助手v1.9.0 之后的版本。 1.
BarcodeUtility.ModuleType - Enum in com.rscja.barcode
BarcodeUtility_mtk - Class in com.rscja.team.mtk.barcode
  条码操作类 barcode operate class 注意： Attention: 1、使用前请确认您的机器已安装键盘助手v1.9.0 之后的版本。 1.
BarcodeUtility_qcom - Class in com.rscja.team.qcom.barcode
  条码操作类 barcode operate class 注意： Attention: 1、使用前请确认您的机器已安装键盘助手v1.9.0 之后的版本。 1.
BatteryEntity - Class in com.rscja.deviceapi.entity
BatteryEntity(int) - Constructor for class com.rscja.deviceapi.entity.BatteryEntity
BatteryManage - Class in com.rscja.team.mtk.utility
BatteryUtils - Class in com.rscja.utility
BatteryUtils() - Constructor for class com.rscja.utility.BatteryUtils
bdOff(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
bdOff(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
bdOn(String) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
bdOn(String) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
BitToByte(String) - Static method in class com.rscja.utility.StringUtility
  Bit转Byte
BLE_UUID_GAP - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
BLE_UUID_GAP_CHARACTERISTIC_DEVICE_NAME - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
BleDevice - Class in com.rscja.deviceapi
  BLE蓝牙的操作对象
  1.通过`#connect(ConnectionStatusCallback
  ` 来连接蓝牙，bleStatusCallback是蓝牙状态的连接回调
  2.通过`BleDevice.setInventoryCallback(IUHFInventoryCallback inventoryCallback)` 标签数据回调接口。
  3.通过`BleDevice.startInventoryTag()` 开始盘点，在盘点过程中，ble设备只会响应`BleDevice.stopInventory()` ()}函数，不能设置和获取ble设备的相关其他参数。
  4.通过`BleDevice.stopInventory()` ()} 停止盘点
BleDevice(String, Context) - Constructor for class com.rscja.deviceapi.BleDevice
BleDevice.BleDeviceInfo - Class in com.rscja.deviceapi
BleDevice_qcom - Class in com.rscja.team.qcom.deviceapi
BleDevice_qcom(String, Context) - Constructor for class com.rscja.team.qcom.deviceapi.BleDevice_qcom
BLEService_qcom - Class in com.rscja.team.qcom.service
BLEService_qcom() - Constructor for class com.rscja.team.qcom.service.BLEService_qcom
BLEService_qcom.BluetoothStateReceiver - Class in com.rscja.team.qcom.service
BLEService_qcom.IDataCallBack - Interface in com.rscja.team.qcom.service
blink() - Method in class com.rscja.scanner.led.ScanLed
  亮0.5S后熄灭
  light up for 0.5s then OFF
blink(int, int) - Method in class com.rscja.scanner.led.ScanLed
  控制亮灯后自动熄灭
blink(Context) - Method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  亮0.5S后熄灭
  light up for 0.5s then OFF
blink(Context, int, int) - Method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  控制亮灯后自动熄灭
blink() - Method in class com.rscja.team.mtk.scanner.led.ScanLed_mtk
  亮0.5S后熄灭
  light up for 0.5s then OFF
blink(int, int) - Method in class com.rscja.team.mtk.scanner.led.ScanLed_mtk
  控制亮灯后自动熄灭
blink(Context) - Method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  亮0.5S后熄灭
  light up for 0.5s then OFF
blink(Context, int, int) - Method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  控制亮灯后自动熄灭
blinkOfLed(int, int, int) - Method in class com.rscja.deviceapi.BluetoothReader
  led 闪烁
blinkOfLed(int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IReader
  led 闪烁
blinkOfLed(int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  led 闪烁
blinkOfLed(int, int, int) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
blinkOfLed(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
  led 闪烁
blinkOfLed(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
  led 闪烁
blinkOfLedSendData(int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
blinkOfLedSendData(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
blockEraseDataSendData(String, char, int, int, String, char, int, char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
blockEraseDataSendData(String, char, int, int, String, char, int, char) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.BleDevice
  向标签写入数据(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入
  Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  向标签写入数据(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入
  Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  将数据写入指定标签(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入(Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.)
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  将数据写入指定标签(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入(Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.)
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  将数据写入指定标签(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入(Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.)
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  将数据写入指定标签(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入(Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.)
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  向标签写入数据(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入
  Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.mtk.deviceapi.RFIDWithUHFUART_mtk
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUART_qcom
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxNetwork_qcom
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart2_qcom
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUart_qcom
  向标签写入数据(支持大数据标签写入)、当需要写入的标签数据比较大可以使用此函数写入
  Write data into tag(support big-sized data writing), user could use this function when big-sized data need to be written.
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUrxUsbToUart_qcom
blockWriteData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
blockWriteDataSendData(String, char, int, int, String, char, int, char, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
blockWriteDataSendData(String, char, int, int, String, char, int, char, String) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
BluetoothReader - Class in com.rscja.deviceapi
  蓝牙读写器操作类：
  Bluetoot reader operation 第一步：调用`BluetoothReader.init(Context context)` 函数初始化蓝牙相关服务，退出应用程序需要调用`BluetoothReader.free()`是否蓝牙相关资源
  First step: Call `BluetoothReader.init(Context context)`to initiate BT service, call `BluetoothReader.free()` to exit application.
BluetoothReader.DecodeCallback - Interface in com.rscja.deviceapi
BluetoothReader.OnDataChangeListener - Interface in com.rscja.deviceapi
  接收蓝牙原始数据的接口
  Interface of receiving initial data.
BluetoothReader_qcom - Class in com.rscja.team.qcom.deviceapi
  蓝牙读写器操作类：
  Bluetoot reader operation 第一步：调用`BluetoothReader_qcom.init(Context context)` 函数初始化蓝牙相关服务，退出应用程序需要调用`BluetoothReader_qcom.free()`是否蓝牙相关资源
  First step: Call `BluetoothReader_qcom.init(Context context)`to initiate BT service, call `BluetoothReader_qcom.free()` to exit application.
BluetoothStateReceiver() - Constructor for class com.rscja.team.qcom.service.BLEService_qcom.BluetoothStateReceiver
BT_DEVICE - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
BT_RECORD - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
BT_RSSI - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
btDeleteAllTagToFlashSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
btDeleteAllTagToFlashSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
btGetAllTagNumFromFlashSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
btGetAllTagNumFromFlashSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
btGetNewTagNumFromFlashSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
btGetNewTagNumFromFlashSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
btGetTagDataFromFlashSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
btGetTagDataFromFlashSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
build(byte[], boolean, boolean) - Static method in class com.rscja.deviceapi.entity.BarcodeResult
build() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity.Builder
build() - Method in class com.rscja.deviceapi.entity.RadarLocationEntity.Builder
build() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
build() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo.Builder
builder(byte[], byte[]) - Static method in class com.rscja.deviceapi.entity.HF14443RequestEntity
Builder() - Constructor for class com.rscja.deviceapi.entity.HF15693RequestEntity.Builder
Builder() - Constructor for class com.rscja.deviceapi.entity.InventoryModeEntity.Builder
Builder() - Constructor for class com.rscja.deviceapi.entity.RadarLocationEntity.Builder
Builder() - Constructor for class com.rscja.deviceapi.entity.ScannerParameterEntity.Builder
Builder() - Constructor for class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo.Builder
builder1DConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建一维条码配置信息
  Create 1D barcode config infor.
builder1DConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建一维条码配置信息
  Create 1D barcode config infor.
builder2DConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建二维条码配置信息
  Create 2D barcode config infor.
builder2DConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建二维条码配置信息
  Create 2D barcode config infor.
builderA8ExtendedUartConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建A8扩展串口配置信息
builderA8ExtendedUartConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建A8扩展串口配置信息
builderBDConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建北斗配置信息
  Create Beidou config infor.
builderBDConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建北斗配置信息
  Create Beidou config infor.
builderDefaultConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
builderDefaultConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
builderFingerprintConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建Fingerprint配置信息
  Create Fingerprint config infor.
builderFingerprintConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建Fingerprint配置信息
  Create Fingerprint config infor.
builderInfraredConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建红外配置信息
  Create infrared config infor.
builderInfraredConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建红外配置信息
  Create infrared config infor.
builderLFConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建低频配置信息
  Create LF config infor.
builderLFConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建低频配置信息
  Create LF config infor.
builderPrinterConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建打印机配置信息
  Create printer config infor.
builderPrinterConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建打印机配置信息
  Create printer config infor.
builderRFIDConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建RFID配置信息
  Create RFID config infor.
builderRFIDConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建RFID配置信息
  Create RFID config infor.
builderUHFConfiguration() - Static method in class com.rscja.team.mtk.DeviceConfiguration_mtk
  创建UHF配置信息
  Create UHF config infor.
builderUHFConfiguration() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建UHF配置信息
  Create UHF config infor.
builderUrx() - Static method in class com.rscja.team.qcom.DeviceConfiguration_qcom
  创建ur 4 配置信息
  Create 1D barcode config infor.
buzzer() - Method in interface com.rscja.deviceapi.interfaces.IURAxOfAndroidUart
  成功的通知提示(发出提示音)
  Success Notification Sound (Play Sound)
buzzer() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  成功的通知提示(发出提示音)
  Success Notification Sound (Play Sound)
buzzer() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
  成功的通知提示(发出提示音)
  Success Notification Sound (Play Sound)
buzzer() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
  成功的通知提示(发出提示音)
  Success Notification Sound (Play Sound)
buzzer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA4_qcom
  成功的通知提示(发出提示音)
  Success Notification Sound (Play Sound)
buzzer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFA8_qcom
  成功的通知提示(发出提示音)
  Success Notification Sound (Play Sound)
buzzer() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
  成功的通知提示(发出提示音)
  Success Notification Sound (Play Sound)
buzzerOn(int, int, int) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFAxBase_qcom
byte2Bit(byte) - Static method in class com.rscja.utility.StringUtility
  Byte转Bit
byte2HexString(byte) - Static method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
byte2HexString(byte) - Static method in class com.rscja.utility.StringUtility
  byte转十六进制字符
byteArrayTolong(byte[]) - Static method in class com.rscja.utility.StringUtility
  将8字节的byte数组转成一个long值
bytes2HexString(byte[], int) - Static method in class com.rscja.utility.StringUtility
  byte类型数组转十六进制字符串
bytes2HexString(byte[], int, int) - Static method in class com.rscja.utility.StringUtility
bytes2HexString(byte[]) - Static method in class com.rscja.utility.StringUtility
bytes2HexString2(byte[], int) - Static method in class com.rscja.utility.StringUtility
bytes2HexString2(ArrayList<Byte>) - Static method in class com.rscja.utility.StringUtility
bytesConvertHexString(byte[], int, int) - Static method in class com.rscja.utility.StringUtility
bytesHexString(ArrayList<Byte>) - Static method in class com.rscja.utility.StringUtility
bytesHexString(byte[], int, int, boolean) - Static method in class com.rscja.utility.StringUtility
bytesHexString(byte[]) - Static method in class com.rscja.utility.StringUtility
bytesHexString(byte[], int) - Static method in class com.rscja.utility.StringUtility
  byte类型数组转十六进制字符串
bytesTochars(byte[], int) - Static method in class com.rscja.utility.StringUtility
bytesToHexString(byte[], int) - Static method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
bytesToHexString(byte[], int) - Static method in class com.rscja.utility.StringUtility
bytesToInt(byte[]) - Static method in class com.rscja.utility.StringUtility
  byte数组转成int值

A B C D E F G H I J K L M N O P Q R S T U V W X Z