## Uses of Interface
com.rscja.deviceapi.interfaces.IRFIDWithUHFUrxUsbToUart

- Packages that use IRFIDWithUHFUrxUsbToUart
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.team.qcom.deviceapi |

- - ### Uses of IRFIDWithUHFUrxUsbToUart in com.rscja.deviceapi

    Classes in com.rscja.deviceapi that implement IRFIDWithUHFUrxUsbToUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFUrxUsbToUart` URx 模块，串口通信操作类 URx module , serial communication operation interface 第一步:通过`RFIDWithUHFUrxUsbToUart.init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`RFIDWithUHFUrxUsbToUart.init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUrxUsbToUart.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUrxUsbToUart.stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.

  - ### Uses of IRFIDWithUHFUrxUsbToUart in com.rscja.team.qcom.deviceapi

    Classes in com.rscja.team.qcom.deviceapi that implement IRFIDWithUHFUrxUsbToUart
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFUrxUsbToUart_qcom` UR4 设备USB转串口,目前已经适配 pl2302芯片的usb转接线