A B C D E F G H I J K L M N O P Q R S T U V W X Z

## C

C - Static variable in class com.rscja.deviceapi.entity.BarcodeResult
C4000_6577 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C4000_6577 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C4000_6582 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C4000_6582 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C4050_6582 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C4050_6582 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C4050_8909 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C4050_8909 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C5_6765 - Static variable in class com.rscja.CWDeviceInfo
C5_6765 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C6000_6735 - Static variable in class com.rscja.CWDeviceInfo
C6000_6735 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C6000_6735 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C6000_6762 - Static variable in class com.rscja.CWDeviceInfo
C6000_6762 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C6000_6762_ScanLed_mtk - Class in com.rscja.team.mtk.scanner.led
C6000_8909 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C6000_8909 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C60_6765_11_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
C60_MTK_6765_110 - Static variable in class com.rscja.CWDeviceInfo
C60_MTK_6765_110 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C60_QCM2150_100 - Static variable in class com.rscja.CWDeviceInfo
C60_QCM2150_100 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C60_qcm2150_10_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
C60_SMD450_100 - Static variable in class com.rscja.CWDeviceInfo
C60_SMD450_100 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C61_SMD450_90 - Static variable in class com.rscja.CWDeviceInfo
C61_SMD450_90 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C61_smd450_90_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
C61P_SM6115_110 - Static variable in class com.rscja.CWDeviceInfo
C61P_SM6115_110 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C66_8953 - Static variable in class com.rscja.CWDeviceInfo
C66_8953 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C66_SMD450_90 - Static variable in class com.rscja.CWDeviceInfo
C66_SMD450_90 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C66_smd450_90_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
C66m_sm6115_10_ScanLed_qcom - Class in com.rscja.team.qcom.scanner.led
C66P_SM6115_110 - Static variable in class com.rscja.CWDeviceInfo
C66P_SM6115_110 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C70_6735 - Static variable in class com.rscja.CWDeviceInfo
C70_6735 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C70_6735 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C70_6763 - Static variable in class com.rscja.CWDeviceInfo
C70_6763 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C70_6763 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C70_6765 - Static variable in class com.rscja.CWDeviceInfo
C70_6765 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C71_6763 - Static variable in class com.rscja.CWDeviceInfo
C71_6763 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C71_6763 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C71_6765 - Static variable in class com.rscja.CWDeviceInfo
C71_6765 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C72_6735 - Static variable in class com.rscja.CWDeviceInfo
C72_6735 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C72_6735 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C72_6763 - Static variable in class com.rscja.CWDeviceInfo
C72_6763 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C72_6763 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C72_6765 - Static variable in class com.rscja.CWDeviceInfo
C72_6765 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C75_6765 - Static variable in class com.rscja.CWDeviceInfo
C75_6765 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C76_6735 - Static variable in class com.rscja.CWDeviceInfo
C76_6735 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C76_6735 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom
C76_6765 - Static variable in class com.rscja.CWDeviceInfo
C76_6765 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C7X_6765_ScanLed_mtk - Class in com.rscja.team.mtk.scanner.led
C90_6762_10 - Static variable in class com.rscja.CWDeviceInfo
C90_6762_10 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
C90_6762_ScanLed_mtk - Class in com.rscja.team.mtk.scanner.led
callback(M775Authenticate.AuthenticateInfo) - Method in interface com.rscja.custom.M775Authenticate.IUHFInventoryCallback
callback(UHFCSYX.TagAuthenticationResponseInfo) - Method in interface com.rscja.custom.UHFCSYX.IUHFInventoryCallback
callback(UHFTemperatureSensors.TemperatureTag) - Method in interface com.rscja.custom.UHFTemperatureSensors.IUHFInventoryTemperatureTagCallback
callback(UHFTemperatureTag.TemperatureTagInfo) - Method in interface com.rscja.custom.UHFTemperatureTag.InventoryTemperatureTagCallback
callback(UHFTemperatureTagsAPI.TempertureInfo) - Method in interface com.rscja.custom.UHFTemperatureTagsAPI.IUHFInventoryTempCallback
callback(UHFUartTemperatureTag.TemperatureTagInfo) - Method in interface com.rscja.custom.UHFUartTemperatureTag.InventoryTemperatureTagCallback
callback(UHFTAGInfo) - Method in class com.rscja.custom.UHFXSAPI
callback(List<GPIStateEntity>) - Method in interface com.rscja.deviceapi.interfaces.IGPIStateCallback
callback(UHFTAGInfo) - Method in interface com.rscja.deviceapi.interfaces.IUHFInventoryCallback
CameraID - Static variable in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
CameraStateFile - Static variable in class com.rscja.team.mtk.barcode.Barcode2DSoftCommon_mtk
  Deprecated.
CardBalance() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
CardBalance() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
CardConsume(byte[], char[], String, int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
CardConsume(byte[], char[], String, int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
cardConsumeConfirm(String, String, String) - Method in class com.rscja.deviceapi.CardWithBYL
cardConsumeConfirm(String, String, String) - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
CardConsumeConfirm(byte[], char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
cardConsumeConfirm(String, String, String) - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
CardConsumeConfirm(byte[], char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
CardWithBYL - Class in com.rscja.deviceapi
  白玉兰公交卡操作类
CardWithBYL_qcom - Class in com.rscja.team.qcom.deviceapi
  白玉兰公交卡操作类
CCCD - Static variable in class com.rscja.team.qcom.service.BLEService_qcom
char2HexString(char) - Static method in class com.rscja.utility.StringUtility
  char转十六进制
charArrayTolong(char[]) - Static method in class com.rscja.utility.StringUtility
  将8字节的Char数组转成一个long值
chars2HexString(char[], int) - Static method in class com.rscja.utility.StringUtility
  char类型数组转十六进制字符串
chars2Long(char[], int, int) - Static method in class com.rscja.utility.StringUtility
  char数组转long
charsTobytes(char[], int) - Static method in class com.rscja.utility.StringUtility
checkAntStatus(int, int) - Method in class com.rscja.custom.UHFSFForUrxNetwork
checkData(List<Byte>) - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom.UHFProtocolParseBase
checkParameter() - Method in class com.rscja.deviceapi.entity.Gen2Entity
checkTagState() - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
checkTagState(int, int, int, String) - Method in interface com.rscja.custom.interfaces.IUHFTemperatureTagsAPI
checkTagState() - Method in class com.rscja.custom.UHFTemperatureTagsAPI
checkTagState(int, int, int, String) - Method in class com.rscja.custom.UHFTemperatureTagsAPI
checkTagState() - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
checkTagState(int, int, int, String) - Method in class com.rscja.team.mtk.custom.UHFTemperatureTagsAPI_mtk
  检查测温状态
checkTagState() - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
checkTagState(int, int, int, String) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsAPI_qcom
  检查测温状态
checkTagState() - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
checkTagState(int, int, int, String) - Method in class com.rscja.team.qcom.custom.UHFTemperatureTagsBLEAPI
checkTagStateRequest(int, int, int, byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
checkTagStateRequest(int, int, int, byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
checkTagStateResponse(byte[]) - Method in interface com.rscja.custom.interfaces.IUHFProtocolParseBLE
checkTagStateResponse(byte[]) - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseBLE
CheckUtils - Class in com.rscja.team.qcom.utility
CheckUtils() - Constructor for class com.rscja.team.qcom.utility.CheckUtils
ChipInfo() - Constructor for class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo
cleanAllData() - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
cleanAllData() - Method in class com.rscja.team.qcom.uhfhandler.UHFUrAxDataHandle
cleanCmd() - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
cleanData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom
cleanFaultCard() - Method in class com.rscja.deviceapi.CardWithBYL
  清除故障卡
cleanFaultCard() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  清除故障卡
cleanFaultCard() - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
  清除故障卡
cleanOldCmd() - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
cleanOldCmd() - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
cleanReceiveData() - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
cleanReceiveData() - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
cleanReceiveData() - Method in class com.rscja.team.qcom.socket.SocketManageA4
cleanTagCmd() - Method in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase
cleanTagCmd() - Method in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase
CleanVar() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
CleanVar() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
clear() - Method in class com.rscja.team.qcom.utility.GyroAngle
clearCache() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  立即清空打印缓存,清空打印机接收缓冲区和打印缓冲区
  Clear up printing cache, clear printer receive zone and buffer zone
clearCache() - Method in class com.rscja.deviceapi.Printer
  立即清空打印缓存,清空打印机接收缓冲区和打印缓冲区
  Clear up printing cache, clear printer receive zone and buffer zone
clearCache() - Method in class com.rscja.team.mtk.deviceapi.Printer_mtk
  立即清空打印缓存,清空打印机接收缓冲区和打印缓冲区
  Clear up printing cache, clear printer receive zone and buffer zone
ClearCacheInfo() - Method in class com.rscja.team.qcom.socket.SocketManageUR4
clearXmlList() - Static method in class com.rscja.team.mtk.utility.FileUtils
clone() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo.ChipInfo
clone() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
close() - Method in class com.rscja.barcode.BarcodeDecoder
  关闭二维扫描设备
  Switch off 2D barcode scannning device
close(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.barcode.BarcodeUtility
  关闭指定功能 Switch off designated function
close() - Method in class com.rscja.deviceapi.Barcode1D
  关闭一维扫描设备
  Switch off 1D barcode scanning device.
close() - Method in class com.rscja.deviceapi.Barcode2D
  关闭二维扫描设备
  Switch off 2D barcode scanning device.
close() - Method in class com.rscja.deviceapi.Infrared
  关闭红外模块
  Switch off infared module
close() - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  关闭一维扫描设备
  Switch off 1D barcode scanning device.
close() - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  关闭二维扫描设备
  Switch off 2D barcode scanning device.
close(Context, BarcodeUtility.ModuleType) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  关闭指定功能 Switch off designated function
close() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  关闭红外模块
  Switch off infared module
close() - Method in interface com.rscja.deviceapi.interfaces.ILedLight
  关闭LED灯
  Switch off LED
close() - Method in class com.rscja.deviceapi.LedLight
  关闭LED灯
  Switch off LED
close(Context) - Method in interface com.rscja.scanner.IScanner
  关闭键盘助手总开关
  Switch off keyboardemulator
close(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
close() - Method in class com.rscja.team.mtk.barcode.barcode2d.KeyboardEmulator2DDecoder_mtk
close() - Method in class com.rscja.team.mtk.barcode.BarcodeDecoder_mtk
  关闭二维扫描设备
  Switch off 2D barcode scannning device
close(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  关闭指定功能 Switch off designated function
close() - Method in class com.rscja.team.mtk.deviceapi.Barcode1D_mtk
  关闭一维扫描设备
  Switch off 1D barcode scanning device.
close() - Method in class com.rscja.team.mtk.deviceapi.Barcode2D_mtk
  关闭二维扫描设备
  Switch off 2D barcode scanning device.
close() - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  关闭红外模块
  Switch off infared module
close() - Method in class com.rscja.team.mtk.deviceapi.LedLight_mtk
  关闭LED灯
  Switch off LED
close(Context) - Method in class com.rscja.team.mtk.scanner.utility.ScannerUtility_mtk
close() - Method in class com.rscja.team.qcom.barcode.barcode2d.KeyboardEmulator2DDecoder_qcom
close(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  关闭指定功能 Switch off designated function
close() - Method in class com.rscja.team.qcom.deviceapi.Barcode1D_qcom
  关闭一维扫描设备
  Switch off 1D barcode scanning device.
close() - Method in class com.rscja.team.qcom.deviceapi.Barcode2D_qcom
  关闭二维扫描设备
  Switch off 2D barcode scanning device.
close() - Method in class com.rscja.team.qcom.deviceapi.LedLight_qcom
  关闭LED灯
  Switch off LED
close() - Method in class com.rscja.team.qcom.rs232utils.UhfUartManage_qcom
close() - Method in class com.rscja.team.qcom.rs232utils.UhfUartUR4Manage_qcom
close(Context) - Method in class com.rscja.team.qcom.scanner.utility.ScannerUtility_qcom
close() - Method in class com.rscja.team.qcom.serialportapi.SerialPort
close() - Method in class com.rscja.team.qcom.service.BLEService_qcom
close() - Method in class com.rscja.team.qcom.socket.SocketManageA4
close() - Method in class com.rscja.team.qcom.socket.SocketManageUR4
close() - Method in class com.rscja.team.qcom.socket.SocketTcpIpBase
close() - Method in class com.rscja.team.qcom.socket.SocketUdpClient
close() - Method in class com.rscja.team.qcom.socket.SocketUdpClientUR4
close() - Method in interface com.rscja.team.qcom.usb.pl2302.UsbSerialPort_qcom
  Closes the port.
close() - Method in class com.rscja.team.qcom.usb.pl2302.UsbSerialPortImpl_qcom
closeAuxiliaryLight(Context) - Method in interface com.rscja.deviceapi.interfaces.IScanerLedLight
  关闭扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
closeAuxiliaryLight(Context) - Method in class com.rscja.deviceapi.ScanerLedLight
closeAuxiliaryLight(Context) - Method in class com.rscja.team.mtk.deviceapi.ScanerLedLight_mtk
  关闭扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
closeAuxiliaryLight(Context) - Method in class com.rscja.team.qcom.deviceapi.ScanerLedLight_qcom
  关闭扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
closeBuzzer() - Method in interface com.rscja.team.qcom.urax.IURAxDevice
closeBuzzer() - Method in class com.rscja.team.qcom.urax.QcomURAxDevice
closeBuzzer() - Method in class com.rscja.team.qcom.urax.RKURA4C8Device
closeBuzzer() - Method in class com.rscja.team.qcom.urax.RKURAxDevice
closeKeyboardHelper(Context) - Method in class com.rscja.barcode.BarcodeUtility
  关闭键盘助手功能总开关 Switch off main function switch of keyboardemulator
closeKeyboardHelper(Context) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  关闭键盘助手功能总开关 Switch off main function switch of keyboardemulator
closeKeyboardHelper(Context) - Method in class com.rscja.team.mtk.barcode.BarcodeUtility_mtk
  关闭键盘助手功能总开关 Switch off main function switch of keyboardemulator
closeKeyboardHelper(Context) - Method in class com.rscja.team.qcom.barcode.BarcodeUtility_qcom
  关闭键盘助手功能总开关 Switch off main function switch of keyboardemulator
closeLed() - Method in class com.rscja.deviceapi.BluetoothReader
  关闭led
closeLED() - Method in class com.rscja.deviceapi.Infrared
  关闭辅助灯
  Close LED
closeLED() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  关闭辅助灯
  Close LED
closeLed() - Method in interface com.rscja.deviceapi.interfaces.IReader
  关闭led
closeLed() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  关闭led
closeLED() - Method in class com.rscja.team.mtk.deviceapi.Infrared_mtk
  关闭辅助灯
  Close LED
closeLed() - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
closeLed() - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
  关闭led
closeLed() - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFUSB_qcom
  关闭led
closeLedSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
closeLedSendData() - Method in class com.rscja.team.qcom.deviceapi.UHFProtocolParseByJava
closeport() - Method in class com.rscja.team.qcom.usb.pl2302.UsbPL2302
closeport() - Method in class com.rscja.team.qcom.usb.RxUsb_qcom
closeport() - Method in class com.rscja.team.qcom.usb.UrxUsb_qcom
closeport() - Method in class com.rscja.team.qcom.usb.UsbBase_qcom
closeScanLed() - Method in interface com.rscja.team.qcom.urax.IURAxDevice
closeScanLed() - Method in class com.rscja.team.qcom.urax.QcomURAxDevice
closeScanLed() - Method in class com.rscja.team.qcom.urax.RKURA4C8Device
closeScanLed() - Method in class com.rscja.team.qcom.urax.RKURAxDevice
closeSerail() - Method in interface com.rscja.deviceapi.interfaces.IModule
  关闭串口
closeSerail() - Method in class com.rscja.deviceapi.Module
  关闭串口
closeSerail() - Method in class com.rscja.team.mtk.deviceapi.Module_mtk
  关闭串口
closeSerail(int) - Method in class com.rscja.team.qcom.deviceapi.HardwareInterface_qcom
  关闭串口
closeSerail() - Method in class com.rscja.team.qcom.deviceapi.Module_qcom
  关闭串口
closeSerialPort() - Method in class com.rscja.team.qcom.serialportapi.SerialportAPI
closeUhfSendData() - Method in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUrAxBase_qcom
closeWifi() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  关闭wifi
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  关闭wifi
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  关闭wifi
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  关闭wifi
closeWorkLed() - Method in interface com.rscja.team.qcom.urax.IURAxDevice
closeWorkLed() - Method in class com.rscja.team.qcom.urax.QcomURAxDevice
closeWorkLed() - Method in class com.rscja.team.qcom.urax.RKURA4C8Device
closeWorkLed() - Method in class com.rscja.team.qcom.urax.RKURAxDevice
cmd - Variable in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom.CMDInfo
cmd - Variable in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase.CMDInfo
cmd - Variable in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase.CMDInfo
CMDInfo() - Constructor for class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom.CMDInfo
CMDInfo() - Constructor for class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase.CMDInfo
CMDInfo() - Constructor for class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase.CMDInfo
CoAsiaBarcodeSymbol_qcom - Class in com.rscja.team.qcom.barcode.symbol
com.rscja.barcode - package com.rscja.barcode
com.rscja.custom - package com.rscja.custom
com.rscja.custom.interfaces - package com.rscja.custom.interfaces
com.rscja.deviceapi.entity - package com.rscja.deviceapi.entity
com.rscja.deviceapi.enums - package com.rscja.deviceapi.enums
com.rscja.deviceapi.exception - package com.rscja.deviceapi.exception
com.rscja.deviceapi.interfaces - package com.rscja.deviceapi.interfaces
com.rscja.scanner - package com.rscja.scanner
com.rscja.scanner.led - package com.rscja.scanner.led
com.rscja.scanner.utility - package com.rscja.scanner.utility
com.rscja.system - package com.rscja.system
com.rscja.team.mtk - package com.rscja.team.mtk
com.rscja.team.mtk.barcode - package com.rscja.team.mtk.barcode
com.rscja.team.mtk.barcode.barcode2d - package com.rscja.team.mtk.barcode.barcode2d
com.rscja.team.mtk.barcode.symbol - package com.rscja.team.mtk.barcode.symbol
com.rscja.team.mtk.custom - package com.rscja.team.mtk.custom
com.rscja.team.mtk.deviceapi - package com.rscja.team.mtk.deviceapi
com.rscja.team.mtk.scanner.led - package com.rscja.team.mtk.scanner.led
com.rscja.team.mtk.scanner.utility - package com.rscja.team.mtk.scanner.utility
com.rscja.team.mtk.system - package com.rscja.team.mtk.system
com.rscja.team.mtk.utility - package com.rscja.team.mtk.utility
com.rscja.team.qcom - package com.rscja.team.qcom
com.rscja.team.qcom.barcode - package com.rscja.team.qcom.barcode
com.rscja.team.qcom.barcode.barcode2d - package com.rscja.team.qcom.barcode.barcode2d
com.rscja.team.qcom.barcode.symbol - package com.rscja.team.qcom.barcode.symbol
com.rscja.team.qcom.ble - package com.rscja.team.qcom.ble
com.rscja.team.qcom.custom - package com.rscja.team.qcom.custom
com.rscja.team.qcom.deviceapi - package com.rscja.team.qcom.deviceapi
com.rscja.team.qcom.http - package com.rscja.team.qcom.http
com.rscja.team.qcom.r1 - package com.rscja.team.qcom.r1
com.rscja.team.qcom.r1.hf - package com.rscja.team.qcom.r1.hf
com.rscja.team.qcom.r1.psam - package com.rscja.team.qcom.r1.psam
com.rscja.team.qcom.rs232utils - package com.rscja.team.qcom.rs232utils
com.rscja.team.qcom.scanner.led - package com.rscja.team.qcom.scanner.led
com.rscja.team.qcom.scanner.utility - package com.rscja.team.qcom.scanner.utility
com.rscja.team.qcom.serialportapi - package com.rscja.team.qcom.serialportapi
com.rscja.team.qcom.service - package com.rscja.team.qcom.service
com.rscja.team.qcom.socket - package com.rscja.team.qcom.socket
com.rscja.team.qcom.system - package com.rscja.team.qcom.system
com.rscja.team.qcom.uhfhandler - package com.rscja.team.qcom.uhfhandler
com.rscja.team.qcom.uhfparse - package com.rscja.team.qcom.uhfparse
com.rscja.team.qcom.urax - package com.rscja.team.qcom.urax
com.rscja.team.qcom.usb - package com.rscja.team.qcom.usb
com.rscja.team.qcom.usb.pl2302 - package com.rscja.team.qcom.usb.pl2302
com.rscja.team.qcom.utility - package com.rscja.team.qcom.utility
com.rscja.utility - package com.rscja.utility
COMMAND_15693_SELECT - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_ACTIVATEIDLE - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_ANTICOLL - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_ANTICOLLINVENTORY - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_AUTHENTICATION - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_COS_COMMAND - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_DECREMENT - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_FM1216RESET - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_GET_MUL_BLOCK - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_GET_SYSTEM_INFO - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_HALT - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_HALT_TYPEB - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_INCREMENT - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_INITVAL - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_INVENTORY - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_LOCK_AFI - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_LOCK_BLOCK - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_LOCK_DSFID - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_READ - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_READ_SM - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_READVAL - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_REQUESTA - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_RESET_TO_READY - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_RESTORE - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_SELECT - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_TRANSFER - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_TRANSFERCOMMAND - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_TYPEARATS - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_TYPEAREST - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_TYPEB_GET_UID - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_TYPEBREST - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_ULANTICOLL - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_ULWRITE - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_WRITE - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_WRITE_AFI - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_WRITE_DSFID - Variable in class com.rscja.team.qcom.r1.hf.HFBase
COMMAND_WRITE_SM - Variable in class com.rscja.team.qcom.r1.hf.HFBase
Config_GetAccess() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Config_GetAccess() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Config_GetPara(int) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Config_GetPara(int) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Config_ReadRTC() - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Config_ReadRTC() - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Config_SetPara(int, byte, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Config_SetPara(int, byte, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Config_SetRTC(byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Config_SetRTC(byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
Config_SetWorkMode(byte, byte[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
Config_SetWorkMode(byte, byte[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
configFDXTag(char[], char[]) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  EM4305 配置成动物标签
  EM4305 configurate animal tag
configFDXTag(char[], char[]) - Method in class com.rscja.deviceapi.RFIDWithLF
  EM4305 配置成动物标签
  EM4305 configurate animal tag
ConfigFDXTag(char[], char[]) - Method in class com.rscja.team.mtk.deviceapi.DeviceAPI
ConfigFDXTag(char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.DeviceAPI
configFDXTag(char[], char[]) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithLF_qcom
  EM4305 配置成动物标签
  EM4305 configurate animal tag
ConfigurationException - Exception in com.rscja.deviceapi.exception
  设备配置异常类
  Device configuration exception type
ConfigurationException() - Constructor for exception com.rscja.deviceapi.exception.ConfigurationException
connect() - Method in class com.rscja.deviceapi.BleDevice
  连接蓝牙(Connect Bluetooth)
connect(ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.BleDevice
  连接蓝牙(Connect Bluetooth)
connect(String, ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.BluetoothReader
connect(String) - Method in class com.rscja.deviceapi.BluetoothReader
connect() - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
connect(ConnectionStatusCallback<Object>) - Method in interface com.rscja.deviceapi.interfaces.IBleDevice
connect(String) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  连接蓝牙(Connect Bluetooth)
connect(String, ConnectionStatusCallback<Object>) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  连接蓝牙(Connect Bluetooth)
connect(Context) - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  连接读写器(Connect to the reader)
connect(String, ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
connect(String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
connect(String) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
connect(String, ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.ble.EmptyUhfBle
connect() - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
connect(ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.BleDevice_qcom
connect(String, ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
connect(String) - Method in class com.rscja.team.qcom.deviceapi.BluetoothReader_qcom
connect(String, ConnectionStatusCallback<Object>) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
connect(String) - Method in class com.rscja.team.qcom.deviceapi.RFIDWithUHFBLE_qcom
connect(String, ConnectionStatusCallback) - Method in class com.rscja.team.qcom.service.BLEService_qcom
connect(String) - Method in class com.rscja.team.qcom.service.BLEService_qcom
connect(String, int, boolean) - Method in class com.rscja.team.qcom.socket.SocketManageA4
connect(String, int) - Method in class com.rscja.team.qcom.socket.SocketManageUR4
connect(String, int) - Method in class com.rscja.team.qcom.socket.SocketTcpIpBase
connect(String, int) - Method in class com.rscja.team.qcom.socket.SocketUdpClient
connect(String, int) - Method in class com.rscja.team.qcom.socket.SocketUdpClientUR4
connectAll() - Method in class com.rscja.deviceapi.RFIDWithUHFBLEManage
  连接所有蓝牙
ConnectionStatus - Enum in com.rscja.deviceapi.interfaces
ConnectionStatusCallback<T> - Interface in com.rscja.deviceapi.interfaces
ConstantUtil - Class in com.rscja.barcode
ConstantUtil() - Constructor for class com.rscja.barcode.ConstantUtil
Consume(float) - Method in class com.rscja.deviceapi.CardWithBYL
  扣费
Consume(float) - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  扣费
Consume(float) - Method in class com.rscja.team.qcom.deviceapi.CardWithBYL_qcom
  扣费
controlWord - Variable in class com.rscja.team.qcom.rs232utils.UHFProtocolParseUtils_qcom.CMDInfo
controlWord - Variable in class com.rscja.team.qcom.uhfhandler.UHFDataHandleBase.CMDInfo
controlWord - Variable in class com.rscja.team.qcom.uhfparse.UHFProtocolProtocolParseBase.CMDInfo
convertToRed(String, byte[]) - Method in class com.rscja.utility.FingerprintPictureUtility
CPU_MTK_6735 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_MTK_6763 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_MTK_6765 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_MTK_8786 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_QUACOMM_4350 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_QUACOMM_8909 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_QUACOMM_8953 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_QUACOMM_QCM2150 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_QUACOMM_SM6115 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_QUACOMM_SMD450 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
CPU_RK_3568 - Static variable in class com.rscja.team.qcom.DeviceConfiguration_qcom.Platform
cpuCommand(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  CPU卡发送命令(execute cpu card command)
cpuCommand(byte[]) - Method in class com.rscja.team.qcom.r1.hf.HF14443A
  CPU卡发送命令(execute cpu card command)
create() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity.Builder
CW102_6761 - Static variable in class com.rscja.CWDeviceInfo
CW103_6765 - Static variable in class com.rscja.CWDeviceInfo
CW103_6765 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
CW107_6762 - Static variable in class com.rscja.CWDeviceInfo
CW108_8781 - Static variable in class com.rscja.CWDeviceInfo
CW108_8791 - Static variable in class com.rscja.CWDeviceInfo
CW95_6762 - Static variable in class com.rscja.CWDeviceInfo
CW95_6762 - Static variable in class com.rscja.team.mtk.DeviceConfiguration_mtk
CWDeviceInfo - Class in com.rscja

A B C D E F G H I J K L M N O P Q R S T U V W X Z