com.rscja.team.qcom.r1

## Interface IPSAM

- All Known Implementing Classes:
    PSAM

      public interface IPSAM

- - ### Method Summary

    All Methods Instance Methods Abstract Methods
    Modifier and Type | Method and Description
    --- | ---
    `boolean` | `free(byte cSlotNum)` 释放PSAM(Release PSAM)
    `boolean` | `init(byte cSlotNum)`
    `byte[]` | `reset(byte cSlotNum)` 重置PSAM卡(reset smart card )
    `byte[]` | `transferCmd(byte cSlotNum, byte[] pcInCmd)` 传输psam命令(smart card transfer command)

- - ### Method Detail

    - #### init

          boolean init(byte cSlotNum)

    - #### free

          boolean free(byte cSlotNum)

      释放PSAM(Release PSAM)
      Parameters:
        `cSlotNum` - psam卡槽0,1 (Card slot,value:0,1)
      Returns:
        true:success false:fail

    - #### reset

          byte[] reset(byte cSlotNum)

      重置PSAM卡(reset smart card )
      Returns:
        success will return HF14443RequestEntity data, failure will return null.

    - #### transferCmd

          byte[] transferCmd(byte cSlotNum,
                             byte[] pcInCmd)

      传输psam命令(smart card transfer command)
      Returns:
        success will return HF14443RequestEntity data, failure will return null.