## Uses of Class
com.rscja.deviceapi.exception.RFIDReadFailureException

- Packages that use RFIDReadFailureException
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |
  com.rscja.team.mtk.deviceapi |
  com.rscja.team.qcom.deviceapi |

- - ### Uses of RFIDReadFailureException in com.rscja.deviceapi

    Methods in com.rscja.deviceapi that throw RFIDReadFailureException
    Modifier and Type | Method and Description
    --- | ---
    `char[]` | RFIDWithISO14443A.`M1_ReadData(int sector, int block)` 读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。 Read data in specified block of specified sector, used for S50 and S70 tag.
    `ISO15693Entity` | RFIDWithISO15693.`read(int block)` 读取块数据 read block data
    `SimpleRFIDEntity` | RFIDWithISO14443A.`read(int block)` 读卡，适用于Urltra light标签 card reading, used for Urltra light tag
    `ISO15693Entity` | RFIDWithISO15693.`read(int startBlock, int Blocklen)` 读取块数据 block data
    `java.lang.String` | RFIDWithISO15693.`read(ISO15693Entity entity, int block)`
    `SimpleRFIDEntity` | RFIDWithISO14443A.`read(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block)` 读卡,此函数包含寻卡和验证密钥步骤 Read card, this formula includes card search and key verfication procedure
    `SimpleRFIDEntity` | RFIDWithISO14443A.`readAllData(java.lang.String key, RFIDWithISO14443A.TagType tagType)` 读卡，读取卡片所有块中的数据 Card reading, read data of all blocks in the card

  - ### Uses of RFIDReadFailureException in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces that throw RFIDReadFailureException
    Modifier and Type | Method and Description
    --- | ---
    `char[]` | IRFIDWithISO14443A.`M1_ReadData(int sector, int block)` 读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。 Read data in specified block of specified sector, used for S50 and S70 tag.
    `ISO15693Entity` | IRFIDWithISO15693.`read(int block)` 读取块数据 read block data
    `SimpleRFIDEntity` | IRFIDWithISO14443A.`read(int block)` 读卡，适用于Urltra light标签 card reading, used for Urltra light tag
    `ISO15693Entity` | IRFIDWithISO15693.`read(int startBlock, int Blocklen)` 读取块数据 block data
    `java.lang.String` | IRFIDWithISO15693.`read(ISO15693Entity entity, int block)`
    `SimpleRFIDEntity` | IRFIDWithISO14443A.`read(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block)` 读卡,此函数包含寻卡和验证密钥步骤 Read card, this formula includes card search and key verfication procedure
    `SimpleRFIDEntity` | IRFIDWithISO14443A.`readAllData(java.lang.String key, RFIDWithISO14443A.TagType tagType)` 读卡，读取卡片所有块中的数据 Card reading, read data of all blocks in the card

  - ### Uses of RFIDReadFailureException in com.rscja.team.mtk.deviceapi

    Methods in com.rscja.team.mtk.deviceapi that throw RFIDReadFailureException
    Modifier and Type | Method and Description
    --- | ---
    `char[]` | RFIDWithISO14443A_mtk.`M1_ReadData(int sector, int block)` 读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。 Read data in specified block of specified sector, used for S50 and S70 tag.
    `ISO15693Entity` | RFIDWithISO15693_mtk.`read(int block)` 读取块数据 read block data
    `SimpleRFIDEntity` | RFIDWithISO14443A_mtk.`read(int block)` 读卡，适用于Urltra light标签 card reading, used for Urltra light tag
    `ISO15693Entity` | RFIDWithISO15693_mtk.`read(int startBlock, int Blocklen)` 读取块数据 block data
    `java.lang.String` | RFIDWithISO15693_mtk.`read(ISO15693Entity entity, int block)`
    `SimpleRFIDEntity` | RFIDWithISO14443A_mtk.`read(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block)` 读卡,此函数包含寻卡和验证密钥步骤 Read card, this formula includes card search and key verfication procedure
    `SimpleRFIDEntity` | RFIDWithISO14443A_mtk.`readAllData(java.lang.String key, RFIDWithISO14443A.TagType tagType)` 读卡，读取卡片所有块中的数据 Card reading, read data of all blocks in the card

  - ### Uses of RFIDReadFailureException in com.rscja.team.qcom.deviceapi

    Methods in com.rscja.team.qcom.deviceapi that throw RFIDReadFailureException
    Modifier and Type | Method and Description
    --- | ---
    `char[]` | RFIDWithISO14443A_qcom.`M1_ReadData(int sector, int block)` 读取指定扇区指定block的数据，适用于S50和S70标签。使用此函数的时候，要确保该扇区密钥验证已通过。 Read data in specified block of specified sector, used for S50 and S70 tag.
    `ISO15693Entity` | RFIDWithISO15693_qcom.`read(int block)` 读取块数据 read block data
    `SimpleRFIDEntity` | RFIDWithISO14443A_qcom.`read(int block)` 读卡，适用于Urltra light标签 card reading, used for Urltra light tag
    `ISO15693Entity` | RFIDWithISO15693_qcom.`read(int startBlock, int Blocklen)` 读取块数据 block data
    `java.lang.String` | RFIDWithISO15693_qcom.`read(ISO15693Entity entity, int block)`
    `SimpleRFIDEntity` | RFIDWithISO14443A_qcom.`read(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block)` 读卡,此函数包含寻卡和验证密钥步骤 Read card, this formula includes card search and key verfication procedure
    `SimpleRFIDEntity` | RFIDWithISO14443A_qcom.`readAllData(java.lang.String key, RFIDWithISO14443A.TagType tagType)` 读卡，读取卡片所有块中的数据 Card reading, read data of all blocks in the card